\HELP\WIN98\WIN98.TXT

               NETGEAR FA120 USB 2.0 Fast Ethernet Adapter
               -------------------------------------------
             Driver Installation for Microsoft Windows 98
             --------------------------------------------

  Getting Started
  ---------------
  First, please refer to the Installation Guide for complete installation
  instructions.  When installing the adapter onto your computer,make sure
  the USB port has Series "A" connector.

  Installation Procedure
  ----------------------
  1.  Plug the Model FA120 USB 2.0 Fast Ethernet Adapter into the USB port of 
      host computer.

  2.  Power on the computer system.
      There will appear "This wizard searches for new drivers for :"
                 
          'NETGEAR FA120 Adapter'
      
      Click 'Next>'
            
  3.  When the Win98 system asks 'What do you want Windows to do ? ' make 
      sure that you select 
        
        "Search for the bast driver for your device. [Recommended]"
      
      Click 'Next>' 
  
  4.  Choose the 'CD-ROM Drive'
      While on the same screen, insert the driver CD.
      Click 'Next>'
  
  5.  WIN98 will find the ' NETGEAR FA120 USB 2.0 Fast Ethernet Adapter ' and
      the location of the driver: D:\FA120.INF assuming that D: is the
      drive letter for your CD-ROM drive.

      Click 'Next>'
  
  6.  The system will copy the necessary driver files into your system.

  7.  Provide the Win98 CD-ROM or the drive path where Win98 files reside
      when asked to do so.

  8.  Reboot the system and check into the Device manager to confirm that
      the Model FA120 USB 2.0 Fast Ethernet Adapter is working properly.

 
