\HELP\WIN2K\WIN2K.TXT

               NETGEAR FA120 USB 2.0 Fast Ethernet Adapter
               -------------------------------------------
             Driver Installation for Microsoft Windows 2000
             ----------------------------------------------

  Getting Started
  ---------------
  First, please refer to the Installation Guide for complete installation
  instructions.  When installing the adapter onto your computer, make sure
  the USB port has Series "A" connector.

  Installation Procedure
  ----------------------
  1.  Plug the Model FA120 USB 2.0 Fast Ethernet Adapter into the USB port of 
      host computer.

  2.  Power on the computer system.After the systen decteced the FA120 ,  
      there will appear a "Welcome to the Found New Hardware Wizard" window.
      
       Click 'Next>'
       
  3.  There will appear "This wizard will complete the installation for 
      this device :"
                 
          ' NETGEAR FA120 Adapter '
      
      System will ask "What do you want the wizard to do ?" make sure 
      that you select 
        
        "Search for a suitable driver for my device. [recommended]"
      
      Click 'Next>'
            
  4.  When the Win2000 system asks 'Where do you want Windows to search for
      driver files ? ' make sure that you choose 'CD-DOM Drive' 
           
      Click 'Next>' 
  
  5.  Then, the windows will find a driver for the device.
      The location of the driver is: D:\fa120.inf assuming that D:
      is the drive letter for your CD-ROM drive.
      
      Click 'Next>' 
  
  6.  A "Microsoft has not digitally signed the driver" window will be
      displayed, click "yes" to continue.
  
  7.  The system will then copy the necessary driver files.

  8.  Check into the Device manager to confirm that the Model FA120 USB 2.0 
      Fast Ethernet Adapter is working properly.

 
