;*****************************************************************************
;*
;*  L1E62x64.INF  -   Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller
;*  Copyright 2001-2008, Atheros Co., Ltd.
;*
;*  INF File for NDIS6.20 Miniport Driver for Windows 7 x64 
;*
;*****************************************************************************
[Version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %ATHR%
CatalogFile = L1E62x64.cat
DriverVer   = 08/23/2009,1.0.0.18

[Manufacturer]
%ATHR% = Atheros, NTamd64

[ControlFlags]
ExcludeFromSelect	= *

[Atheros.NTamd64]
; DisplayName           Section               DeviceID
; -----------           -------	              --------
%ATHR.L1E%   = 	        L1E.ndi,              PCI\VEN_1969&DEV_1026
%ATHR.L1E%   = 	        L2E.ndi,              PCI\VEN_1969&DEV_1026&REV_F0
%ATHR.L1E%   =          L1E.ndi,              PCI\VEN_1969&DEV_1026&SUBSYS_10261969&REV_B0
%ATHR.L1E%   =          L1E.ndi,              PCI\VEN_1969&DEV_1026&SUBSYS_83041043&REV_B0
%ATHR.L1E%   =          L1E.ndi,              PCI\VEN_1969&DEV_1026&SUBSYS_83391043&REV_B0
%ATHR.L1E%   =          L1E.ndi,              PCI\VEN_1969&DEV_1026&SUBSYS_831C1043&REV_B0
%ATHR.L1E%   =          L1E.ECS.ndi,          PCI\VEN_1969&DEV_1026&SUBSYS_10261019&REV_B0
%ATHR.L1E%   =          L1E.ECS.ndi,          PCI\VEN_1969&DEV_1026&SUBSYS_00501B0A&REV_B0  ; Pegatron
%ATHR.L1E%   =          L1E.ECS.ndi,          PCI\VEN_1969&DEV_1026&SUBSYS_00681B0A&REV_B0  ; Pegatron
%ATHR.L1E%   =          L1E.ShutOn.ndi,       PCI\VEN_1969&DEV_1026&SUBSYS_00821B0A&REV_B0  ; Pegatron
%ATHR.L1E%   =          L1E.WOLMagic.ndi,     PCI\VEN_1969&DEV_1026&SUBSYS_00631B0A&REV_B0  ; Pegatron
%ATHR.L1E%   =          L1E.WOLMagic.ndi,     PCI\VEN_1969&DEV_1026&SUBSYS_00871B0A&REV_B0  ; Pegatron
%ATHR.L1E%   =          L1E.PEGA.ndi,         PCI\VEN_1969&DEV_1026&SUBSYS_00911B0A&REV_B0  ; Pegatron
%ATHR.L1E%   =          L1E.PEGA.ndi,         PCI\VEN_1969&DEV_1026&SUBSYS_00A51B0A&REV_B0  ; Pegatron
%ATHR.L1E%   =          L1E.DisS5.ndi,        PCI\VEN_1969&DEV_1026&SUBSYS_15051043&REV_B0  ; ASUS
%ATHR.L1E%   =          L1E.DisS5.ndi,        PCI\VEN_1969&DEV_1026&SUBSYS_14F51043&REV_B0  ; ASUS
%ATHR.L1E%   =          L1E.ndi,              PCI\VEN_1969&DEV_1026&SUBSYS_202A1B0A&REV_B0  ; Pegatron_Colt
%ATHR.L1E%   =          L2E.ndi,              PCI\VEN_1969&DEV_1026&SUBSYS_10261969&REV_F0

%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_002F1B0A&REV_B0  ; Unihan

%ATHR.L1E%   =          L1E.kili.ndi,	      PCI\VEN_1969&DEV_1026&SUBSYS_01461025&REV_B0  ; Kili
%ATHR.L1E%   =          L2E.kili.ndi,         PCI\VEN_1969&DEV_1026&SUBSYS_01461025&REV_F0
%ATHR.L1E%   =          L1E.kili.ndi,         PCI\VEN_1969&DEV_1026&SUBSYS_01451025&REV_B0  ; Teton
%ATHR.L1E%   =          L2E.kili.ndi,         PCI\VEN_1969&DEV_1026&SUBSYS_01451025&REV_F0

%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_01671025&REV_B0  ; KAL90
%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_01281025&REV_B0  ; KAVH0
%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_019C1025&REV_B0  ; KAV10
%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_02101025&REV_B0  ; KAWH0
%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_02111025&REV_B0  ; KBWH0
%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_02121025&REV_B0  ; KAWF0
%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_02131025&REV_B0  ; KAWG0
%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_022C1025&REV_B0  ; ZG8
%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_021B1025&REV_B0  ; KBLG0
%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_02601025&REV_B0  ; KALG0
%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_022E1025&REV_B0  ; KAW10
%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_028D1025&REV_B0  ; HM50/70-PU

%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_015E1025&REV_B0  ; ZK2
%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_01661025&REV_B0  ; ZK3
%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_02161025&REV_B0  ; HM20-YK

%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_02141025&REV_B0  ; HM40-MV
%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_019D1025&REV_B0  ; 
%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_02151025&REV_B0  ; HM40-YK
%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_030D1025&REV_B0  ; HM41

%ATHR.L1E%   =       	L1e.zk.ndi,           PCI\VEN_1969&DEV_1026&SUBSYS_0CD9105B&REV_B0  ; SZ902

[L1E.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
AddReg          = L1E.reg, L1E.params, Common.params, ShutOff.params, WOLDefault.params
CopyFiles       = L1E.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1E.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1E.ndi.Services]
AddService = L1E, 2, L1E.Service, Common.EventLog

[L1E.ShutOn.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
AddReg          = L1E.reg, L1E.pega.params, L1E.params, Common.params, ShutOn.params, WOLDefault.params
CopyFiles       = L1E.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1E.ShutOn.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1E.ShutOn.ndi.Services]
AddService = L1E, 2, L1E.Service, Common.EventLog

[L1E.DisS5.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
AddReg          = L1E.reg, L1E.ecs.params, L1E.params, Common.params, WOLDefault.params
CopyFiles       = L1E.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1E.DisS5.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1E.DisS5.ndi.Services]
AddService = L1E, 2, L1E.Service, Common.EventLog

[L1E.WOLMagic.ndi]
Characteristics = 0x84
BusType         = 5				 ;PCI
AddReg          = L1E.reg, L1E.pega.params, L1E.params, Common.params, ShutOn.params, WOLMagic.params
CopyFiles       = L1E.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1E.WOLMagic.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1E.WOLMagic.ndi.Services]
AddService = L1E, 2, L1E.Service, Common.EventLog

;-----------------------------------------------------------------------------

[L1E.ECS.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1E.reg, L1E.ecs.params, L1E.params, Common.params, ShutOff.params, WOLDefault.params
CopyFiles       = L1E.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1E.ECS.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1E.ECS.ndi.Services]
AddService = L1E, 2, L1E.Service, Common.EventLog


;-----------------------------------------------------------------------------

[L1E.kili.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1E.reg, L1E.kili.params, L1E.params, Common.params, ShutOff.params, WOLDefault.params
CopyFiles       = L1E.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1E.kili.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1E.kili.ndi.Services]
AddService = L1E, 2, L1E.Service, Common.EventLog

;-----------------------------------------------------------------------------

[L1E.zk.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1E.reg, L1E.zk.params, L1E.params, Common.params, ShutOff.params, WOLDefault.params
CopyFiles       = L1E.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1E.zk.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1E.zk.ndi.Services]
AddService = L1E, 2, L1E.Service, Common.EventLog

;-----------------------------------------------------------------------------

[L1E.PEGA.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1E.reg, L1E.pega.params, L1E.params, Common.params, ShutOff.params, WOLDefault.params
CopyFiles       = L1E.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L1E.PEGA.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L1E.PEGA.ndi.Services]
AddService = L1E, 2, L1E.Service, Common.EventLog

;-----------------------------------------------------------------------------

[L2E.kili.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1E.reg, L1E.kili.params, L2E.rev.params, Common.params, ShutOff.params, WOLDefault.params
CopyFiles       = L1E.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2E.kili.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2E.kili.ndi.Services]
AddService = L1E, 2, L1E.Service, Common.EventLog

;-----------------------------------------------------------------------------

[L2E.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1E.reg, L2E.rev.params, Common.params, ShutOff.params, WOLDefault.params
CopyFiles       = L1E.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[L2E.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = Msi.Addreg

[L2E.ndi.Services]
AddService = L1E, 2, L1E.Service, Common.EventLog

;-----------------------------------------------------------------------------
; L1E  specific
;
[L1E.reg]
HKR, Ndi, HelpText,, %HelpText%
HKR, Ndi, Service,    0, "L1E"
; use ndis5 as the upper bound because NT supports it
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

[Msi.Addreg]
HKR, "Interrupt Management", 0x00000010 
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 0
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1

[L1E.ecs.params]
HKR,, LedMode,	0x00010001,	1

[L1E.kili.params]
HKR,, LedMode,	0x00010001,	2 ;for kili,teton

[L1E.zk.params]
HKR,, LedMode,	0x00010001,	3 ;for ZK2,ZK3

[L1E.pega.params]
HKR,, LedMode,	0x00010001,	4 ;for Pegatron

[L2E.rev.params]
HKR,, ChipL2EB,	0x00010001,	1

[L1E.Service]
DisplayName     = %L1E.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\L1E62x64.sys
LoadOrderGroup  = NDIS

[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR,, EventMessageFile,	0x00020000, "%%SystemRoot%%\System32\Drivers\L1E62x64.sys"
HKR,, TypesSupported,	0x00010001, 7

[L1E.params]
HKR,Ndi\params\*JumboPacket,        		ParamDesc,  	0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        		default,    	0, "1514"
HKR,Ndi\params\*JumboPacket,        		type,       	0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   		"1514",     	0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   		"2048",     	0, %2KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   		"3072",     	0, %3KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   		"4096",     	0, %4KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   		"5120",     	0, %5KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   		"6144",     	0, %6KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   		"7168",     	0, %7KBMTU%

;-----------------------------------------------------------------------------
;
[Common.params]
HKR, Ndi\Params\MaxInterrupt,			ParamDesc,	0, %MaxIrq%
HKR, Ndi\Params\MaxInterrupt,			Type,		0, "int"
HKR, Ndi\Params\MaxInterrupt,			Base,		0, "10"
HKR, Ndi\Params\MaxInterrupt,			Min,		0, "1000"
HKR, Ndi\Params\MaxInterrupt,			Max,		0, "30000"
HKR, Ndi\Params\MaxInterrupt,			Step,		0, "500"
HKR, Ndi\Params\MaxInterrupt,			Default,	0, "5000"

HKR, Ndi\Params\*SpeedDuplex,			ParamDesc,	0, %SpeedDuplex%
HKR, Ndi\Params\*SpeedDuplex,			Type,		0, "enum"
HKR, Ndi\Params\*SpeedDuplex,			Default,	0, "0"
HKR, Ndi\Params\*SpeedDuplex\enum, 		"0",		0, %Auto%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"1",		0, %10MHD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"2",		0, %10MFD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"3",		0, %100MHD%
HKR, Ndi\Params\*SpeedDuplex\enum, 		"4",		0, %100MFD%

HKR, Ndi\Params\*ReceiveBuffers,		ParamDesc,	0, %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,		Type,		0, "int"
HKR, Ndi\Params\*ReceiveBuffers,		Base,		0, "10"
HKR, Ndi\Params\*ReceiveBuffers,		Min,		0, "3"
HKR, Ndi\Params\*ReceiveBuffers,		Max,		0, "64"
HKR, Ndi\Params\*ReceiveBuffers,		Step,		0, "1"
HKR, Ndi\Params\*ReceiveBuffers,		Default,	0, "16"

HKR, Ndi\Params\*TransmitBuffers,		ParamDesc,	0, %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers,		Type,		0, "int"
HKR, Ndi\Params\*TransmitBuffers,		Base,		0, "10"
HKR, Ndi\Params\*TransmitBuffers,		Min,		0, "256"
HKR, Ndi\Params\*TransmitBuffers,		Max,		0, "512"
HKR, Ndi\Params\*TransmitBuffers,		Step,		0, "128"
HKR, Ndi\Params\*TransmitBuffers,		Default,	0, "256"

HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	ParamDesc,	0, %TCPChksumOffv4%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Type,		0, "enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Default,	0, "3"

HKR, Ndi\Params\*IPChecksumOffloadIPv4,		ParamDesc,	0, %IPChksumOffv4%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Type,		0, "enum"
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Default,	0, "3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	ParamDesc,	0, %UDPChksumOffv4%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Type,		0, "enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Default,	0, "3"

HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	ParamDesc,	0, %TCPChksumOffv6%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	Type,		0, "enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	Default,	0, "3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	ParamDesc,	0, %UDPChksumOffv6%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	Type,		0, "enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	Default,	0, "3"

HKR, Ndi\Params\*LsoV1IPv4,			ParamDesc,	0, %LSOv1IPv4%
HKR, Ndi\Params\*LsoV1IPv4,			Type,		0, "enum"
HKR, Ndi\Params\*LsoV1IPv4\enum,		"1",		0, %Enabled%
HKR, Ndi\Params\*LsoV1IPv4\enum,		"0",		0, %Disabled%
HKR, Ndi\Params\*LsoV1IPv4,			Default,	0, "1"

HKR, Ndi\Params\NetworkAddress,			ParamDesc,	0, %NetAddress%
HKR, Ndi\Params\NetworkAddress,			Type,		0, "edit"
HKR, Ndi\Params\NetworkAddress,			LimitText,	0, "12"
HKR, Ndi\Params\NetworkAddress,			UpperCase,	0, "1"
HKR, Ndi\Params\NetworkAddress,			Default,	0, ""
HKR, Ndi\Params\NetworkAddress,			Optional,	0, "1"

HKR, Ndi\Params\*InterruptModeration,		ParamDesc,	0, %IntMod%
HKR, Ndi\Params\*InterruptModeration,		Type,		0, "enum"
HKR, Ndi\Params\*InterruptModeration\enum,	"1",		0, %Enabled%
HKR, Ndi\Params\*InterruptModeration\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*InterruptModeration,		Default,	0, "1"

HKR, Ndi\Params\*FlowControl,			ParamDesc,	0, %FlowCtrl%
HKR, Ndi\Params\*FlowControl,			Type,		0, "enum"
HKR, Ndi\Params\*FlowControl\enum,		"3",		0, %TXRXEna%
HKR, Ndi\Params\*FlowControl\enum,		"0",		0, %Disabled%
HKR, Ndi\Params\*FlowControl,			Default,	0, "0"

HKR, Ndi\Params\APSmode,			ParamDesc,	0, %APSmode%
HKR, Ndi\Params\APSmode,			Type,		0, "enum"
HKR, Ndi\Params\APSmode\enum,			"1",		0, %Enabled%
HKR, Ndi\Params\APSmode\enum,			"0",		0, %Disabled%
HKR, Ndi\Params\APSmode,			Default,	0, "0"

[WOLDefault.params]
HKR, Ndi\Params\WakeUpCapabilities,		ParamDesc,	0, %WakeUpCapabilities%
HKR, Ndi\Params\WakeUpCapabilities,		Type,		0, "enum"
HKR, Ndi\Params\WakeUpCapabilities\enum, 	"0",		0, %None%
HKR, Ndi\Params\WakeUpCapabilities\enum, 	"1",		0, %MagicPacket%
HKR, Ndi\Params\WakeUpCapabilities\enum, 	"2",		0, %PatternMatch%
HKR, Ndi\Params\WakeUpCapabilities\enum, 	"3",		0, %MagicPacket_PatternMatch%
HKR, Ndi\Params\WakeUpCapabilities,		Default,	0, "3"

[WOLMagic.params]
HKR, Ndi\Params\WakeUpCapabilities,		ParamDesc,	0, %WakeUpCapabilities%
HKR, Ndi\Params\WakeUpCapabilities,		Type,		0, "enum"
HKR, Ndi\Params\WakeUpCapabilities\enum, 	"0",		0, %None%
HKR, Ndi\Params\WakeUpCapabilities\enum, 	"1",		0, %MagicPacket%
HKR, Ndi\Params\WakeUpCapabilities\enum, 	"2",		0, %PatternMatch%
HKR, Ndi\Params\WakeUpCapabilities\enum, 	"3",		0, %MagicPacket_PatternMatch%
HKR, Ndi\Params\WakeUpCapabilities,		Default,	0, "1"

[ShutOn.params]
HKR, Ndi\Params\ShutdownWake,			ParamDesc,	0, %ShutDW%
HKR, Ndi\Params\ShutdownWake,			Type,		0, "enum"
HKR, Ndi\Params\ShutdownWake\enum,		1,		0, %Enabled%
HKR, Ndi\Params\ShutdownWake\enum,		0,		0, %Disabled%
HKR, Ndi\Params\ShutdownWake,			Default,	0, "1"

[ShutOff.params]
HKR, Ndi\Params\ShutdownWake,			ParamDesc,	0, %ShutDW%
HKR, Ndi\Params\ShutdownWake,			Type,		0, "enum"
HKR, Ndi\Params\ShutdownWake\enum,		1,		0, %Enabled%
HKR, Ndi\Params\ShutdownWake\enum,		0,		0, %Disabled%
HKR, Ndi\Params\ShutdownWake,			Default,	0, "0"

;-----------------------------------------------------------------------------
; DestinationDirs
;
[L1E.CopyFiles]
L1E62x64.sys,,,2

[SourceDisksNames]
;
; diskid = description[, [tagfile] [, <unused>, subdir]]
;
1 = %DriverDisk%,,,

[SourceDisksFiles]
;
; filename_on_source = diskID[, [subdir][, size]]
;
L1E62x64.sys = 1

[DestinationDirs]
L1E.CopyFiles     	= 12
DefaultDestDir       	= 11

[Strings]
ATHR 			 = "Atheros"
JumboFrame  		 = "Jumbo Frame"
2KBMTU      		 = "2KB MTU"
3KBMTU      		 = "3KB MTU"
4KBMTU      		 = "4KB MTU"
5KBMTU      		 = "5KB MTU"
6KBMTU      		 = "6KB MTU"
7KBMTU      		 = "7KB MTU"
IntMod 			 = "Interrupt Moderation"
MaxIrq			 = "Max IRQ per Second"
Enabled			 = "Enabled"
Disabled		 = "Disabled"
SpeedDuplex		 = "Speed & Duplex"
Auto		  	 = "Auto Negotiation"
10MHD		  	 = "10 Mbps Half Duplex"
10MFD		  	 = "10 Mbps Full Duplex"
100MHD			 = "100 Mbps Half Duplex"
100MFD			 = "100 Mbps Full Duplex"
FlowCtrl		 = "FlowControl"
ShutDW			 = "Shutdown Wake Up"
RSS			 = "Receive Side Scaling"
TXEna 			 = "Tx Enabled"
RXEna 			 = "Rx Enabled"
TXRXEna 		 = "Tx & Rx Enabled"
ReceiveBuffers 		 = "Receive Buffers"
TransmitBuffers 	 = "Transmit Buffers"
IPChksumOffv4 		 = "IPv4 Checksum Offload"
TCPChksumOffv4 		 = "TCP Checksum Offload (IPv4)"
TCPChksumOffv6 		 = "TCP Checksum Offload (IPv6)"
UDPChksumOffv4 		 = "UDP Checksum Offload (IPv4)"
UDPChksumOffv6 		 = "UDP Checksum Offload (IPv6)"
LSOv1IPv4 		 = "Large Send Offload (IPv4)"
NetAddress   		 = "Network Address"
WakeUpCapabilities       = "Wake Up Capabilities"
APSmode			 = "APS mode"
None		         = "None"
LinkChange	         = "Link Change"
MagicPacket	         = "Magic Packet"
PatternMatch	         = "Pattern Match"
MagicPacket_PatternMatch = "MagicPacket & PatternMatch"
All 			 = "All"

ATHR.L1E 		= "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
L1E.Service.DispName 	= "NDIS Miniport Driver for Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Chinese (Taiwan)
[Strings.0404]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Atheros"
JumboFrame  		 = "大型框架"
2KBMTU      		 = "2KB MTU"
3KBMTU      		 = "3KB MTU"
4KBMTU      		 = "4KB MTU"
5KBMTU      		 = "5KB MTU"
6KBMTU      		 = "6KB MTU"
7KBMTU      		 = "7KB MTU"
IntMod 			 = "中斷調節"
MaxIrq			 = "每秒 IRQ 上限"
Enabled			 = "已啟用"
Disabled		 = "已停用"
SpeedDuplex		 = "速度和雙工"
Auto		  	 = "自動協調"
10MHD		  	 = "10 Mbps 半雙工"
10MFD		  	 = "10 Mbps 全雙工"
100MHD			 = "100 Mbps 半雙工"
100MFD			 = "100 Mbps 全雙工"
FlowCtrl		 = "FlowControl"
ShutDW			 = "關閉狀態喚醒"
RSS			 = "接收側邊調整"
TXEna 			 = "傳輸已啟用"
RXEna 			 = "接收已啟用"
TXRXEna 		 = "傳輸和接收已啟用"
ReceiveBuffers 		 = "接收緩衝"
TransmitBuffers 	 = "傳輸緩衝"
IPChksumOffv4 		 = "IPv4 檢查總和卸載"
TCPChksumOffv4 		 = "TCP 檢查總和卸載 (IPv4)"
TCPChksumOffv6 		 = "TCP 檢查總和卸載 (IPv6)"
UDPChksumOffv4 		 = "UDP 檢查總和卸載 (IPv4)"
UDPChksumOffv6 		 = "UDP 檢查總和卸載 (IPv6)"
LSOv1IPv4 		 = "大型傳送卸載 (IPv4)"
NetAddress   		 = "網路位址"
WakeUpCapabilities       = "喚醒功能"
APSmode			 = "APS 模式"
None		         = "無"
LinkChange	         = "Link Change"
MagicPacket	         = "Magic Packet"
PatternMatch	         = "Pattern Match"
MagicPacket_PatternMatch = "MagicPacket & PatternMatch"
All 			 = "全部"

ATHR.L1E 		= "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
L1E.Service.DispName 	= "NDIS Miniport Driver for Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; German (Standard)
[Strings.0407]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Atheros"
JumboFrame  		 = "Jumbo-Frame"
2KBMTU      		 = "2 KB MTU"
3KBMTU      		 = "3 KB MTU"
4KBMTU      		 = "4 KB MTU"
5KBMTU      		 = "5 KB MTU"
6KBMTU      		 = "6 KB MTU"
7KBMTU      		 = "7 KB MTU"
IntMod 			 = "Interrupt Moderation"
MaxIrq			 = "Max. IRQ pro Sekunde"
Enabled			 = "Aktiviert"
Disabled		 = "Deaktiviert"
SpeedDuplex		 = "Speed & Duplex"
Auto		  	 = "Autonegotiation"
10MHD		  	 = "10 Mbit/s Halbduplex"
10MFD		  	 = "10 Mbit/s Vollduplex"
100MHD			 = "100 Mbit/s Halbduplex"
100MFD			 = "100 Mbit/s Vollduplex"
FlowCtrl		 = "FlowControl"
ShutDW			 = "Shutdown/Wakeup"
RSS			 = "Empfangsskalierung"
TXEna 			 = "Tx aktiviert"
RXEna 			 = "Rx aktiviert"
TXRXEna 		 = "Tx & Rx aktiviert"
ReceiveBuffers 		 = "Pufferempfang"
TransmitBuffers 	 = "Pufferertragung"
IPChksumOffv4 		 = "IPv4 Checksum Offload"
TCPChksumOffv4 		 = "TCP Checksum Offload (IPv4)"
TCPChksumOffv6 		 = "TCP Checksum Offload (IPv6)"
UDPChksumOffv4 		 = "UDP Checksum Offload (IPv4)"
UDPChksumOffv6 		 = "UDP Checksum Offload (IPv6)"
LSOv1IPv4 		 = "Large Send Offload (IPv4)"
NetAddress   		 = "Netzwerkadresse"
WakeUpCapabilities       = "WakeUp-Eigenschaften"
APSmode			 = "APS-Modus"
None		         = "Keine"
LinkChange	         = "Link Change"
MagicPacket	         = "Magic Packet"
PatternMatch	         = "Pattern Match"
MagicPacket_PatternMatch = "MagicPacket & PatternMatch"
All 			 = "Alle"

ATHR.L1E 		= "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
L1E.Service.DispName 	= "NDIS Miniport Driver for Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Spanish (Spain, Traditional Sort)
[Strings.040A]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Atheros"
JumboFrame  		 = "Trama gigante"
2KBMTU      		 = "MTU de 2KB"
3KBMTU      		 = "MTU de 3KB"
4KBMTU      		 = "MTU de 4KB"
5KBMTU      		 = "MTU de 5KB"
6KBMTU      		 = "MTU de 6KB"
7KBMTU      		 = "MTU de 7KB"
IntMod 			 = "Moderación de interrupciones"
MaxIrq			 = "IRQ máx por segundo"
Enabled			 = "Habilitado"
Disabled		 = "Inhabilitado"
SpeedDuplex		 = "Velocidad y Dúplex"
Auto		  	 = "Negociación automática"
10MHD		  	 = "Dúplex medio 10Mbps"
10MFD		  	 = "Dúplex completo 10Mbps"
100MHD			 = "Dúplex medio 100Mbps"
100MFD			 = "Dúplex completo 100Mbps"
FlowCtrl		 = "FlowControl"
ShutDW			 = "Reactivar cierre"
RSS			 = "Ajuste de escala en lado de recepción"
TXEna 			 = "Transmisión habilitada"
RXEna 			 = "Recepción habilitada"
TXRXEna 		 = "Transmisión y recepción habilitadas"
ReceiveBuffers 		 = "Recibir búferes"
TransmitBuffers 	 = "Búfers de transmisión"
IPChksumOffv4 		 = "Carga de suma de comprobación IPv4"
TCPChksumOffv4 		 = "Carga de suma de comprobación TCP (IPv4)"
TCPChksumOffv6 		 = "Carga de suma de comprobación TCP (IPv6)"
UDPChksumOffv4 		 = "Carga de suma de comprobación UDP (IPv4)"
UDPChksumOffv6 		 = "Carga de suma de comprobación UDP (IPv6)"
LSOv1IPv4 		 = "Gran carga de envío (IPv4)"
NetAddress   		 = "Dirección de red"
WakeUpCapabilities       = "Capacidades de reactivación"
APSmode			 = "Modo APS"
None		         = "Ninguno"
LinkChange	         = "Link Change"
MagicPacket	         = "Magic Packet"
PatternMatch	         = "Pattern Match"
MagicPacket_PatternMatch = "MagicPacket & PatternMatch"
All 			 = "Todo"

ATHR.L1E 		= "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
L1E.Service.DispName 	= "NDIS Miniport Driver for Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."
; French (Standard)
[Strings.040C]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Atheros"
JumboFrame  		 = "Trame Jumbo"
2KBMTU      		 = "MTU de 2 Ko"
3KBMTU      		 = "MTU de 3 Ko"
4KBMTU      		 = "MTU de 4 Ko"
5KBMTU      		 = "MTU de 5 Ko"
6KBMTU      		 = "MTU de 6 Ko"
7KBMTU      		 = "MTU de 7 Ko"
IntMod 			 = "Modération de l'interruption"
MaxIrq			 = "IRQ maxi. par seconde"
Enabled			 = "Activée"
Disabled		 = "Désactivée"
SpeedDuplex		 = "Vitesse et Duplex"
Auto		  	 = "Négociation automatique"
10MHD		  	 = "10 Mbits/s Semi-duplex"
10MFD		  	 = "10 Mbits/s Duplex intégral"
100MHD			 = "100 Mbits/s Semi-duplex"
100MFD			 = "100 Mbits/s Duplex intégral"
FlowCtrl		 = "Contrôle de flux"
ShutDW			 = "Sortie de veille à l'arrêt"
RSS			 = "Mise à l'échelle côté réception"
TXEna 			 = "Tx activé"
RXEna 			 = "Rx activé"
TXRXEna 		 = "Tx et rx activés"
ReceiveBuffers 		 = "Mémoires tampon de réception"
TransmitBuffers 	 = "Mémoires tampon de transmission"
IPChksumOffv4 		 = "Déchargement de somme de contrôle IPv4"
TCPChksumOffv4 		 = "Déchargement de somme de contrôle TCP (IPv4)"
TCPChksumOffv6 		 = "Déchargement de somme de contrôle TCP (Ipv6)"
UDPChksumOffv4 		 = "Déchargement de somme de contrôle UDP (IPv4)"
UDPChksumOffv6 		 = "Déchargement de somme de contrôle UDP (Ipv6)"
LSOv1IPv4 		 = "Déchargement d'envoi important (IPv4)"
NetAddress   		 = "Adresse réseau"
WakeUpCapabilities       = "Capacités de mise en éveil"
APSmode			 = "Mode APS"
None		         = "Aucun"
LinkChange	         = "Changement de liaison"
MagicPacket	         = "Paquet magique"
PatternMatch	         = "Correspondance au modèle"
MagicPacket_PatternMatch = "MagicPack et PatternMatch"
All 			 = "Tous"

ATHR.L1E 		= "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
L1E.Service.DispName 	= "NDIS Miniport Driver for Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Italian (Standard)
[Strings.0410]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Atheros"
JumboFrame  		 = "Frame jumbo"
2KBMTU      		 = "MTU 2 KB"
3KBMTU      		 = "MTU 3 KB"
4KBMTU      		 = "MTU 4 KB"
5KBMTU      		 = "MTU 5 KB"
6KBMTU      		 = "MTU 6 KB"
7KBMTU      		 = "MTU 7 KB"
IntMod 			 = "Regolazione di interrupt (interrupt moderation)"
MaxIrq			 = "Numero massimo di IRQ per secondo"
Enabled			 = "Abilitata"
Disabled		 = "Disabilitato"
SpeedDuplex		 = "Velocità e duplex"
Auto		  	 = "Negoziazione automatica"
10MHD		  	 = "Half Duplex 10 Mbps"
10MFD		  	 = "Full Duplex 10 Mbps"
100MHD			 = "Half Duplex 100 Mbps"
100MFD			 = "Full Duplex 100 Mbps"
FlowCtrl		 = "FlowControl"
ShutDW			 = "Attivazione arresto"
RSS			 = "Receive-Side Scaling"
TXEna 			 = "Tx attivato"
RXEna 			 = "Rx attivato"
TXRXEna 		 = "Abilitato Tx e Rx"
ReceiveBuffers 		 = "Buffer di ricezione"
TransmitBuffers 	 = "Buffer di trasmissione"
IPChksumOffv4 		 = "Offload checksum IPv4"
TCPChksumOffv4 		 = "Offload di checksum TCP (IPv4)"
TCPChksumOffv6 		 = "Offload di checksum TCP (IPv6)"
UDPChksumOffv4 		 = "Offload di checksum UDP (IPv4)"
UDPChksumOffv6 		 = "Offload di checksum UDP (IPv6)"
LSOv1IPv4 		 = "Offload invio di grandi dimensioni (IPv4)"
NetAddress   		 = "Indirizzo di rete"
WakeUpCapabilities       = "Capacità di attivazione"
APSmode			 = "Modalità APS"
None		         = "Nessuno"
LinkChange	         = "Modifica collegamento"
MagicPacket	         = "Magic Packet"
PatternMatch	         = "Corrispondenza motivo"
MagicPacket_PatternMatch = "MagicPacket e PatternMatch"
All 			 = "Tutti"

ATHR.L1E 		= "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
L1E.Service.DispName 	= "NDIS Miniport Driver for Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Japanese
[Strings.0411]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Atheros"
JumboFrame  		 = "ジャンボ フレーム"
2KBMTU      		 = "2 KB MTU"
3KBMTU      		 = "3 KB MTU"
4KBMTU      		 = "4 KB MTU"
5KBMTU      		 = "5 KB MTU"
6KBMTU      		 = "6 KB MTU"
7KBMTU      		 = "7 KB MTU"
IntMod 			 = "割り込み調停"
MaxIrq			 = "最大 IRQ/秒"
Enabled			 = "有効化"
Disabled		 = "無効化"
SpeedDuplex		 = "スピードと二重"
Auto		  	 = "自動ネゴシエーション"
10MHD		  	 = "10 Mbps 半二重"
10MFD		  	 = "10 Mbps 全二重"
100MHD			 = "100 Mbps 半二重"
100MFD			 = "100 Mbps 全二重"
FlowCtrl		 = "FlowControl"
ShutDW			 = "シャットダウン ウェークアップ"
RSS			 = "受信側スケーリング"
TXEna 			 = "Tx 有効化"
RXEna 			 = "Rx 有効化"
TXRXEna 		 = "Tx と Rx の有効化"
ReceiveBuffers 		 = "受信バッファ"
TransmitBuffers 	 = "送信バッファ"
IPChksumOffv4 		 = "IPv4 チェックサム オフロード"
TCPChksumOffv4 		 = "TCP チェックサム オフロード (IPv4)"
TCPChksumOffv6 		 = "TCP チェックサム オフロード (IPv6)"
UDPChksumOffv4 		 = "UDP チェックサム オフロード (IPv4)"
UDPChksumOffv6 		 = "UDP チェックサム オフロード (IPv6)"
LSOv1IPv4 		 = "大量送信オフロード (IPv4)"
NetAddress   		 = "ネットワーク アドレス"
WakeUpCapabilities       = "ウェークアップ機能"
APSmode			 = "APS モード"
None		         = "なし"
LinkChange	         = "リンク変更"
MagicPacket	         = "マジック パケット"
PatternMatch	         = "パターン マッチ"
MagicPacket_PatternMatch = "MagicPacket と PatternMatch"
All 			 = "すべて"

ATHR.L1E 		= "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
L1E.Service.DispName 	= "NDIS Miniport Driver for Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Dutch (Netherlands)
[Strings.0413]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Atheros"
JumboFrame  		 = "Jumboframe"
2KBMTU      		 = "2 KB MTU"
3KBMTU      		 = "3 KB MTU"
4KBMTU      		 = "4 KB MTU"
5KBMTU      		 = "5 KB MTU"
6KBMTU      		 = "6 KB MTU"
7KBMTU      		 = "7 KB MTU"
IntMod 			 = "Interruptcontrole"
MaxIrq			 = "Max. IRQ per seconde"
Enabled			 = "Ingeschakeld"
Disabled		 = "Uitgeschakeld"
SpeedDuplex		 = "Snelheid en duplex"
Auto		  	 = "Automatisch onderhandelen"
10MHD		  	 = "10 Mbps half-duplex"
10MFD		  	 = "10 Mbps volledige duplex"
100MHD			 = "100 Mbps half-duplex"
100MFD			 = "100 Mbps volledige duplex"
FlowCtrl		 = "FlowControl"
ShutDW			 = "Afsluiten Ontwaken"
RSS			 = "Schalen aan de ontvangstzijde"
TXEna 			 = "Tx ingeschakeld"
RXEna 			 = "Rx ingeschakeld"
TXRXEna 		 = "Tx en Rx ingeschakeld"
ReceiveBuffers 		 = "Buffers ontvangen"
TransmitBuffers 	 = "Buffers verzenden"
IPChksumOffv4 		 = "Offload van IPv4-controlesom"
TCPChksumOffv4 		 = "Offload van TCP-controlesom (IPv4)"
TCPChksumOffv6 		 = "Offload van TCP-controlesom (IPv6)"
UDPChksumOffv4 		 = "Offload van UDP-controlesom (IPv4)"
UDPChksumOffv6 		 = "Offload van UDP-controlesom (IPv6)"
LSOv1IPv4 		 = "Grote verzendings-offload (IPv4)"
NetAddress   		 = "Netwerkadres"
WakeUpCapabilities       = "Mogelijkheden voor ontwaken"
APSmode			 = "APS-modus"
None		         = "Geen"
LinkChange	         = "Wijziging koppeling"
MagicPacket	         = "Magic-pakket"
PatternMatch	         = "Patroonovereenkomst"
MagicPacket_PatternMatch = "Magic-pakket en Patroonovereenkomst"
All 			 = "Alles"

ATHR.L1E 		= "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
L1E.Service.DispName 	= "NDIS Miniport Driver for Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Portuguese (Brazil)
[Strings.0416]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Atheros"
JumboFrame  		 = "Jumbo Frame"
2KBMTU      		 = "2KB MTU"
3KBMTU      		 = "3KB MTU"
4KBMTU      		 = "4KB MTU"
5KBMTU      		 = "5KB MTU"
6KBMTU      		 = "6KB MTU"
7KBMTU      		 = "7KB MTU"
IntMod 			 = "Interromper Moderação"
MaxIrq			 = "Max IRQ por Segundo"
Enabled			 = "Activado"
Disabled		 = "Desactivado"
SpeedDuplex		 = "Velocidade e Duplex"
Auto		  	 = "Negociação Auotmática"
10MHD		  	 = "10 Mbps Half Duplex"
10MFD		  	 = "10 Mbps Full Duplex"
100MHD			 = "100 Mbps Half Duplex"
100MFD			 = "100 Mbps Full Duplex"
FlowCtrl		 = "FlowControl"
ShutDW			 = "Encerramento Reactivação"
RSS			 = "Receive Side Scaling"
TXEna 			 = "Tx Activada"
RXEna 			 = "Rx Activada"
TXRXEna 		 = "Tx e Rx Activadas"
ReceiveBuffers 		 = "Buffers de Recepção"
TransmitBuffers 	 = "Buffers de Transmissão"
IPChksumOffv4 		 = "IPv4 Checksum Offload"
TCPChksumOffv4 		 = "TCP Checksum Offload (IPv4)"
TCPChksumOffv6 		 = "TCP Checksum Offload (IPv6)"
UDPChksumOffv4 		 = "UDP Checksum Offload (IPv4)"
UDPChksumOffv6 		 = "UDP Checksum Offload (IPv6)"
LSOv1IPv4 		 = "Large Send Offload (IPv4)"
NetAddress   		 = "Endereço de Rede"
WakeUpCapabilities       = "Capacidades de Reactivação"
APSmode			 = "Modo APS"
None		         = "Nenhum"
LinkChange	         = "Alteração de Ligação"
MagicPacket	         = "Magic Packet"
PatternMatch	         = "Correspondência por Padrão"
MagicPacket_PatternMatch = "MagicPacket e Correspondência por Padrão"
All 			 = "Todos"

ATHR.L1E 		= "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
L1E.Service.DispName 	= "NDIS Miniport Driver for Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."
; Chinese (PRC)
[Strings.0804]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
ATHR 			 = "Atheros"
JumboFrame  		 = "Jumbo 帧"
2KBMTU      		 = "2KB MTU"
3KBMTU      		 = "3KB MTU"
4KBMTU      		 = "4KB MTU"
5KBMTU      		 = "5KB MTU"
6KBMTU      		 = "6KB MTU"
7KBMTU      		 = "7KB MTU"
IntMod 			 = "中断裁决"
MaxIrq			 = "每秒最大 IRQ"
Enabled			 = "启用"
Disabled		 = "禁用"
SpeedDuplex		 = "速度和双工"
Auto		  	 = "自动协商"
10MHD		  	 = "10 Mbps 半双工"
10MFD		  	 = "10 Mbps 全双工"
100MHD			 = "100 Mbps 半双工"
100MFD			 = "100 Mbps 全双工"
FlowCtrl		 = "流控制"
ShutDW			 = "关闭状态唤醒"
RSS			 = "接收方缩放"
TXEna 			 = "Tx 已启用"
RXEna 			 = "Rx 已启用"
TXRXEna 		 = "Tx 和 Rx 已启用"
ReceiveBuffers 		 = "接收缓冲区"
TransmitBuffers 	 = "传输缓冲区"
IPChksumOffv4 		 = "IPv4 校验和卸载"
TCPChksumOffv4 		 = "TCP 校验和卸载 (IPv4)"
TCPChksumOffv6 		 = "TCP 校验和卸载 (IPv6)"
UDPChksumOffv4 		 = "UDP 校验和卸载 (IPv4)"
UDPChksumOffv6 		 = "UDP 校验和卸载 (IPv6)"
LSOv1IPv4 		 = "大量发送卸载 (IPv4)"
NetAddress   		 = "网络地址"
WakeUpCapabilities       = "唤醒功能"
APSmode			 = "APS 模式"
None		         = "无"
LinkChange	         = "链接更改"
MagicPacket	         = "幻数据包"
PatternMatch	         = "模式匹配"
MagicPacket_PatternMatch = "MagicPacket & PatternMatch"
All 			 = "全部"

;; Do NOT translate
;---------------------------------------------------------------------------------------------------

;-----------------------------------------------------------------------------

ATHR.L1E 		= "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
L1E.Service.DispName 	= "NDIS Miniport Driver for Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."
