!_TAG_FILE_FORMAT	2	/extended format; --format=1 will not append ;" to lines/
!_TAG_FILE_SORTED	1	/0=unsorted, 1=sorted, 2=foldcase/
!_TAG_PROGRAM_AUTHOR	Darren Hiebert	/dhiebert@users.sourceforge.net/
!_TAG_PROGRAM_NAME	Exuberant Ctags	//
!_TAG_PROGRAM_URL	http://ctags.sourceforge.net	/official site/
!_TAG_PROGRAM_VERSION	5.7	//
AC0_BE	r8187.h	627;"	d
AC1_BK	r8187.h	628;"	d
AC2UP	ieee80211.h	965;"	d
AC2_VI	r8187.h	629;"	d
AC3_VO	r8187.h	630;"	d
ACCEPT_ALLMAC_FRAME_SHIFT	r8180_hw.h	136;"	d
ACCEPT_BCAST_FRAME_SHIFT	r8180_hw.h	134;"	d
ACCEPT_CRCERR_FRAME_SHIFT	r8180_hw.h	133;"	d
ACCEPT_CTL_FRAME_SHIFT	r8180_hw.h	130;"	d
ACCEPT_DATA_FRAME_SHIFT	r8180_hw.h	131;"	d
ACCEPT_ICVERR_FRAME_SHIFT	r8180_hw.h	132;"	d
ACCEPT_MCAST_FRAME_SHIFT	r8180_hw.h	135;"	d
ACCEPT_MNG_FRAME_SHIFT	r8180_hw.h	129;"	d
ACCEPT_NICMAC_FRAME_SHIFT	r8180_hw.h	137;"	d
ACCEPT_PWR_FRAME_SHIFT	r8180_hw.h	128;"	d
ACI	r8187.h	/^		u8	ACI:2;$/;"	m	struct:_ACI_AIFSN::__anon17
ACI_AIFSN	r8187.h	/^}ACI_AIFSN, *PACI_AIFSN;$/;"	t	typeref:union:_ACI_AIFSN
ACM	r8187.h	/^		u8	ACM:1;$/;"	m	struct:_ACI_AIFSN::__anon17
ACM_CONTROL	r8180_hw.h	433;"	d
ACM_HW_EN	r8180_hw.h	503;"	d
AC_BE_PARAM	r8180_hw.h	439;"	d
AC_BK_PARAM	r8180_hw.h	440;"	d
AC_CODING	r8187.h	/^typedef u32 AC_CODING;$/;"	t
AC_MAX	r8187.h	631;"	d
AC_PARAM	r8187.h	/^}AC_PARAM, *PAC_PARAM;$/;"	t	typeref:union:_AC_PARAM
AC_PARAM_AIFS_OFFSET	r8180_hw.h	495;"	d
AC_PARAM_ECW_MAX_OFFSET	r8180_hw.h	493;"	d
AC_PARAM_ECW_MIN_OFFSET	r8180_hw.h	494;"	d
AC_PARAM_TXOP_LIMIT_OFFSET	r8180_hw.h	492;"	d
AC_VI_PARAM	r8180_hw.h	438;"	d
AC_VO_PARAM	r8180_hw.h	437;"	d
AESMSK_FC	r8187.h	104;"	d
AESMSK_FC_DEFAULT	r8187.h	108;"	d
AESMSK_QC	r8187.h	106;"	d
AESMSK_QC_DEFAULT	r8187.h	110;"	d
AESMSK_SC	r8187.h	105;"	d
AESMSK_SC_DEFAULT	r8187.h	109;"	d
AGCRESET_SHIFT	r8180_hw.h	204;"	d
AIFSN	r8187.h	/^		u8	AIFSN:4;$/;"	m	struct:_ACI_AIFSN::__anon17
ALG_KEY_LEN	ieee80211.h	734;"	d
ANAPARAM	r8180_hw.h	179;"	d
ANAPARAM2	r8180_hw.h	333;"	d
ANAPARAM_PWR0_MASK	r8180_hw.h	66;"	d
ANAPARAM_PWR0_SHIFT	r8180_hw.h	67;"	d
ANAPARAM_PWR1_MASK	r8180_hw.h	68;"	d
ANAPARAM_PWR1_SHIFT	r8180_hw.h	69;"	d
ANAPARAM_TXDACOFF_SHIFT	r8180_hw.h	65;"	d
ANAPARM2_ASIC_ON	r8180_hw.h	746;"	d
ANAPARM2_ASIC_ON	r8180_hw.h	755;"	d
ANAPARM2_OFF	r8180_hw.h	762;"	d
ANAPARM2_ON	r8180_hw.h	758;"	d
ANAPARM_ASIC_ON	r8180_hw.h	744;"	d
ANAPARM_ASIC_ON	r8180_hw.h	754;"	d
ANAPARM_OFF	r8180_hw.h	761;"	d
ANAPARM_ON	r8180_hw.h	757;"	d
ANA_PARAM	r8180_hw.h	279;"	d
ANA_PARAM2	r8180_hw.h	296;"	d
ANA_PARAM2_END	r8180_hw.h	297;"	d
ANA_PARAM3	r8180_hw.h	466;"	d
ANA_PARAM_END	r8180_hw.h	280;"	d
ANTSEL	r8180_hw.h	342;"	d
ARFR	r8180_hw.h	368;"	d
ATIM	r8180_hw.h	185;"	d
ATIM_MASK	r8180_hw.h	183;"	d
AciAifsn	r8187.h	/^		ACI_AIFSN	AciAifsn;$/;"	m	struct:_AC_PARAM::__anon18
AckTimeOutReg	r8180_hw.h	315;"	d
AcmControl	r8187.h	/^	u8	AcmControl;$/;"	m	struct:r8180_priv
ActSetWirelessMode8187	r8180_rtl8225z2.c	/^void ActSetWirelessMode8187(struct net_device* dev, u8	btWirelessMode)$/;"	f
ActUpdateChannelAccessSetting	r8180_rtl8225z2.c	/^void ActUpdateChannelAccessSetting(struct net_device *dev,$/;"	f
ActionHeadLen	r8187_core.c	2480;"	d	file:
AtimWnd	r8180_hw.h	302;"	d
AtimWnd_AtimWnd	r8180_hw.h	700;"	d
AtimWnd_END	r8180_hw.h	303;"	d
AtimtrItv	r8180_hw.h	308;"	d
AtimtrItv_AtimtrItv	r8180_hw.h	704;"	d
AtimtrItv_END	r8180_hw.h	309;"	d
BBAddr	r8180_hw.h	317;"	d
BB_ANTATTEN_CHAN14	r8180_hw.h	56;"	d
BB_ANTENNA_B	r8180_hw.h	57;"	d
BB_HOST_BANG	r8180_hw.h	59;"	d
BB_HOST_BANG_CLK	r8180_hw.h	61;"	d
BB_HOST_BANG_DATA	r8180_hw.h	63;"	d
BB_HOST_BANG_EN	r8180_hw.h	60;"	d
BB_HOST_BANG_RW	r8180_hw.h	62;"	d
BEACON_INTERVAL	r8180_hw.h	180;"	d
BEACON_INTERVAL_MASK	r8180_hw.h	181;"	d
BEACON_PRIORITY	r8187.h	/^	BEACON_PRIORITY, \/\/0x0A$/;"	e	enum:__anon14
BEACON_PROBE_SSID_ID_POSITION	ieee80211.h	776;"	d
BEQ_ACM_CTL	r8180_hw.h	507;"	d
BEQ_ACM_EN	r8180_hw.h	502;"	d
BE_PRIORITY	r8187.h	/^	BE_PRIORITY,$/;"	e	enum:__anon14
BIT0	r8187.h	65;"	d
BIT1	r8187.h	66;"	d
BIT10	r8187.h	75;"	d
BIT11	r8187.h	76;"	d
BIT12	r8187.h	77;"	d
BIT13	r8187.h	78;"	d
BIT14	r8187.h	79;"	d
BIT15	r8187.h	80;"	d
BIT16	r8187.h	81;"	d
BIT17	r8187.h	82;"	d
BIT18	r8187.h	83;"	d
BIT19	r8187.h	84;"	d
BIT2	r8187.h	67;"	d
BIT20	r8187.h	85;"	d
BIT21	r8187.h	86;"	d
BIT22	r8187.h	87;"	d
BIT23	r8187.h	88;"	d
BIT24	r8187.h	89;"	d
BIT25	r8187.h	90;"	d
BIT26	r8187.h	91;"	d
BIT27	r8187.h	92;"	d
BIT28	r8187.h	93;"	d
BIT29	r8187.h	94;"	d
BIT3	r8187.h	68;"	d
BIT30	r8187.h	95;"	d
BIT31	r8187.h	96;"	d
BIT4	r8187.h	69;"	d
BIT5	r8187.h	70;"	d
BIT6	r8187.h	71;"	d
BIT7	r8187.h	72;"	d
BIT8	r8187.h	73;"	d
BIT9	r8187.h	74;"	d
BK_PRIORITY	r8187.h	/^	BK_PRIORITY,$/;"	e	enum:__anon14
BQREQ	r8180_hw.h	82;"	d
BRSR_8187	r8180_hw.h	243;"	d
BRSR_8187B	r8180_hw.h	245;"	d
BRSR_8187B_END	r8180_hw.h	246;"	d
BRSR_8187_END	r8180_hw.h	244;"	d
BRSR_BPLCP	r8180_hw.h	525;"	d
BRSR_MBR	r8180_hw.h	526;"	d
BRSR_MBR0	r8180_hw.h	528;"	d
BRSR_MBR1	r8180_hw.h	529;"	d
BRSR_MBR_8185	r8180_hw.h	527;"	d
BSSID	r8180_hw.h	248;"	d
BSSID_END	r8180_hw.h	249;"	d
BULK_PRIORITY	r8187.h	/^	BULK_PRIORITY = 0x01,$/;"	e	enum:__anon14
BcnIntTime	r8180_hw.h	80;"	d
BcnIntv	r8180_hw.h	299;"	d
BcnItv_BcnItv	r8180_hw.h	698;"	d
BcnItv_END	r8180_hw.h	300;"	d
BintrItv	r8180_hw.h	305;"	d
BintrItv_BintrItv	r8180_hw.h	702;"	d
BintrItv_END	r8180_hw.h	306;"	d
BlinkTimer	r8187_led.h	/^	struct timer_list		BlinkTimer;  \/\/ Timer object for led blinking.$/;"	m	struct:_LED_8187	typeref:struct:_LED_8187::timer_list
BlinkTimes	r8187_led.h	/^	u32				BlinkTimes; \/\/ Number of times to toggle led state for blinking.$/;"	m	struct:_LED_8187
BlinkingLedState	r8187_led.h	/^	LED_STATE_8187		BlinkingLedState; \/\/ Next state for blinking, either LED_ON or LED_OFF are.$/;"	m	struct:_LED_8187
CAM_AES	r8187.h	134;"	d
CAM_CONFIG_NO_USEDK	r8187.h	144;"	d
CAM_CONFIG_USEDK	r8187.h	143;"	d
CAM_CONTENT_COUNT	r8187.h	112;"	d
CAM_ENTRY_LEN_IN_BYTE	r8187.h	141;"	d
CAM_ENTRY_LEN_IN_DW	r8187.h	140;"	d
CAM_NONE	r8187.h	131;"	d
CAM_NOTVALID	r8187.h	127;"	d
CAM_POLLINIG	r8187.h	148;"	d
CAM_READ	r8187.h	147;"	d
CAM_TKIP	r8187.h	133;"	d
CAM_USEDK	r8187.h	128;"	d
CAM_VALID	r8187.h	126;"	d
CAM_WEP104	r8187.h	135;"	d
CAM_WEP40	r8187.h	132;"	d
CAM_WRITE	r8187.h	146;"	d
CAM_empty_entry	r8187_core.c	/^void CAM_empty_entry(struct net_device *dev, u8 ucIndex)$/;"	f
CAM_mark_invalid	r8187_core.c	/^void CAM_mark_invalid(struct net_device *dev, u8 ucIndex)$/;"	f
CARDBUS	r8187.h	/^	enum card_type {PCI,MINIPCI,CARDBUS,USB\/*rtl8187*\/}card_type;$/;"	e	enum:r8180_priv::card_type
CARRIER_SENSE_COUNTER	r8180_hw.h	192;"	d
CC	Makefile	/^CC = gcc$/;"	m
CCKLowerTh	r8187.h	/^	u16  CCKLowerTh;$/;"	m	struct:r8180_priv
CCKUpperTh	r8187.h	/^	u16  CCKUpperTh;$/;"	m	struct:r8180_priv
CCK_FALSE_ALARM	r8180_hw.h	443;"	d
CCK_TXAGC	r8180_hw.h	340;"	d
CFG_DEFAULT_KEY	r8187.h	113;"	d
CFG_IEEE80211_COMPUTE_FCS	ieee80211.h	1094;"	d
CFG_IEEE80211_RESERVE_FCS	ieee80211.h	1093;"	d
CFG_VALID	r8187.h	114;"	d
CFLAGS	Makefile	/^CFLAGS := -O2 -DMODULE -D__KERNEL__ ${WARN} ${INCLUDE}$/;"	m
CHANNEL_ACCESS_SETTING	r8187.h	/^}*PCHANNEL_ACCESS_SETTING,CHANNEL_ACCESS_SETTING;$/;"	t	typeref:struct:ChnlAccessSetting
CHANNEL_LIST	r8187.h	/^}CHANNEL_LIST, *PCHANNEL_LIST;$/;"	t	typeref:struct:_CHANNEL_LIST
CHECK_FOR_HANG_PERIOD	r8187.h	207;"	d
CIS	r8180_93cx6.h	36;"	d
CMD	r8180_hw.h	84;"	d
CMD_RESERVED_MASK	r8180_hw.h	86;"	d
CMD_RST_SHIFT	r8180_hw.h	85;"	d
CMD_RX_ENABLE_SHIFT	r8180_hw.h	87;"	d
CMD_TX_ENABLE_SHIFT	r8180_hw.h	88;"	d
CONFIG0	r8180_hw.h	275;"	d
CONFIG0_Aux_Status	r8180_hw.h	631;"	d
CONFIG0_GL	r8180_hw.h	632;"	d
CONFIG0_GL0	r8180_hw.h	634;"	d
CONFIG0_GL1	r8180_hw.h	633;"	d
CONFIG0_LEDGPO_En	r8180_hw.h	630;"	d
CONFIG0_WEP104	r8180_hw.h	629;"	d
CONFIG0_WEP104_SHIFT	r8180_hw.h	203;"	d
CONFIG0_WEP40_SHIFT	r8180_hw.h	202;"	d
CONFIG1	r8180_hw.h	276;"	d
CONFIG1_IOMAP	r8180_hw.h	641;"	d
CONFIG1_LEDS	r8180_hw.h	636;"	d
CONFIG1_LEDS0	r8180_hw.h	638;"	d
CONFIG1_LEDS1	r8180_hw.h	637;"	d
CONFIG1_LWACT	r8180_hw.h	639;"	d
CONFIG1_MEMMAP	r8180_hw.h	640;"	d
CONFIG1_PMEn	r8180_hw.h	643;"	d
CONFIG1_VPD	r8180_hw.h	642;"	d
CONFIG2	r8180_hw.h	277;"	d
CONFIG2_ANT	r8180_hw.h	646;"	d
CONFIG2_ANTENNA_SHIFT	r8180_hw.h	200;"	d
CONFIG2_DMA_POLLING_MODE_SHIFT	r8180_hw.h	102;"	d
CONFIG2_DPS	r8180_hw.h	647;"	d
CONFIG2_LCK	r8180_hw.h	645;"	d
CONFIG2_PAPE_sign	r8180_hw.h	648;"	d
CONFIG2_PAPE_time	r8180_hw.h	649;"	d
CONFIG2_PAPE_time0	r8180_hw.h	651;"	d
CONFIG2_PAPE_time1	r8180_hw.h	650;"	d
CONFIG3	r8180_hw.h	284;"	d
CONFIG3_ANAPARAM_W_SHIFT	r8180_hw.h	178;"	d
CONFIG3_CLKRUN_En	r8180_hw.h	657;"	d
CONFIG3_CLKRUN_SHIFT	r8180_hw.h	177;"	d
CONFIG3_CardB_En	r8180_hw.h	656;"	d
CONFIG3_FBtbEn	r8180_hw.h	659;"	d
CONFIG3_FuncRegEn	r8180_hw.h	658;"	d
CONFIG3_GNTSel	r8180_hw.h	653;"	d
CONFIG3_Magic	r8180_hw.h	655;"	d
CONFIG3_PARM_En	r8180_hw.h	654;"	d
CONFIG4	r8180_hw.h	285;"	d
CONFIG4_LWPME	r8180_hw.h	664;"	d
CONFIG4_LWPTN	r8180_hw.h	665;"	d
CONFIG4_PWRMGT	r8180_hw.h	663;"	d
CONFIG4_PWROFF	r8180_hw.h	662;"	d
CONFIG4_RFTYPE	r8180_hw.h	666;"	d
CONFIG4_RFTYPE0	r8180_hw.h	668;"	d
CONFIG4_RFTYPE1	r8180_hw.h	667;"	d
CONFIG4_VCOPDN	r8180_hw.h	661;"	d
CONFIG5	r8180_hw.h	449;"	d
CONFIG5_CALON	r8180_hw.h	672;"	d
CONFIG5_EACPI	r8180_hw.h	673;"	d
CONFIG5_LANWake	r8180_hw.h	674;"	d
CONFIG5_PME_STS	r8180_hw.h	675;"	d
CONFIG5_RX_FIFO_OK	r8180_hw.h	671;"	d
CONFIG5_TX_FIFO_OK	r8180_hw.h	670;"	d
CONFIG_RTL8180_IO_MAP	r8187_core.c	61;"	d	file:
CONF_WEP104	r8180_wx.c	844;"	d	file:
CONF_WEP40	r8180_wx.c	843;"	d	file:
CR9346	r8180_hw.h	273;"	d
CR9346_EECS	r8180_hw.h	624;"	d
CR9346_EED0	r8180_hw.h	627;"	d
CR9346_EED1	r8180_hw.h	626;"	d
CR9346_EEM	r8180_hw.h	621;"	d
CR9346_EEM0	r8180_hw.h	623;"	d
CR9346_EEM1	r8180_hw.h	622;"	d
CR9346_EESK	r8180_hw.h	625;"	d
CRC0	r8180_hw.h	397;"	d
CRC0_END	r8180_hw.h	398;"	d
CRC1	r8180_hw.h	399;"	d
CRC1_END	r8180_hw.h	400;"	d
CRC2	r8180_hw.h	401;"	d
CRC2_END	r8180_hw.h	402;"	d
CRC3	r8180_hw.h	403;"	d
CRC3_END	r8180_hw.h	404;"	d
CRC4	r8180_hw.h	405;"	d
CRC4_END	r8180_hw.h	406;"	d
CRC_LENGTH	ieee80211.h	925;"	d
CR_MulRW	r8180_hw.h	534;"	d
CR_RE	r8180_hw.h	532;"	d
CR_RST	r8180_hw.h	531;"	d
CR_TE	r8180_hw.h	533;"	d
CWR	r8180_hw.h	455;"	d
CWR_CW	r8180_hw.h	717;"	d
CWR_END	r8180_hw.h	456;"	d
CW_CONF	r8180_hw.h	357;"	d
CW_CONF_PERPACKET_CW	r8180_hw.h	359;"	d
CW_CONF_PERPACKET_CW_SHIFT	r8180_hw.h	361;"	d
CW_CONF_PERPACKET_RETRY_LIMIT	r8180_hw.h	358;"	d
CW_CONF_PERPACKET_RETRY_SHIFT	r8180_hw.h	360;"	d
CW_VAL	r8180_hw.h	356;"	d
CWmaxIndex	r8187.h	/^	u16 CWmaxIndex;$/;"	m	struct:ChnlAccessSetting
CWminIndex	r8187.h	/^	u16 CWminIndex;$/;"	m	struct:ChnlAccessSetting
CamResetAllEntry	r8187_core.c	/^void CamResetAllEntry(struct net_device *dev)$/;"	f
Channel	r8187.h	/^	u8	Channel[MAX_CHANNEL_NUMBER + 1];$/;"	m	struct:_CHANNEL_LIST
ChannelAccessSetting	r8187.h	/^	struct 	ChnlAccessSetting  ChannelAccessSetting;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::ChnlAccessSetting
CheckDig	r8180_dm.c	/^bool CheckDig(struct net_device *dev)$/;"	f
CheckHighPower	r8180_dm.c	/^bool CheckHighPower(struct net_device *dev)$/;"	f
ChnlAccessSetting	r8187.h	/^typedef struct 	ChnlAccessSetting {$/;"	s
ComputeTxTime	r8187_core.c	/^u16 ComputeTxTime( $/;"	f
Config4_PowerOff	r8180_hw.h	760;"	d
CurCCKRSSI	r8187.h	/^	u8   CurCCKRSSI;$/;"	m	struct:r8180_priv
CurrLedState	r8187_led.h	/^	LED_STATE_8187		CurrLedState; \/\/ Current LED state.$/;"	m	struct:_LED_8187
CurrRetryCnt	r8187.h	/^        u16                                     CurrRetryCnt;$/;"	m	struct:r8180_priv
CurrRetryRate	r8187.h	/^        u16                                     CurrRetryRate;$/;"	m	struct:r8180_priv
CurrTxRate	r8187.h	/^        u8                                      CurrTxRate;     \/\/the rate before up$/;"	m	struct:r8180_priv
CurrentOperaRate	r8187.h	/^        u8                  CurrentOperaRate;$/;"	m	struct:r8180_priv
CustomerID	r8187.h	/^        RT_CID_TYPE     CustomerID;$/;"	m	struct:r8180_priv
DCAM	r8187.h	102;"	d
DEBUG_EPROM	r8187_core.c	43;"	d	file:
DEBUG_IRQ	r8187_core.c	52;"	d	file:
DEBUG_IRQ_TASKLET	r8187_core.c	57;"	d	file:
DEBUG_REGISTERS	r8187_core.c	55;"	d	file:
DEBUG_RING	r8187_core.c	56;"	d	file:
DEBUG_RX	r8187_core.c	53;"	d	file:
DEBUG_RXALLOC	r8187_core.c	54;"	d	file:
DEBUG_RX_FRAG	r8187_core.c	49;"	d	file:
DEBUG_RX_SKB	r8187_core.c	47;"	d	file:
DEBUG_RX_VERBOSE	r8187_core.c	44;"	d	file:
DEBUG_TX	r8187_core.c	51;"	d	file:
DEBUG_TX_ALLOC	r8187_core.c	58;"	d	file:
DEBUG_TX_DESC	r8187_core.c	59;"	d	file:
DEBUG_TX_DESC2	r8187_core.c	41;"	d	file:
DEBUG_TX_FILLDESC	r8187_core.c	50;"	d	file:
DEBUG_TX_FRAG	r8187_core.c	48;"	d	file:
DEBUG_ZERO_RX	r8187_core.c	46;"	d	file:
DEFAULT_BEACONINTERVAL	r8187.h	158;"	d
DEFAULT_BEACON_ESSID	r8187.h	159;"	d
DEFAULT_FRAG_THRESHOLD	r8187.h	156;"	d
DEFAULT_FTS	ieee80211.h	1073;"	d
DEFAULT_KEEP_ALIVE_LEVEL	r8187.h	208;"	d
DEFAULT_MAX_SCAN_AGE	ieee80211.h	1072;"	d
DEFAULT_RATE_ADAPTIVE_TIMER_PERIOD	r8187_core.c	182;"	d	file:
DEFAULT_RETRY_DATA	r8187.h	163;"	d
DEFAULT_RETRY_RTS	r8187.h	162;"	d
DEFAULT_SLOT_NUM	r8187.h	205;"	d
DEFAULT_SSID	r8187.h	161;"	d
DIFS	r8180_hw.h	352;"	d
DIFS_Timer	r8187.h	/^	u16 DIFS_Timer; $/;"	m	struct:ChnlAccessSetting
DIG_NumberFallbackVote	r8187.h	/^	u8   DIG_NumberFallbackVote;$/;"	m	struct:r8180_priv
DIG_NumberUpgradeVote	r8187.h	/^	u8   DIG_NumberUpgradeVote;$/;"	m	struct:r8180_priv
DIG_Zebra	r8180_dm.c	/^void DIG_Zebra(struct net_device *dev)$/;"	f
DK0	r8180_hw.h	419;"	d
DK0_END	r8180_hw.h	420;"	d
DK1	r8180_hw.h	421;"	d
DK1_END	r8180_hw.h	422;"	d
DK2	r8180_hw.h	423;"	d
DK2_END	r8180_hw.h	424;"	d
DK3	r8180_hw.h	425;"	d
DK3_END	r8180_hw.h	426;"	d
DMESG	r8187.h	23;"	d
DMESGE	r8187.h	25;"	d
DMESGW	r8187.h	24;"	d
DUMMY_RX	r8187_core.c	45;"	d	file:
DUMP_RX	r8187_core.c	39;"	d	file:
DUMP_TX	r8187_core.c	40;"	d	file:
DeInitLed8187	r8187_led.c	/^DeInitLed8187($/;"	f
DeInitSwLeds	r8187_led.c	/^DeInitSwLeds($/;"	f
DefaultChannelPlan	r8187_core.c	/^CHANNEL_LIST	DefaultChannelPlan[] = {$/;"	v
DoRxHighPower	r8180_dm.c	/^void DoRxHighPower(struct net_device *dev)$/;"	f
DynamicCCKThreshold	r8180_dm.c	/^void DynamicCCKThreshold(struct net_device *dev)$/;"	f
DynamicInitGain	r8180_dm.c	/^void DynamicInitGain(struct net_device *dev)$/;"	f
EAPOL_ENCAP_ASF_ALERT	ieee80211.h	/^	EAPOL_ENCAP_ASF_ALERT$/;"	e	enum:eap_type
EAPOL_KEY	ieee80211.h	/^	EAPOL_KEY,$/;"	e	enum:eap_type
EAPOL_LOGOFF	ieee80211.h	/^	EAPOL_LOGOFF,$/;"	e	enum:eap_type
EAPOL_START	ieee80211.h	/^	EAPOL_START,$/;"	e	enum:eap_type
EAP_PACKET	ieee80211.h	/^	EAP_PACKET = 0,$/;"	e	enum:eap_type
ECW	r8187.h	/^}ECW, *PECW;$/;"	t	typeref:union:_ECW
ECWmax	r8187.h	/^		u8	ECWmax:4;$/;"	m	struct:_ECW::__anon16
ECWmin	r8187.h	/^		u8	ECWmin:4;$/;"	m	struct:_ECW::__anon16
EEPROMCustomerID	r8187.h	/^        u8                      EEPROMCustomerID;$/;"	m	struct:r8180_priv
EEPROM_CID_ALPHA0	r8187_led.h	37;"	d
EEPROM_CID_DELL	r8187_led.h	42;"	d
EEPROM_CID_HW_LED	r8187_led.h	39;"	d
EEPROM_CID_MASK	r8187_led.h	34;"	d
EEPROM_CID_QMI	r8187_led.h	41;"	d
EEPROM_CID_RSVD0	r8187_led.h	35;"	d
EEPROM_CID_RSVD1	r8187_led.h	36;"	d
EEPROM_CID_SERCOMM_PS	r8187_led.h	38;"	d
EEPROM_SW_REVD_OFFSET	r8187_led.h	32;"	d
EIFS_8187	r8180_hw.h	353;"	d
EIFS_8187B	r8180_hw.h	354;"	d
EIFS_Timer	r8187.h	/^	u16 EIFS_Timer;$/;"	m	struct:ChnlAccessSetting
EPROM_93c46	r8187.h	153;"	d
EPROM_93c56	r8187.h	154;"	d
EPROM_ANAPARAM_ADDRHWORD	r8180_93cx6.h	22;"	d
EPROM_ANAPARAM_ADDRLWORD	r8180_93cx6.h	21;"	d
EPROM_CHANNEL_PLAN	r8180_93cx6.h	24;"	d
EPROM_CK_SHIFT	r8180_hw.h	187;"	d
EPROM_CK_SHIFT	r8180_hw.h	99;"	d
EPROM_CMD	r8180_hw.h	90;"	d
EPROM_CMD_CONFIG	r8180_hw.h	94;"	d
EPROM_CMD_LOAD	r8180_hw.h	96;"	d
EPROM_CMD_NORMAL	r8180_hw.h	95;"	d
EPROM_CMD_OPERATING_MODE_MASK	r8180_hw.h	93;"	d
EPROM_CMD_OPERATING_MODE_SHIFT	r8180_hw.h	92;"	d
EPROM_CMD_PROGRAM	r8180_hw.h	97;"	d
EPROM_CMD_RESERVED_MASK	r8180_hw.h	91;"	d
EPROM_CONFIG2	r8180_93cx6.h	31;"	d
EPROM_CS_SHIFT	r8180_hw.h	186;"	d
EPROM_CS_SHIFT	r8180_hw.h	98;"	d
EPROM_DELAY	r8180_93cx6.h	19;"	d
EPROM_RFCHIPID	r8180_93cx6.h	26;"	d
EPROM_RFCHIPID_RTL8225U	r8180_93cx6.h	28;"	d
EPROM_RFCHIPID_RTL8225U_VF	r8180_93cx6.h	29;"	d
EPROM_RF_PARAM	r8180_93cx6.h	30;"	d
EPROM_R_SHIFT	r8180_hw.h	101;"	d
EPROM_TXPW0	r8180_93cx6.h	38;"	d
EPROM_TXPW1	r8180_93cx6.h	40;"	d
EPROM_TXPW2	r8180_93cx6.h	39;"	d
EPROM_TXPW_BASE	r8180_93cx6.h	27;"	d
EPROM_TYPE_SHIFT	r8180_hw.h	146;"	d
EPROM_VERSION	r8180_93cx6.h	33;"	d
EPROM_W_SHIFT	r8180_hw.h	100;"	d
ETHERTYPE_IP	ieee80211.h	982;"	d
ETHERTYPE_PAE	ieee80211.h	979;"	d
ETHER_ADDR_LEN	ieee80211.h	971;"	d
ETH_P_80211_RAW	ieee80211.h	480;"	d
ETH_P_PAE	ieee80211.h	474;"	d
ETH_P_PREAUTH	ieee80211.h	477;"	d
EarlyRxThreshold	r8187.h	/^	u16	EarlyRxThreshold;$/;"	m	struct:r8180_priv
Ecw	r8187.h	/^		ECW		Ecw;$/;"	m	struct:_AC_PARAM::__anon18
EnableHWSecurityConfig8187	r8187_core.c	/^void EnableHWSecurityConfig8187(struct net_device *dev)$/;"	f
FALSE	r8187.h	60;"	d
FEMR	r8180_hw.h	471;"	d
FEMR_END	r8180_hw.h	473;"	d
FEMR_GWAKE	r8180_hw.h	724;"	d
FEMR_INTR	r8180_hw.h	722;"	d
FEMR_WKUP	r8180_hw.h	723;"	d
FER	r8180_hw.h	468;"	d
FER_END	r8180_hw.h	469;"	d
FER_GWAKE	r8180_hw.h	720;"	d
FER_INTR	r8180_hw.h	719;"	d
FFER	r8180_hw.h	478;"	d
FFER_END	r8180_hw.h	479;"	d
FFER_GWAKE	r8180_hw.h	730;"	d
FFER_INTR	r8180_hw.h	729;"	d
FPSR	r8180_hw.h	475;"	d
FPSR_END	r8180_hw.h	476;"	d
FPSR_GWAKE	r8180_hw.h	727;"	d
FPSR_INTR	r8180_hw.h	726;"	d
FailTxRateCount	r8187.h	/^        u8                                      FailTxRateCount;$/;"	m	struct:r8180_priv
FalseAlarmRegValue	r8187.h	/^	u32  FalseAlarmRegValue; \/\/added by david, 2008.3.6	$/;"	m	struct:r8180_priv
GPE	r8180_hw.h	429;"	d
GPI	r8180_hw.h	430;"	d
GPIO	r8180_hw.h	337;"	d
GPIOChangeRFWorkItem	ieee80211.h	/^	struct delayed_work GPIOChangeRFWorkItem;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::delayed_work
GPIOChangeRFWorkItem	ieee80211.h	/^	struct work_struct GPIOChangeRFWorkItem;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::work_struct
GPIOChangeRFWorkItemCallBack	r8187_core.c	/^void GPIOChangeRFWorkItemCallBack(struct work_struct *work)$/;"	f
GPO	r8180_hw.h	428;"	d
GP_ENABLE	r8180_hw.h	336;"	d
GetDegradeTxRate	r8187_core.c	/^GetDegradeTxRate($/;"	f
GetSupportedWirelessMode8187	r8180_rtl8225z2.c	/^u8 GetSupportedWirelessMode8187(struct net_device* dev)$/;"	f
GetTxCckHighPowerBias	r8180_rtl8225.h	/^extern inline char GetTxCckHighPowerBias(struct net_device *dev)$/;"	f
GetTxOfdmHighPowerBias	r8180_rtl8225.h	/^extern inline  char GetTxOfdmHighPowerBias(struct net_device *dev)$/;"	f
GetUpgradeTxRate	r8187_core.c	/^GetUpgradeTxRate($/;"	f
Gpio0Led	r8187.h	/^        LED_8187        Gpio0Led;$/;"	m	struct:r8180_priv
Gpio0LedBlinkTimerCallback	r8187_led.c	/^Gpio0LedBlinkTimerCallback($/;"	f
Gpio0LedWorkItem	r8187.h	/^        struct work_struct              Gpio0LedWorkItem;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::work_struct
Gpio0LedWorkItemCallback	r8187_led.c	/^void Gpio0LedWorkItemCallback(struct work_struct *work)$/;"	f
HIGH_PRIORITY	r8187.h	/^	HIGH_PRIORITY,$/;"	e	enum:__anon14
HSSI_PARA	r8180_hw.h	338;"	d
HW_LED	r8187_led.h	/^	HW_LED, 		\/\/ HW control 2 LEDs, LED0 and LED1 (there are 4 different control modes, see MAC.CONFIG1 for details.)$/;"	e	enum:_LED_STRATEGY_8187
HW_THREE_WIRE	r8187.h	317;"	d
HW_THREE_WIRE_BY_8051	r8187.h	318;"	d
HW_VERID_R8180_ABCD	r8180_hw.h	571;"	d
HW_VERID_R8180_F	r8180_hw.h	570;"	d
HW_VERID_R8185_ABC	r8180_hw.h	572;"	d
HW_VERID_R8185_D	r8180_hw.h	573;"	d
IC_DEFAULT_THREE_WIRE	r8187.h	313;"	d
IDR0	r8180_hw.h	213;"	d
IDR1	r8180_hw.h	214;"	d
IDR2	r8180_hw.h	215;"	d
IDR3	r8180_hw.h	216;"	d
IDR4	r8180_hw.h	217;"	d
IDR5	r8180_hw.h	218;"	d
IEEE80211_24GHZ_BAND	ieee80211.h	576;"	d
IEEE80211_3ADDR_LEN	ieee80211.h	337;"	d
IEEE80211_4ADDR_LEN	ieee80211.h	338;"	d
IEEE80211_52GHZ_BAND	ieee80211.h	577;"	d
IEEE80211_ASSOCIATING	ieee80211.h	/^	IEEE80211_ASSOCIATING,$/;"	e	enum:ieee80211_state
IEEE80211_ASSOCIATING_AUTHENTICATED	ieee80211.h	/^	IEEE80211_ASSOCIATING_AUTHENTICATED,$/;"	e	enum:ieee80211_state
IEEE80211_ASSOCIATING_AUTHENTICATING	ieee80211.h	/^	IEEE80211_ASSOCIATING_AUTHENTICATING,$/;"	e	enum:ieee80211_state
IEEE80211_ASSOCIATING_RETRY	ieee80211.h	/^	IEEE80211_ASSOCIATING_RETRY,$/;"	e	enum:ieee80211_state
IEEE80211_BASIC_RATE_MASK	ieee80211.h	593;"	d
IEEE80211_CCK_BASIC_RATES_MASK	ieee80211.h	609;"	d
IEEE80211_CCK_DEFAULT_RATES_MASK	ieee80211.h	611;"	d
IEEE80211_CCK_MODULATION	ieee80211.h	573;"	d
IEEE80211_CCK_RATES_MASK	ieee80211.h	608;"	d
IEEE80211_CCK_RATE_11MB	ieee80211.h	583;"	d
IEEE80211_CCK_RATE_11MB_MASK	ieee80211.h	598;"	d
IEEE80211_CCK_RATE_1MB	ieee80211.h	580;"	d
IEEE80211_CCK_RATE_1MB_MASK	ieee80211.h	595;"	d
IEEE80211_CCK_RATE_2MB	ieee80211.h	581;"	d
IEEE80211_CCK_RATE_2MB_MASK	ieee80211.h	596;"	d
IEEE80211_CCK_RATE_5MB	ieee80211.h	582;"	d
IEEE80211_CCK_RATE_5MB_MASK	ieee80211.h	597;"	d
IEEE80211_CCK_RATE_LEN	ieee80211.h	579;"	d
IEEE80211_CRYPT_H	ieee80211_crypt.h	24;"	d
IEEE80211_DATA_HDR3_LEN	ieee80211.h	562;"	d
IEEE80211_DATA_HDR4_LEN	ieee80211.h	563;"	d
IEEE80211_DATA_LEN	ieee80211.h	213;"	d
IEEE80211_DEBUG	ieee80211.h	405;"	d
IEEE80211_DEBUG	ieee80211.h	410;"	d
IEEE80211_DEBUG_DROP	ieee80211.h	461;"	d
IEEE80211_DEBUG_EAP	ieee80211.h	460;"	d
IEEE80211_DEBUG_FRAG	ieee80211.h	459;"	d
IEEE80211_DEBUG_INFO	ieee80211.h	453;"	d
IEEE80211_DEBUG_MGMT	ieee80211.h	458;"	d
IEEE80211_DEBUG_RX	ieee80211.h	463;"	d
IEEE80211_DEBUG_SCAN	ieee80211.h	456;"	d
IEEE80211_DEBUG_STATE	ieee80211.h	457;"	d
IEEE80211_DEBUG_TX	ieee80211.h	462;"	d
IEEE80211_DEBUG_WX	ieee80211.h	455;"	d
IEEE80211_DEFAULT_BASIC_RATE	ieee80211.h	821;"	d
IEEE80211_DEFAULT_MESHID	ieee80211.h	822;"	d
IEEE80211_DEFAULT_MESH_CHAN	ieee80211.h	823;"	d
IEEE80211_DEFAULT_RATES_MASK	ieee80211.h	625;"	d
IEEE80211_DEFAULT_TX_ESSID	ieee80211.h	820;"	d
IEEE80211_DL_DROP	ieee80211.h	446;"	d
IEEE80211_DL_EAP	ieee80211.h	445;"	d
IEEE80211_DL_FRAG	ieee80211.h	444;"	d
IEEE80211_DL_INFO	ieee80211.h	439;"	d
IEEE80211_DL_MGMT	ieee80211.h	443;"	d
IEEE80211_DL_RX	ieee80211.h	449;"	d
IEEE80211_DL_SCAN	ieee80211.h	441;"	d
IEEE80211_DL_STATE	ieee80211.h	442;"	d
IEEE80211_DL_TX	ieee80211.h	448;"	d
IEEE80211_DL_WX	ieee80211.h	440;"	d
IEEE80211_DTIM_INVALID	ieee80211.h	936;"	d
IEEE80211_DTIM_MBCAST	ieee80211.h	933;"	d
IEEE80211_DTIM_UCAST	ieee80211.h	934;"	d
IEEE80211_DTIM_VALID	ieee80211.h	935;"	d
IEEE80211_ERROR	ieee80211.h	451;"	d
IEEE80211_FC0_SUBTYPE_MASK	ieee80211.h	229;"	d
IEEE80211_FC0_SUBTYPE_QOS	ieee80211.h	230;"	d
IEEE80211_FC0_TYPE_DATA	ieee80211.h	228;"	d
IEEE80211_FC0_TYPE_MASK	ieee80211.h	227;"	d
IEEE80211_FCS_LEN	ieee80211.h	339;"	d
IEEE80211_FCTL_DSTODS	ieee80211.h	350;"	d
IEEE80211_FCTL_FROMDS	ieee80211.h	349;"	d
IEEE80211_FCTL_FTYPE	ieee80211.h	346;"	d
IEEE80211_FCTL_MOREDATA	ieee80211.h	354;"	d
IEEE80211_FCTL_MOREFRAGS	ieee80211.h	351;"	d
IEEE80211_FCTL_ORDER	ieee80211.h	356;"	d
IEEE80211_FCTL_PM	ieee80211.h	353;"	d
IEEE80211_FCTL_RETRY	ieee80211.h	352;"	d
IEEE80211_FCTL_STYPE	ieee80211.h	347;"	d
IEEE80211_FCTL_TODS	ieee80211.h	348;"	d
IEEE80211_FCTL_VERS	ieee80211.h	345;"	d
IEEE80211_FCTL_WEP	ieee80211.h	355;"	d
IEEE80211_FRAG_CACHE_LEN	ieee80211.h	657;"	d
IEEE80211_FRAME_LEN	ieee80211.h	224;"	d
IEEE80211_FTYPE_CTL	ieee80211.h	359;"	d
IEEE80211_FTYPE_DATA	ieee80211.h	360;"	d
IEEE80211_FTYPE_MGMT	ieee80211.h	358;"	d
IEEE80211_H	ieee80211.h	25;"	d
IEEE80211_HLEN	ieee80211.h	223;"	d
IEEE80211_LINKED	ieee80211.h	/^	IEEE80211_LINKED,$/;"	e	enum:ieee80211_state
IEEE80211_LINKED_SCANNING	ieee80211.h	/^	IEEE80211_LINKED_SCANNING,$/;"	e	enum:ieee80211_state
IEEE80211_MESH_LINKED	ieee80211.h	/^	IEEE80211_MESH_LINKED,$/;"	e	enum:ieee80211_state
IEEE80211_MESH_SCANNING	ieee80211.h	/^	IEEE80211_MESH_SCANNING,$/;"	e	enum:ieee80211_state
IEEE80211_MGMT_HDR_LEN	ieee80211.h	561;"	d
IEEE80211_NOLINK	ieee80211.h	/^	IEEE80211_NOLINK = 0,$/;"	e	enum:ieee80211_state
IEEE80211_NUM_CCK_RATES	ieee80211.h	629;"	d
IEEE80211_NUM_OFDM_RATES	ieee80211.h	628;"	d
IEEE80211_OFDM_BASIC_RATES_MASK	ieee80211.h	616;"	d
IEEE80211_OFDM_DEFAULT_RATES_MASK	ieee80211.h	619;"	d
IEEE80211_OFDM_MODULATION	ieee80211.h	574;"	d
IEEE80211_OFDM_RATES_MASK	ieee80211.h	615;"	d
IEEE80211_OFDM_RATE_12MB	ieee80211.h	587;"	d
IEEE80211_OFDM_RATE_12MB_MASK	ieee80211.h	601;"	d
IEEE80211_OFDM_RATE_18MB	ieee80211.h	588;"	d
IEEE80211_OFDM_RATE_18MB_MASK	ieee80211.h	602;"	d
IEEE80211_OFDM_RATE_24MB	ieee80211.h	589;"	d
IEEE80211_OFDM_RATE_24MB_MASK	ieee80211.h	603;"	d
IEEE80211_OFDM_RATE_36MB	ieee80211.h	590;"	d
IEEE80211_OFDM_RATE_36MB_MASK	ieee80211.h	604;"	d
IEEE80211_OFDM_RATE_48MB	ieee80211.h	591;"	d
IEEE80211_OFDM_RATE_48MB_MASK	ieee80211.h	605;"	d
IEEE80211_OFDM_RATE_54MB	ieee80211.h	592;"	d
IEEE80211_OFDM_RATE_54MB_MASK	ieee80211.h	606;"	d
IEEE80211_OFDM_RATE_6MB	ieee80211.h	585;"	d
IEEE80211_OFDM_RATE_6MB_MASK	ieee80211.h	599;"	d
IEEE80211_OFDM_RATE_9MB	ieee80211.h	586;"	d
IEEE80211_OFDM_RATE_9MB_MASK	ieee80211.h	600;"	d
IEEE80211_OFDM_RATE_LEN	ieee80211.h	584;"	d
IEEE80211_OFDM_SHIFT_MASK_A	ieee80211.h	630;"	d
IEEE80211_PS_DISABLED	ieee80211.h	938;"	d
IEEE80211_PS_MBCAST	ieee80211.h	940;"	d
IEEE80211_PS_UNICAST	ieee80211.h	939;"	d
IEEE80211_QOS_HAS_SEQ	ieee80211.h	232;"	d
IEEE80211_QOS_TID	ieee80211.h	906;"	d
IEEE80211_SCTL_FRAG	ieee80211.h	397;"	d
IEEE80211_SCTL_SEQ	ieee80211.h	398;"	d
IEEE80211_SOFTMAC_ASSOC_RETRY_TIME	ieee80211.h	923;"	d
IEEE80211_SOFTMAC_SCAN_TIME	ieee80211.h	921;"	d
IEEE80211_STATMASK_NOISE	ieee80211.h	568;"	d
IEEE80211_STATMASK_RATE	ieee80211.h	569;"	d
IEEE80211_STATMASK_RSSI	ieee80211.h	567;"	d
IEEE80211_STATMASK_SIGNAL	ieee80211.h	566;"	d
IEEE80211_STATMASK_WEMASK	ieee80211.h	570;"	d
IEEE80211_STYPE_ACK	ieee80211.h	380;"	d
IEEE80211_STYPE_ASSOC_REQ	ieee80211.h	363;"	d
IEEE80211_STYPE_ASSOC_RESP	ieee80211.h	364;"	d
IEEE80211_STYPE_ATIM	ieee80211.h	370;"	d
IEEE80211_STYPE_AUTH	ieee80211.h	372;"	d
IEEE80211_STYPE_BEACON	ieee80211.h	369;"	d
IEEE80211_STYPE_CFACK	ieee80211.h	390;"	d
IEEE80211_STYPE_CFACKPOLL	ieee80211.h	392;"	d
IEEE80211_STYPE_CFEND	ieee80211.h	381;"	d
IEEE80211_STYPE_CFENDACK	ieee80211.h	382;"	d
IEEE80211_STYPE_CFPOLL	ieee80211.h	391;"	d
IEEE80211_STYPE_CTS	ieee80211.h	379;"	d
IEEE80211_STYPE_DATA	ieee80211.h	385;"	d
IEEE80211_STYPE_DATA_CFACK	ieee80211.h	386;"	d
IEEE80211_STYPE_DATA_CFACKPOLL	ieee80211.h	388;"	d
IEEE80211_STYPE_DATA_CFPOLL	ieee80211.h	387;"	d
IEEE80211_STYPE_DEAUTH	ieee80211.h	373;"	d
IEEE80211_STYPE_DISASSOC	ieee80211.h	371;"	d
IEEE80211_STYPE_MANAGE_ACT	ieee80211.h	374;"	d
IEEE80211_STYPE_NULLFUNC	ieee80211.h	389;"	d
IEEE80211_STYPE_PROBE_REQ	ieee80211.h	367;"	d
IEEE80211_STYPE_PROBE_RESP	ieee80211.h	368;"	d
IEEE80211_STYPE_PSPOLL	ieee80211.h	377;"	d
IEEE80211_STYPE_QOS_DATA	ieee80211.h	393;"	d
IEEE80211_STYPE_QOS_NULL	ieee80211.h	394;"	d
IEEE80211_STYPE_REASSOC_REQ	ieee80211.h	365;"	d
IEEE80211_STYPE_REASSOC_RESP	ieee80211.h	366;"	d
IEEE80211_STYPE_RTS	ieee80211.h	378;"	d
IEEE80211_WARNING	ieee80211.h	452;"	d
IEEE80211_WATCH_DOG_TIME	r8187_core.c	185;"	d	file:
IEEE_A	ieee80211.h	1521;"	d
IEEE_B	ieee80211.h	1522;"	d
IEEE_CMD_MLME	ieee80211.h	77;"	d
IEEE_CMD_SET_ENCRYPTION	ieee80211.h	76;"	d
IEEE_CMD_SET_WPA_IE	ieee80211.h	75;"	d
IEEE_CMD_SET_WPA_PARAM	ieee80211.h	74;"	d
IEEE_CRYPT_ALG_NAME_LEN	ieee80211.h	118;"	d
IEEE_CRYPT_ERR_CARD_CONF_FAILED	ieee80211.h	115;"	d
IEEE_CRYPT_ERR_CRYPT_INIT_FAILED	ieee80211.h	112;"	d
IEEE_CRYPT_ERR_KEY_SET_FAILED	ieee80211.h	113;"	d
IEEE_CRYPT_ERR_TX_KEY_SET_FAILED	ieee80211.h	114;"	d
IEEE_CRYPT_ERR_UNKNOWN_ADDR	ieee80211.h	111;"	d
IEEE_CRYPT_ERR_UNKNOWN_ALG	ieee80211.h	110;"	d
IEEE_G	ieee80211.h	1523;"	d
IEEE_IBSS_MAC_HASH_SIZE	ieee80211.h	237;"	d
IEEE_KEY_MGMT_IEEE8021X	ieee80211.h	101;"	d
IEEE_KEY_MGMT_PSK	ieee80211.h	102;"	d
IEEE_MESH_MAC_HASH_SIZE	ieee80211.h	238;"	d
IEEE_MLME_STA_DEAUTH	ieee80211.h	106;"	d
IEEE_MLME_STA_DISASSOC	ieee80211.h	107;"	d
IEEE_MODE_MASK	ieee80211.h	1524;"	d
IEEE_PARAM_AUTH_ALGS	ieee80211.h	83;"	d
IEEE_PARAM_DROP_UNENCRYPTED	ieee80211.h	81;"	d
IEEE_PARAM_IEEE_802_1X	ieee80211.h	84;"	d
IEEE_PARAM_PRIVACY_INVOKED	ieee80211.h	82;"	d
IEEE_PARAM_TKIP_COUNTERMEASURES	ieee80211.h	80;"	d
IEEE_PARAM_WPAX_SELECT	ieee80211.h	87;"	d
IEEE_PARAM_WPA_ENABLED	ieee80211.h	79;"	d
IEEE_PROTO_RSN	ieee80211.h	91;"	d
IEEE_PROTO_WPA	ieee80211.h	90;"	d
IEEE_SOFTMAC_ASSOCIATE	ieee80211.h	1534;"	d
IEEE_SOFTMAC_BEACONS	ieee80211.h	1555;"	d
IEEE_SOFTMAC_PROBERQ	ieee80211.h	1537;"	d
IEEE_SOFTMAC_PROBERS	ieee80211.h	1540;"	d
IEEE_SOFTMAC_SCAN	ieee80211.h	1531;"	d
IEEE_SOFTMAC_SINGLE_QUEUE	ieee80211.h	1550;"	d
IEEE_SOFTMAC_TX_QUEUE	ieee80211.h	1545;"	d
IEEE_WPAX_CCMP	ieee80211.h	98;"	d
IEEE_WPAX_TKIP	ieee80211.h	96;"	d
IEEE_WPAX_USEGROUP	ieee80211.h	94;"	d
IEEE_WPAX_WEP104	ieee80211.h	99;"	d
IEEE_WPAX_WEP40	ieee80211.h	95;"	d
IEEE_WPAX_WRAP	ieee80211.h	97;"	d
IMR	r8180_hw.h	255;"	d
IMR_ATIMInt	r8180_hw.h	539;"	d
IMR_BcnInt	r8180_hw.h	538;"	d
IMR_END	r8180_hw.h	256;"	d
IMR_RDU	r8180_hw.h	547;"	d
IMR_RER	r8180_hw.h	550;"	d
IMR_ROK	r8180_hw.h	551;"	d
IMR_RXFOVW	r8180_hw.h	546;"	d
IMR_TBDER	r8180_hw.h	540;"	d
IMR_TBDOK	r8180_hw.h	541;"	d
IMR_THPDER	r8180_hw.h	542;"	d
IMR_THPDOK	r8180_hw.h	543;"	d
IMR_TLPDER	r8180_hw.h	548;"	d
IMR_TLPDOK	r8180_hw.h	549;"	d
IMR_TNPDER	r8180_hw.h	544;"	d
IMR_TNPDOK	r8180_hw.h	545;"	d
IMR_TXFOVW	r8180_hw.h	536;"	d
IMR_TimeOut	r8180_hw.h	537;"	d
INCLUDE	Makefile	/^INCLUDE := -isystem \/lib\/modules\/`uname -r`\/build\/include$/;"	m
INSTALL_PREFIX	Makefile	/^INSTALL_PREFIX :=$/;"	m
INTA	r8180_hw.h	103;"	d
INTA_ATIM	r8180_hw.h	107;"	d
INTA_BEACONDESCERR	r8180_hw.h	108;"	d
INTA_BEACONDESCOK	r8180_hw.h	109;"	d
INTA_BEACONTIMEOUT	r8180_hw.h	106;"	d
INTA_HIPRIORITYDESCERR	r8180_hw.h	110;"	d
INTA_HIPRIORITYDESCOK	r8180_hw.h	111;"	d
INTA_LOWPRIORITYDESCERR	r8180_hw.h	116;"	d
INTA_LOWPRIORITYDESCOK	r8180_hw.h	117;"	d
INTA_MASK	r8180_hw.h	120;"	d
INTA_NORMPRIORITYDESCERR	r8180_hw.h	112;"	d
INTA_NORMPRIORITYDESCOK	r8180_hw.h	113;"	d
INTA_RXCRCERR	r8180_hw.h	118;"	d
INTA_RXDESCERR	r8180_hw.h	115;"	d
INTA_RXOK	r8180_hw.h	119;"	d
INTA_RXOVERFLOW	r8180_hw.h	114;"	d
INTA_TIMEOUT	r8180_hw.h	105;"	d
INTA_TXOVERFLOW	r8180_hw.h	104;"	d
INT_MIG	r8180_hw.h	434;"	d
INT_TIMEOUT	r8180_hw.h	176;"	d
IPSEnter	r8187_core.c	/^IPSEnter($/;"	f
IPSLeave	r8187_core.c	/^EXPORT_SYMBOL(IPSLeave);$/;"	v
IPSLeave	r8187_core.c	/^IPSLeave($/;"	f
ISR	r8180_hw.h	258;"	d
ISR_ATIMInt	r8180_hw.h	556;"	d
ISR_BcnInt	r8180_hw.h	555;"	d
ISR_END	r8180_hw.h	259;"	d
ISR_RDU	r8180_hw.h	564;"	d
ISR_RER	r8180_hw.h	567;"	d
ISR_ROK	r8180_hw.h	568;"	d
ISR_RXFOVW	r8180_hw.h	563;"	d
ISR_TBDER	r8180_hw.h	557;"	d
ISR_TBDOK	r8180_hw.h	558;"	d
ISR_THPDER	r8180_hw.h	559;"	d
ISR_THPDOK	r8180_hw.h	560;"	d
ISR_TLPDER	r8180_hw.h	565;"	d
ISR_TLPDOK	r8180_hw.h	566;"	d
ISR_TNPDER	r8180_hw.h	561;"	d
ISR_TNPDOK	r8180_hw.h	562;"	d
ISR_TXFOVW	r8180_hw.h	553;"	d
ISR_TimeOut	r8180_hw.h	554;"	d
IW_MODE_MESH	r8180_wx.c	34;"	d	file:
IW_QUAL_LEVEL_INVALID	ieee80211.h	176;"	d
IW_QUAL_LEVEL_UPDATED	ieee80211.h	179;"	d
IW_QUAL_NOISE_INVALID	ieee80211.h	177;"	d
IW_QUAL_NOISE_UPDATED	ieee80211.h	180;"	d
IW_QUAL_QUAL_INVALID	ieee80211.h	175;"	d
IW_QUAL_QUAL_UPDATED	ieee80211.h	178;"	d
IdleCount	r8187.h	/^	u8				IdleCount;     \/\/ (KEEP_ALIVE_INTERVAL \/ CHECK_FOR_HANG_PERIOD)$/;"	m	struct:_link_detect_t
InactivePowerSave	r8187_core.c	/^InactivePowerSave($/;"	f
IncludedInSupportedRates	r8187_core.c	/^IncludedInSupportedRates($/;"	f
InitLed8187	r8187_led.c	/^InitLed8187($/;"	f
InitSwLeds	r8187_led.c	/^InitSwLeds($/;"	f
InitialGain	r8187.h	/^	u8   InitialGain;$/;"	m	struct:r8180_priv
InitializeExtraRegsOn8185	r8180_rtl8225z2.c	/^InitializeExtraRegsOn8185(struct net_device	*dev)$/;"	f
KEEP_ALIVE_INTERVAL	r8187.h	206;"	d
KEY0	r8180_hw.h	199;"	d
KEY_BUF_SIZE	r8187.h	63;"	d
KEY_TYPE_CCMP	ieee80211.h	64;"	d
KEY_TYPE_NA	ieee80211.h	61;"	d
KEY_TYPE_TKIP	ieee80211.h	63;"	d
KEY_TYPE_WEP104	ieee80211.h	65;"	d
KEY_TYPE_WEP40	ieee80211.h	62;"	d
KSRC	Makefile	/^KSRC := \/lib\/modules\/$(KVER)\/build$/;"	m
KVER	Makefile	/^KVER  := $(shell uname -r)$/;"	m
LED_8187	r8187_led.h	/^} LED_8187, *PLED_8187;$/;"	t	typeref:struct:_LED_8187
LED_BLINK_CM3	r8187_led.h	/^	LED_BLINK_CM3 = 8, 		\/\/ Customzied for Sercomm Printer Server case$/;"	e	enum:_LED_STATE_8187
LED_BLINK_NORMAL	r8187_led.h	/^	LED_BLINK_NORMAL = 3,$/;"	e	enum:_LED_STATE_8187
LED_BLINK_NORMAL_INTERVAL	r8187_led.h	44;"	d
LED_BLINK_SLOWLY	r8187_led.h	/^	LED_BLINK_SLOWLY = 4,$/;"	e	enum:_LED_STATE_8187
LED_BLINK_SLOWLY_INTERVAL	r8187_led.h	45;"	d
LED_CM2_BLINK_OFF_INTERVAL	r8187_led.h	49;"	d
LED_CM2_BLINK_ON_INTERVAL	r8187_led.h	48;"	d
LED_CM3_BLINK_INTERVAL	r8187_led.h	53;"	d
LED_CM4_BLINK_OFF_INTERVAL	r8187_led.h	58;"	d
LED_CM4_BLINK_ON_INTERVAL	r8187_led.h	57;"	d
LED_CTL_LINK	ieee80211.h	/^	LED_CTL_LINK,$/;"	e	enum:_LED_CTL_MODE
LED_CTL_MODE	ieee80211.h	/^} LED_CTL_MODE;$/;"	t	typeref:enum:_LED_CTL_MODE
LED_CTL_NO_LINK	ieee80211.h	/^	LED_CTL_NO_LINK,$/;"	e	enum:_LED_CTL_MODE
LED_CTL_POWER_OFF	ieee80211.h	/^	LED_CTL_POWER_OFF,$/;"	e	enum:_LED_CTL_MODE
LED_CTL_POWER_ON	ieee80211.h	/^	LED_CTL_POWER_ON,$/;"	e	enum:_LED_CTL_MODE
LED_CTL_RX	ieee80211.h	/^	LED_CTL_RX,$/;"	e	enum:_LED_CTL_MODE
LED_CTL_SITE_SURVEY	ieee80211.h	/^	LED_CTL_SITE_SURVEY,$/;"	e	enum:_LED_CTL_MODE
LED_CTL_TX	ieee80211.h	/^	LED_CTL_TX,$/;"	e	enum:_LED_CTL_MODE
LED_NO_LINK_BLINK	r8187_led.h	/^	LED_NO_LINK_BLINK = 7,	\/\/ LED is blinking during no link state.$/;"	e	enum:_LED_STATE_8187
LED_OFF	r8187_led.h	/^	LED_OFF = 2,$/;"	e	enum:_LED_STATE_8187
LED_ON	r8187_led.h	/^	LED_ON = 1,$/;"	e	enum:_LED_STATE_8187
LED_PIN_8187	r8187_led.h	/^}LED_PIN_8187;$/;"	t	typeref:enum:_LED_PIN_8187
LED_PIN_GPIO0	r8187_led.h	/^	LED_PIN_GPIO0,$/;"	e	enum:_LED_PIN_8187
LED_PIN_LED0	r8187_led.h	/^	LED_PIN_LED0,$/;"	e	enum:_LED_PIN_8187
LED_PIN_LED1	r8187_led.h	/^	LED_PIN_LED1$/;"	e	enum:_LED_PIN_8187
LED_POWER_ON_BLINK	r8187_led.h	/^	LED_POWER_ON_BLINK = 5,$/;"	e	enum:_LED_STATE_8187
LED_SCAN_BLINK	r8187_led.h	/^	LED_SCAN_BLINK = 6, 	\/\/ LED is blinking during scanning period, the # of times to blink is depend on time for scanning.$/;"	e	enum:_LED_STATE_8187
LED_STATE_8187	r8187_led.h	/^}LED_STATE_8187;$/;"	t	typeref:enum:_LED_STATE_8187
LED_STRATEGY_8187	r8187_led.h	/^}LED_STRATEGY_8187, *PLED_STRATEGY_8187;$/;"	t	typeref:enum:_LED_STRATEGY_8187
LED_UNKNOWN	r8187_led.h	/^	LED_UNKNOWN = 0,$/;"	e	enum:_LED_STATE_8187
LOOP_TEST	r8187_core.c	38;"	d	file:
LOW_PRIORITY	r8187.h	/^	LOW_PRIORITY,$/;"	e	enum:__anon14
LastFailTxRate	r8187.h	/^        u8                                      LastFailTxRate;$/;"	m	struct:r8180_priv
LastFailTxRateSS	r8187.h	/^        long                            LastFailTxRateSS;$/;"	m	struct:r8180_priv
LastNumRxUnicast	r8187.h	/^	u32				LastNumRxUnicast;$/;"	m	struct:_link_detect_t
LastNumTxUnicast	r8187.h	/^	u32				LastNumTxUnicast;$/;"	m	struct:_link_detect_t
LastRetryCnt	r8187.h	/^    u16                                 LastRetryCnt;$/;"	m	struct:r8180_priv
LastRetryRate	r8187.h	/^        u16                                     LastRetryRate;$/;"	m	struct:r8180_priv
LastRxokCnt	r8187.h	/^        unsigned long           LastRxokCnt;$/;"	m	struct:r8180_priv
LastSignalStrengthInPercent	r8187.h	/^        long            LastSignalStrengthInPercent;$/;"	m	struct:r8180_priv
LastTxOKBytes	r8187.h	/^        unsigned long           LastTxOKBytes;$/;"	m	struct:r8180_priv
LastTxThroughput	r8187.h	/^        u32                             LastTxThroughput;$/;"	m	struct:r8180_priv
LastTxokCnt	r8187.h	/^        unsigned long           LastTxokCnt;$/;"	m	struct:r8180_priv
LedControl8187	r8187_led.c	/^LedControl8187($/;"	f
LedPin	r8187_led.h	/^	LED_PIN_8187		LedPin;	\/\/ Identify how to implement this SW led.$/;"	m	struct:_LED_8187
LedStrategy	r8187.h	/^        LED_STRATEGY_8187       LedStrategy;$/;"	m	struct:r8180_priv
Len	r8187.h	/^	u8	Len;$/;"	m	struct:_CHANNEL_LIST
ListenInterval	ieee80211.h	/^	u16 ListenInterval;$/;"	m	struct:ieee80211_device
LongRetryLimit	r8187.h	/^	u16	LongRetryLimit;$/;"	m	struct:r8180_priv
MAC0	r8180_hw.h	71;"	d
MAC1	r8180_hw.h	72;"	d
MAC2	r8180_hw.h	73;"	d
MAC3	r8180_hw.h	74;"	d
MAC4	r8180_hw.h	75;"	d
MAC5	r8180_hw.h	76;"	d
MAC_ADR	r8180_93cx6.h	34;"	d
MAC_ARG	ieee80211.h	1075;"	d
MAC_FILTER_MASK	r8180_hw.h	125;"	d
MAC_FMT	ieee80211.h	1074;"	d
MAC_REG_TABLE	r8180_rtl8225z2.c	/^static u32 MAC_REG_TABLE[][3]={ $/;"	v	file:
MAC_TABLE_SIZE	msh_class.h	21;"	d
MANAGE_PRIORITY	r8187.h	/^	MANAGE_PRIORITY,$/;"	e	enum:__anon14
MAR0	r8180_hw.h	222;"	d
MAR1	r8180_hw.h	223;"	d
MAR2	r8180_hw.h	224;"	d
MAR3	r8180_hw.h	225;"	d
MAR4	r8180_hw.h	226;"	d
MAR5	r8180_hw.h	227;"	d
MAR6	r8180_hw.h	228;"	d
MAR7	r8180_hw.h	229;"	d
MAX_CHANNEL_NUMBER	ieee80211.h	919;"	d
MAX_DOZE_WAITING_TIMES_87B	r8180_hw.h	765;"	d
MAX_DOZE_WAITING_TIMES_87B	r8187_core.c	4936;"	d	file:
MAX_FRAG_THRESHOLD	ieee80211.h	342;"	d
MAX_KEY_LEN	r8187.h	62;"	d
MAX_LD_SLOT_NUM	r8187.h	204;"	d
MAX_MP	ieee80211.h	737;"	d
MAX_NETWORK_COUNT	ieee80211.h	918;"	d
MAX_RATES_EX_LENGTH	ieee80211.h	917;"	d
MAX_RATES_LENGTH	ieee80211.h	916;"	d
MAX_RESP_RATE_SHIFT	r8180_hw.h	362;"	d
MAX_RX_DMA_1024	r8180_hw.h	174;"	d
MAX_RX_DMA_2048	r8180_hw.h	173;"	d
MAX_RX_DMA_MASK	r8180_hw.h	172;"	d
MAX_RX_DMA_SHIFT	r8180_hw.h	175;"	d
MAX_RX_URB	r8180_hw.h	49;"	d
MAX_SP_Len	ieee80211.h	905;"	d
MAX_SWEEP_TAB_ENTRIES	ieee80211.h	910;"	d
MAX_SWEEP_TAB_ENTRIES_PER_PACKET	ieee80211.h	911;"	d
MAX_TX_URB	r8180_hw.h	48;"	d
MAX_WPA_IE_LEN	ieee80211.h	927;"	d
MFIE_TYPE_CF_SET	ieee80211.h	783;"	d
MFIE_TYPE_CHALLENGE	ieee80211.h	786;"	d
MFIE_TYPE_DS_SET	ieee80211.h	782;"	d
MFIE_TYPE_ERP	ieee80211.h	787;"	d
MFIE_TYPE_FH_SET	ieee80211.h	781;"	d
MFIE_TYPE_GENERIC	ieee80211.h	790;"	d
MFIE_TYPE_IBSS_SET	ieee80211.h	785;"	d
MFIE_TYPE_RATES	ieee80211.h	780;"	d
MFIE_TYPE_RATES_EX	ieee80211.h	789;"	d
MFIE_TYPE_RSN	ieee80211.h	788;"	d
MFIE_TYPE_SSID	ieee80211.h	779;"	d
MFIE_TYPE_TIM	ieee80211.h	784;"	d
MGMT_QUEUE_NUM	ieee80211.h	71;"	d
MINIPCI	r8187.h	/^	enum card_type {PCI,MINIPCI,CARDBUS,USB\/*rtl8187*\/}card_type;$/;"	e	enum:r8180_priv::card_type
MIN_FRAG_THRESHOLD	ieee80211.h	341;"	d
MIN_FRAG_THRESHOLD	r8187.h	157;"	d
MIN_RESP_RATE_SHIFT	r8180_hw.h	363;"	d
MODDESTDIR	Makefile	/^MODDESTDIR := \/lib\/modules\/$(KVER)\/kernel\/drivers\/net\/wireless\/$(NIC_SELECT)$/;"	m
MSECS	ieee80211.h	197;"	d
MSECS	ieee80211.h	209;"	d
MSR	r8180_hw.h	282;"	d
MSR_LINK_ADHOC	r8180_hw.h	681;"	d
MSR_LINK_ENEDCA	r8180_hw.h	683;"	d
MSR_LINK_MANAGED	r8180_hw.h	678;"	d
MSR_LINK_MASK	r8180_hw.h	677;"	d
MSR_LINK_MASTER	r8180_hw.h	682;"	d
MSR_LINK_NONE	r8180_hw.h	679;"	d
MSR_LINK_SHIFT	r8180_hw.h	680;"	d
MacConfig_87BASIC	r8180_rtl8225z2.c	/^static void MacConfig_87BASIC(struct net_device *dev)$/;"	f	file:
MacConfig_87BASIC_HardCode	r8180_rtl8225z2.c	/^MacConfig_87BASIC_HardCode(struct net_device *dev)$/;"	f
MgntActSet_RF_State	r8187_core.c	/^MgntActSet_RF_State($/;"	f
MgntIsCckRate	r8187_core.c	/^MgntIsCckRate($/;"	f
NETWORK_EMPTY_ESSID	ieee80211.h	929;"	d
NETWORK_HAS_CCK	ieee80211.h	931;"	d
NETWORK_HAS_OFDM	ieee80211.h	930;"	d
NIC_8187	r8187.h	/^	NIC_8187 = 1,$/;"	e	enum:__anon15
NIC_8187B	r8187.h	/^	NIC_8187B$/;"	e	enum:__anon15
NIC_SELECT	Makefile	/^NIC_SELECT = RTL8187B$/;"	m
NORM_PRIORITY	r8187.h	/^	NORM_PRIORITY, $/;"	e	enum:__anon14
N_DBPSOfRate	r8187_core.c	/^u16 N_DBPSOfRate(u16 DataRate)$/;"	f
NetgearSignalStrengthTranslate	r8187_core.c	/^long NetgearSignalStrengthTranslate(long LastSS,long CurrSS)$/;"	f
NumRxBcnInPeriod	ieee80211.h	/^	unsigned long NumRxBcnInPeriod;  \/\/YJ,add,080828$/;"	m	struct:ieee80211_device
NumRxData	ieee80211.h	/^	u32 NumRxData;$/;"	m	struct:ieee80211_device
NumRxDataInPeriod	ieee80211.h	/^	unsigned long NumRxDataInPeriod; \/\/YJ,add,080828$/;"	m	struct:ieee80211_device
NumRxOkInPeriod	r8187.h	/^	u32				NumRxOkInPeriod;  \/\/number of packet received during CheckForHang$/;"	m	struct:_link_detect_t
NumRxOkInPeriod	r8187.h	/^	u32 NumRxOkInPeriod;$/;"	m	struct:r8180_priv
NumTxOkInPeriod	r8187.h	/^	u32				NumTxOkInPeriod;  \/\/number of packet transmitted during CheckForHang$/;"	m	struct:_link_detect_t
NumTxOkInPeriod	r8187.h	/^	u32 NumTxOkInPeriod;$/;"	m	struct:r8180_priv
OBJS	Makefile	/^OBJS := ${patsubst %.c, %.o, ${wildcard *.c}}$/;"	m
OFDM_CONFIG	r8180_rtl8225z2.c	/^static u8 OFDM_CONFIG[]={$/;"	v	file:
OFDM_FALSE_ALARM	r8180_hw.h	444;"	d
OFDM_TXAGC	r8180_hw.h	341;"	d
P80211_OUI_LEN	ieee80211.h	485;"	d
PACI_AIFSN	r8187.h	/^}ACI_AIFSN, *PACI_AIFSN;$/;"	t	typeref:union:_ACI_AIFSN
PAC_PARAM	r8187.h	/^}AC_PARAM, *PAC_PARAM;$/;"	t	typeref:union:_AC_PARAM
PCHANNEL_ACCESS_SETTING	r8187.h	/^}*PCHANNEL_ACCESS_SETTING,CHANNEL_ACCESS_SETTING;$/;"	t	typeref:struct:ChnlAccessSetting
PCHANNEL_LIST	r8187.h	/^}CHANNEL_LIST, *PCHANNEL_LIST;$/;"	t	typeref:struct:_CHANNEL_LIST
PCI	r8187.h	/^	enum card_type {PCI,MINIPCI,CARDBUS,USB\/*rtl8187*\/}card_type;$/;"	e	enum:r8180_priv::card_type
PECW	r8187.h	/^}ECW, *PECW;$/;"	t	typeref:union:_ECW
PGSELECT	r8180_hw.h	122;"	d
PGSELECT_PG_SHIFT	r8180_hw.h	123;"	d
PHY_ADR	r8180_hw.h	190;"	d
PHY_CONFIG	r8180_hw.h	189;"	d
PHY_DELAY	r8180_hw.h	188;"	d
PHY_READ	r8180_hw.h	191;"	d
PLED_8187	r8187_led.h	/^} LED_8187, *PLED_8187;$/;"	t	typeref:struct:_LED_8187
PLED_STRATEGY_8187	r8187_led.h	/^}LED_STRATEGY_8187, *PLED_STRATEGY_8187;$/;"	t	typeref:enum:_LED_STRATEGY_8187
PRF_TYPE_8187	r8180_hw.h	/^}RF_TYPE_8187,*PRF_TYPE_8187;$/;"	t	typeref:enum:_RF_TYPE_8187
PRI2EP	r8187_core.c	/^unsigned int PRI2EP[4] = {0x06,0x07,0x05,0x04};$/;"	v
PRISM_HDR_SIZE	r8187.h	164;"	d
PSR	r8180_hw.h	291;"	d
PSR_GPI	r8180_hw.h	686;"	d
PSR_GPO	r8180_hw.h	685;"	d
PSR_LEDGPO0	r8180_hw.h	688;"	d
PSR_LEDGPO1	r8180_hw.h	687;"	d
PSR_PSEn	r8180_hw.h	690;"	d
PSR_UWF	r8180_hw.h	689;"	d
PTR_SWITCH_STATE	r8187.h	/^}TR_SWITCH_STATE, *PTR_SWITCH_STATE;$/;"	t	typeref:enum:_TR_SWITCH_STATE
PVERSION_8187	r8180_hw.h	/^}VERSION_8187,*PVERSION_8187;$/;"	t	typeref:enum:_VERSION_8187
PWD	Makefile	/^PWD = $(shell pwd)$/;"	m
PerformUndecoratedSignalSmoothing8187	r8187_core.c	/^void PerformUndecoratedSignalSmoothing8187(struct net_device *dev, struct ieee80211_rx_stats *stats)$/;"	f
PhyAddr	r8180_hw.h	320;"	d
PhyCFG	r8180_hw.h	325;"	d
PhyCFG_END	r8180_hw.h	326;"	d
PhyConfig8187	r8180_rtl8225z2.c	/^void PhyConfig8187(struct net_device *dev)$/;"	f
PhyDataR	r8180_hw.h	322;"	d
PhyDataW	r8180_hw.h	321;"	d
PhyDelay	r8180_hw.h	311;"	d
PhyDelay_PhyDelay	r8180_hw.h	706;"	d
PlatformSwLedBlink	r8187_led.c	/^PlatformSwLedBlink($/;"	f
PsrValue	r8187.h	/^        u8                      PsrValue;$/;"	m	struct:r8180_priv
QOS_CTL_NOTCONTAIN_ACK	ieee80211.h	907;"	d
QOS_ctl	ieee80211.h	/^	u16 QOS_ctl;$/;"	m	struct:ieee80211_hdr_3addr_QOS
QOS_ctl	ieee80211.h	/^	u16 QOS_ctl;$/;"	m	struct:ieee80211_hdr_QOS
QoS_Enable	ieee80211.h	/^	u8 QoS_Enable;$/;"	m	struct:ieee80211_network
R8180H	r8187.h	19;"	d
R8180_DM_H	r8180_dm.h	8;"	d
R8180_HW	r8180_hw.h	21;"	d
R8180_MAX_RETRY	r8180_hw.h	156;"	d
R8180_PM_H	r8180_pm.h	16;"	d
R8180_WX_H	r8180_wx.h	16;"	d
R8187_LED_H	r8187_led.h	21;"	d
RATE_COUNT	r8180_wx.c	31;"	d	file:
RATE_FALLBACK	r8180_hw.h	364;"	d
RATE_FALLBACK_CTL_AUTO_STEP0	r8180_hw.h	366;"	d
RATE_FALLBACK_CTL_ENABLE	r8180_hw.h	365;"	d
RCAMO	r8187.h	101;"	d
RCR	r8180_hw.h	264;"	d
RCR_9356SEL	r8180_hw.h	614;"	d
RCR_AAP	r8180_hw.h	619;"	d
RCR_AB	r8180_hw.h	616;"	d
RCR_ACF	r8180_hw.h	603;"	d
RCR_ACRC32	r8180_hw.h	615;"	d
RCR_ADD3	r8180_hw.h	601;"	d
RCR_ADF	r8180_hw.h	604;"	d
RCR_AICV	r8180_hw.h	609;"	d
RCR_AM	r8180_hw.h	617;"	d
RCR_AMF	r8180_hw.h	602;"	d
RCR_APM	r8180_hw.h	618;"	d
RCR_APWRMGT	r8180_hw.h	600;"	d
RCR_CBSSID	r8180_hw.h	599;"	d
RCR_CS_MASK	r8180_hw.h	597;"	d
RCR_CS_SHIFT	r8180_hw.h	596;"	d
RCR_END	r8180_hw.h	265;"	d
RCR_ENMARP	r8180_hw.h	598;"	d
RCR_MXDMA	r8180_hw.h	610;"	d
RCR_MXDMA0	r8180_hw.h	613;"	d
RCR_MXDMA1	r8180_hw.h	612;"	d
RCR_MXDMA2	r8180_hw.h	611;"	d
RCR_ONLYERLPKT	r8180_hw.h	595;"	d
RCR_RXFTH	r8180_hw.h	605;"	d
RCR_RXFTH0	r8180_hw.h	608;"	d
RCR_RXFTH1	r8180_hw.h	607;"	d
RCR_RXFTH2	r8180_hw.h	606;"	d
RDSAR	r8180_hw.h	462;"	d
RDSAR_END	r8180_hw.h	463;"	d
RESP_RATE	r8180_hw.h	350;"	d
RFChangeInProgress	r8187.h	/^	bool RFChangeInProgress;$/;"	m	struct:r8180_priv
RFPinsEnable	r8180_hw.h	330;"	d
RFPinsInput	r8180_hw.h	335;"	d
RFPinsOutput	r8180_hw.h	329;"	d
RFPinsSelect	r8180_hw.h	332;"	d
RFProgType	r8187.h	/^	u8	RFProgType;$/;"	m	struct:r8180_priv
RFSW_CTRL	r8180_hw.h	485;"	d
RFTiming	r8180_hw.h	432;"	d
RF_CHANGE_BY_HW	r8180_hw.h	751;"	d
RF_CHANGE_BY_IPS	r8180_hw.h	753;"	d
RF_CHANGE_BY_PS	r8180_hw.h	752;"	d
RF_CHANGE_BY_SW	r8180_hw.h	750;"	d
RF_PARA	r8180_hw.h	334;"	d
RF_Ready	r8180_hw.h	323;"	d
RF_TIMING	r8180_hw.h	331;"	d
RF_TYPE_8187	r8180_hw.h	/^}RF_TYPE_8187,*PRF_TYPE_8187;$/;"	t	typeref:enum:_RF_TYPE_8187
RF_TYPE_MAX	r8180_hw.h	/^	RF_TYPE_MAX,$/;"	e	enum:_RF_TYPE_8187
RF_TYPE_MIN	r8180_hw.h	/^	RF_TYPE_MIN,$/;"	e	enum:_RF_TYPE_8187
RF_ZEBRA	r8180_hw.h	/^	RF_ZEBRA = 5,$/;"	e	enum:_RF_TYPE_8187
RF_ZEBRA2	r8180_hw.h	/^	RF_ZEBRA2,		\/\/ added by Annie, 2005-08-01.$/;"	e	enum:_RF_TYPE_8187
RMS	r8180_hw.h	369;"	d
RSVD2	r8187.h	/^	RSVD2,$/;"	e	enum:__anon14
RSVD3	r8187.h	/^	RSVD3,$/;"	e	enum:__anon14
RSVD4	r8187.h	/^	RSVD4,$/;"	e	enum:__anon14
RSVD5	r8187.h	/^	RSVD5,$/;"	e	enum:__anon14
RTL8187_MODULE_NAME	r8187.h	22;"	d
RTL8187_REQT_READ	r8180_hw.h	41;"	d
RTL8187_REQT_WRITE	r8180_hw.h	42;"	d
RTL8187_REQ_GET_REGS	r8180_hw.h	43;"	d
RTL8187_REQ_SET_REGS	r8180_hw.h	44;"	d
RTL8187_RF_INDEX	r8180_hw.h	40;"	d
RTL8225H	r8180_rtl8225.h	14;"	d
RTL8225_ANAPARAM2_OFF	r8180_rtl8225.h	22;"	d
RTL8225_ANAPARAM2_ON	r8180_rtl8225.h	24;"	d
RTL8225_ANAPARAM_OFF	r8180_rtl8225.h	21;"	d
RTL8225_ANAPARAM_ON	r8180_rtl8225.h	18;"	d
RTL8225_RF_DEF_SENS	r8180_rtl8225.h	45;"	d
RTL8225_RF_MAX_SENS	r8180_rtl8225.h	44;"	d
RTL_IOCTL_WPA_SUPPLICANT	r8187.h	180;"	d
RT_CID_8187_ALPHA0	r8187_led.h	/^	RT_CID_8187_ALPHA0,$/;"	e	enum:_RT_CID_TYPE
RT_CID_8187_HW_LED	r8187_led.h	/^	RT_CID_8187_HW_LED,$/;"	e	enum:_RT_CID_TYPE
RT_CID_8187_SERCOMM_PS	r8187_led.h	/^	RT_CID_8187_SERCOMM_PS,$/;"	e	enum:_RT_CID_TYPE
RT_CID_87B_DELL	r8187_led.h	/^	RT_CID_87B_DELL,	\/\/Added by lizhaoming 2008.6.3$/;"	e	enum:_RT_CID_TYPE
RT_CID_87B_QMI	r8187_led.h	/^	RT_CID_87B_QMI ,	\/\/Added by lizhaoming 2008.6.3$/;"	e	enum:_RT_CID_TYPE
RT_CID_DEFAULT	r8187_led.h	/^	RT_CID_DEFAULT,$/;"	e	enum:_RT_CID_TYPE
RT_CID_TYPE	r8187_led.h	/^} RT_CID_TYPE;$/;"	t	typeref:enum:_RT_CID_TYPE
RT_PS_MODE	r8187.h	/^}RT_PS_MODE;$/;"	t	typeref:enum:_RT_PS_MODE
RT_RF_POWER_STATE	r8187.h	/^}RT_RF_POWER_STATE;$/;"	t	typeref:enum:_RT_RF_POWER_STATE
RWCAM	r8187.h	99;"	d
RXFIFOCOUNT	r8180_hw.h	78;"	d
RXRING_ADDR	r8180_hw.h	121;"	d
RX_AUTORESETPHY_SHIFT	r8180_hw.h	145;"	d
RX_CHECK_BSSID_SHIFT	r8180_hw.h	127;"	d
RX_CONF	r8180_hw.h	124;"	d
RX_DONT_PASS_UL	r8187_core.c	42;"	d	file:
RX_FIFO_THRESHOLD_1024	r8180_hw.h	143;"	d
RX_FIFO_THRESHOLD_128	r8180_hw.h	140;"	d
RX_FIFO_THRESHOLD_256	r8180_hw.h	141;"	d
RX_FIFO_THRESHOLD_512	r8180_hw.h	142;"	d
RX_FIFO_THRESHOLD_MASK	r8180_hw.h	138;"	d
RX_FIFO_THRESHOLD_NONE	r8180_hw.h	144;"	d
RX_FIFO_THRESHOLD_SHIFT	r8180_hw.h	139;"	d
RX_URB_SIZE	r8180_hw.h	50;"	d
ReceiveConfig	r8187.h	/^	u32	ReceiveConfig;$/;"	m	struct:r8180_priv
RecvSignalPower	r8187.h	/^        long                            RecvSignalPower;$/;"	m	struct:r8180_priv
RegBModeGainStage	r8187.h	/^	u8   RegBModeGainStage;$/;"	m	struct:r8180_priv
RegCWinMin	r8187.h	/^	u8	RegCWinMin;		\/\/ For turbo mode CW adaptive. Added by Annie, 2005-10-27.$/;"	m	struct:r8180_priv
RegDigOfdmFaUpTh	r8187.h	/^	u8   RegDigOfdmFaUpTh;	 \/\/added by david, 2008.3.6$/;"	m	struct:r8180_priv
RegThreeWireMode	r8187.h	/^	u8 RegThreeWireMode;$/;"	m	struct:r8180_priv
Reserved	r8187.h	/^		u8	Reserved:1;$/;"	m	struct:_ACI_AIFSN::__anon17
RetryCTR	r8180_hw.h	458;"	d
RfOffReason	r8187.h	/^	u32 RfOffReason;$/;"	m	struct:r8180_priv
RxFrameNum	r8187.h	/^	u32				RxFrameNum[MAX_LD_SLOT_NUM];	\/\/ number of Rx Frame \/ CheckForHang_period  to determine link status$/;"	m	struct:_link_detect_t
SCR	r8180_hw.h	293;"	d
SCR_KM	r8180_hw.h	692;"	d
SCR_KM0	r8180_hw.h	694;"	d
SCR_KM1	r8180_hw.h	693;"	d
SCR_RXSECON	r8180_hw.h	696;"	d
SCR_RxSecEnable	r8187.h	121;"	d
SCR_TXSECON	r8180_hw.h	695;"	d
SCR_TxSecEnable	r8187.h	120;"	d
SCR_UseDK	r8187.h	119;"	d
SECR	r8187.h	103;"	d
SECURITY	r8180_hw.h	193;"	d
SECURITY_ENCRYP_104	r8180_hw.h	196;"	d
SECURITY_ENCRYP_MASK	r8180_hw.h	198;"	d
SECURITY_ENCRYP_SHIFT	r8180_hw.h	197;"	d
SECURITY_WEP_RX_ENABLE_SHIFT	r8180_hw.h	195;"	d
SECURITY_WEP_TX_ENABLE_SHIFT	r8180_hw.h	194;"	d
SEC_ACTIVE_KEY	ieee80211.h	720;"	d
SEC_AUTH_MODE	ieee80211.h	721;"	d
SEC_ENABLED	ieee80211.h	724;"	d
SEC_KEY_1	ieee80211.h	716;"	d
SEC_KEY_2	ieee80211.h	717;"	d
SEC_KEY_3	ieee80211.h	718;"	d
SEC_KEY_4	ieee80211.h	719;"	d
SEC_LEVEL	ieee80211.h	723;"	d
SEC_LEVEL_0	ieee80211.h	726;"	d
SEC_LEVEL_1	ieee80211.h	727;"	d
SEC_LEVEL_2	ieee80211.h	728;"	d
SEC_LEVEL_2_CKIP	ieee80211.h	729;"	d
SEC_LEVEL_3	ieee80211.h	730;"	d
SEC_UNICAST_GROUP	ieee80211.h	722;"	d
SIFS	r8180_hw.h	351;"	d
SIFS_Timer	r8187.h	/^	u16 SIFS_Timer;$/;"	m	struct:ChnlAccessSetting
SLOT	r8180_hw.h	355;"	d
SNAP_SIZE	ieee80211.h	496;"	d
SW_CONTROL_GPIO	r8180_hw.h	339;"	d
SW_LED_MODE0	r8187_led.h	/^	SW_LED_MODE0, \/\/ SW control 1 LED via GPIO0. It is default option.$/;"	e	enum:_LED_STRATEGY_8187
SW_LED_MODE1	r8187_led.h	/^	SW_LED_MODE1, \/\/ 2 LEDs, through LED0 and LED1. For ALPHA.$/;"	e	enum:_LED_STRATEGY_8187
SW_LED_MODE2	r8187_led.h	/^	SW_LED_MODE2, \/\/ SW control 1 LED via GPIO0, customized for AzWave 8187 minicard.$/;"	e	enum:_LED_STRATEGY_8187
SW_LED_MODE3	r8187_led.h	/^	SW_LED_MODE3, \/\/ SW control 1 LED via GPIO0, customized for Sercomm Printer Server case.$/;"	e	enum:_LED_STRATEGY_8187
SW_LED_MODE4	r8187_led.h	/^	SW_LED_MODE4, \/\/added by lizhaoming for bluetooth 2008.6.3$/;"	e	enum:_LED_STRATEGY_8187
SW_LED_MODE5	r8187_led.h	/^	SW_LED_MODE5, \/\/added by lizhaoming for bluetooth 2008.6.3			$/;"	e	enum:_LED_STRATEGY_8187
SW_THREE_WIRE	r8187.h	314;"	d
SW_THREE_WIRE_BY_8051	r8187.h	316;"	d
SetRFPowerState	r8187_core.c	/^SetRFPowerState($/;"	f
SetRFPowerStateInProgress	r8187.h	/^	bool SetRFPowerStateInProgress;$/;"	m	struct:r8180_priv
SetTxPowerLevel8187	r8180_dm.c	/^void SetTxPowerLevel8187(struct net_device *dev, short chan)$/;"	f
SetZebraRFPowerState8187B	r8187_core.c	/^SetZebraRFPowerState8187B($/;"	f
SetupRFEInitialTiming	r8180_rtl8225z2.c	/^SetupRFEInitialTiming(struct net_device*  dev)$/;"	f
ShortRetryLimit	r8187.h	/^	u16	ShortRetryLimit;$/;"	m	struct:r8180_priv
SignalQuality	r8187.h	/^        long                SignalQuality;$/;"	m	struct:r8180_priv
SignalStrength	ieee80211.h	/^	u8 SignalStrength;$/;"	m	struct:ieee80211_network
SignalStrength	r8187.h	/^        long            SignalStrength;$/;"	m	struct:r8180_priv
SlotIndex	r8187.h	/^	u16				SlotIndex;$/;"	m	struct:_link_detect_t
SlotNum	r8187.h	/^	u16				SlotNum;	\/\/ number of CheckForHang period to determine link status, default is 2$/;"	m	struct:_link_detect_t
SlotTimeTimer	r8187.h	/^	u16 SlotTimeTimer;$/;"	m	struct:ChnlAccessSetting
StageCCKTh	r8187.h	/^	u8   StageCCKTh;$/;"	m	struct:r8180_priv
Stats	r8187.h	/^typedef struct Stats$/;"	s
Stats	r8187.h	/^} Stats;$/;"	t	typeref:struct:Stats
SwLed0	r8187.h	/^        LED_8187        SwLed0;$/;"	m	struct:r8180_priv
SwLed0BlinkTimerCallback	r8187_led.c	/^SwLed0BlinkTimerCallback($/;"	f
SwLed0WorkItem	r8187.h	/^        struct work_struct              SwLed0WorkItem;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::work_struct
SwLed0WorkItemCallback	r8187_led.c	/^void SwLed0WorkItemCallback(struct work_struct *work)$/;"	f
SwLed1	r8187.h	/^        LED_8187        SwLed1;$/;"	m	struct:r8180_priv
SwLed1BlinkTimerCallback	r8187_led.c	/^SwLed1BlinkTimerCallback($/;"	f
SwLed1WorkItem	r8187.h	/^        struct work_struct              SwLed1WorkItem;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::work_struct
SwLed1WorkItemCallback	r8187_led.c	/^void SwLed1WorkItemCallback(struct work_struct *work)$/;"	f
SwLedBlink	r8187_led.c	/^SwLedBlink($/;"	f
SwLedCm2Blink	r8187_led.c	/^SwLedCm2Blink($/;"	f
SwLedCm4Blink	r8187_led.c	/^SwLedCm4Blink($/;"	f
SwLedControlMode0	r8187_led.c	/^SwLedControlMode0($/;"	f
SwLedControlMode1	r8187_led.c	/^SwLedControlMode1($/;"	f
SwLedControlMode2	r8187_led.c	/^SwLedControlMode2($/;"	f
SwLedControlMode3	r8187_led.c	/^SwLedControlMode3($/;"	f
SwLedControlMode4	r8187_led.c	/^SwLedControlMode4($/;"	f
SwLedControlMode5	r8187_led.c	/^SwLedControlMode5(	$/;"	f
SwLedOff	r8187_led.c	/^SwLedOff($/;"	f
SwLedOn	r8187_led.c	/^SwLedOn($/;"	f
TALLY_SEL	r8180_hw.h	81;"	d
TBDA	r8180_hw.h	270;"	d
TBDA_END	r8180_hw.h	271;"	d
TCR	r8180_hw.h	261;"	d
TCR_CRC	r8180_hw.h	590;"	d
TCR_DISCW	r8180_hw.h	585;"	d
TCR_DISReqQsize	r8180_hw.h	576;"	d
TCR_DurProcMode	r8180_hw.h	575;"	d
TCR_END	r8180_hw.h	262;"	d
TCR_HWVERID_MASK	r8180_hw.h	577;"	d
TCR_HWVERID_SHIFT	r8180_hw.h	578;"	d
TCR_ICV	r8180_hw.h	586;"	d
TCR_LBK	r8180_hw.h	587;"	d
TCR_LBK0	r8180_hw.h	589;"	d
TCR_LBK1	r8180_hw.h	588;"	d
TCR_LRL_MASK	r8180_hw.h	592;"	d
TCR_MXDMA_1024	r8180_hw.h	582;"	d
TCR_MXDMA_2048	r8180_hw.h	583;"	d
TCR_MXDMA_MASK	r8180_hw.h	581;"	d
TCR_MXDMA_SHIFT	r8180_hw.h	584;"	d
TCR_PLCP_LEN	r8180_hw.h	580;"	d
TCR_PROBE_NOTIMESTAMP_SHIFT	r8180_hw.h	593;"	d
TCR_SRL_MASK	r8180_hw.h	591;"	d
TCR_SWPLCPLEN	r8180_hw.h	579;"	d
TESTR	r8180_hw.h	287;"	d
TFPC	r8180_hw.h	759;"	d
TFPC_AC	r8180_hw.h	290;"	d
THPDA	r8180_hw.h	240;"	d
THPDA_END	r8180_hw.h	241;"	d
TID_AC_MAP	r8180_hw.h	435;"	d
TLPDA	r8180_hw.h	236;"	d
TLPDA_END	r8180_hw.h	237;"	d
TNPDA	r8180_hw.h	238;"	d
TNPDA_END	r8180_hw.h	239;"	d
TOTAL_CAM_ENTRY	r8187.h	139;"	d
TPPoll	r8180_hw.h	451;"	d
TPPoll_BQ	r8180_hw.h	708;"	d
TPPoll_HPQ	r8180_hw.h	709;"	d
TPPoll_LPQ	r8180_hw.h	711;"	d
TPPoll_NPQ	r8180_hw.h	710;"	d
TPPoll_SBQ	r8180_hw.h	712;"	d
TPPoll_SHPQ	r8180_hw.h	713;"	d
TPPoll_SLPQ	r8180_hw.h	715;"	d
TPPoll_SNPQ	r8180_hw.h	714;"	d
TRUE	r8187.h	61;"	d
TR_HW_CONTROLLED	r8187.h	/^	TR_HW_CONTROLLED = 0,$/;"	e	enum:_TR_SWITCH_STATE
TR_SWITCH_STATE	r8187.h	/^}TR_SWITCH_STATE, *PTR_SWITCH_STATE;$/;"	t	typeref:enum:_TR_SWITCH_STATE
TR_SW_MASK_8187	r8180_hw.h	514;"	d
TR_SW_MASK_RX_8187	r8180_hw.h	513;"	d
TR_SW_MASK_TX_8187	r8180_hw.h	512;"	d
TR_SW_TX	r8187.h	/^	TR_SW_TX = 1,$/;"	e	enum:_TR_SWITCH_STATE
TSFTR	r8180_hw.h	233;"	d
TSFTR_END	r8180_hw.h	234;"	d
TXAGC_CTL_PER_PACKET_ANT_SEL	r8180_hw.h	343;"	d
TXFIFOCOUNT	r8180_hw.h	79;"	d
TXISR_SELECT	r8187_core.c	87;"	d	file:
TXOPLimit	r8187.h	/^		u16		TXOPLimit;$/;"	m	struct:_AC_PARAM::__anon18
TXOPSEL	r8180_hw.h	504;"	d
TX_AGC_CTL	r8180_hw.h	345;"	d
TX_AGC_CTL_FEEDBACK_ANT	r8180_hw.h	349;"	d
TX_AGC_CTL_PERPACKET_ANTSEL_SHIFT	r8180_hw.h	348;"	d
TX_AGC_CTL_PERPACKET_GAIN_SHIFT	r8180_hw.h	347;"	d
TX_AGC_CTL_PER_PACKET_TXAGC	r8180_hw.h	346;"	d
TX_BEACON_RING_ADDR	r8180_hw.h	201;"	d
TX_CONF	r8180_hw.h	147;"	d
TX_CONF_HEADER_AUTOICREMENT_SHIFT	r8180_hw.h	148;"	d
TX_DMA_POLLING	r8180_hw.h	160;"	d
TX_DMA_POLLING_BEACON_SHIFT	r8180_hw.h	161;"	d
TX_DMA_POLLING_HIPRIORITY_SHIFT	r8180_hw.h	162;"	d
TX_DMA_POLLING_LOWPRIORITY_SHIFT	r8180_hw.h	164;"	d
TX_DMA_POLLING_NORMPRIORITY_SHIFT	r8180_hw.h	163;"	d
TX_DMA_STOP_BEACON_SHIFT	r8180_hw.h	165;"	d
TX_DMA_STOP_HIPRIORITY_SHIFT	r8180_hw.h	166;"	d
TX_DMA_STOP_LOWPRIORITY_SHIFT	r8180_hw.h	168;"	d
TX_DMA_STOP_NORMPRIORITY_SHIFT	r8180_hw.h	167;"	d
TX_HIGHPRIORITY_RING_ADDR	r8180_hw.h	170;"	d
TX_LOOPBACK_BASEBAND	r8180_hw.h	151;"	d
TX_LOOPBACK_CONTINUE	r8180_hw.h	153;"	d
TX_LOOPBACK_MAC	r8180_hw.h	150;"	d
TX_LOOPBACK_MASK	r8180_hw.h	154;"	d
TX_LOOPBACK_NONE	r8180_hw.h	152;"	d
TX_LOOPBACK_SHIFT	r8180_hw.h	149;"	d
TX_LOWPRIORITY_RING_ADDR	r8180_hw.h	171;"	d
TX_LRLRETRY_SHIFT	r8180_hw.h	155;"	d
TX_NOCRC_SHIFT	r8180_hw.h	159;"	d
TX_NOICV_SHIFT	r8180_hw.h	158;"	d
TX_NORMPRIORITY_RING_ADDR	r8180_hw.h	169;"	d
TX_SRLRETRY_SHIFT	r8180_hw.h	157;"	d
TimerInt	r8180_hw.h	267;"	d
TimerInt_END	r8180_hw.h	268;"	d
TrSwitchState	r8187.h	/^	TR_SWITCH_STATE TrSwitchState;$/;"	m	struct:r8180_priv
TranslateToDbm8187	r8187_core.c	/^TranslateToDbm8187($/;"	f
TransmitConfig	r8187.h	/^	u32	TransmitConfig;$/;"	m	struct:r8180_priv
TryDownCountLowData	r8187.h	/^        u8                                      TryDownCountLowData;$/;"	m	struct:r8180_priv
TryupingCount	r8187.h	/^        u16                                     TryupingCount;$/;"	m	struct:r8180_priv
TryupingCountNoData	r8187.h	/^        u8                                      TryupingCountNoData;$/;"	m	struct:r8180_priv
Turbo_Enable	ieee80211.h	/^	u8 Turbo_Enable;\/\/enable turbo mode, added by thomas$/;"	m	struct:ieee80211_network
UART_PRIORITY	r8187.h	/^	UART_PRIORITY \/\/0x0F$/;"	e	enum:__anon14
UP2AC	ieee80211.h	958;"	d
USB	r8187.h	/^	enum card_type {PCI,MINIPCI,CARDBUS,USB\/*rtl8187*\/}card_type;$/;"	e	enum:r8180_priv::card_type
USB_VENDOR_ID_NETGEAR	r8187_core.c	84;"	d	file:
USB_VENDOR_ID_REALTEK	r8187_core.c	81;"	d	file:
USE_8051_3WIRE	r8180_rtl8225.c	18;"	d	file:
UndecoratedSmoothedSS	r8187.h	/^	int  UndecoratedSmoothedSS;$/;"	m	struct:r8180_priv
UpdateCCKThreshold	r8180_rtl8225z2.c	/^UpdateCCKThreshold($/;"	f
UpdateInitialGain	r8180_rtl8225z2.c	/^UpdateInitialGain($/;"	f
VERSION_8187	r8180_hw.h	/^}VERSION_8187,*PVERSION_8187;$/;"	t	typeref:enum:_VERSION_8187
VERSION_8187B_B	r8180_hw.h	/^	VERSION_8187B_B, \/\/ B-cut$/;"	e	enum:_VERSION_8187
VERSION_8187B_D	r8180_hw.h	/^	VERSION_8187B_D,  \/\/D-cut   \/\/added 2007-9-14$/;"	e	enum:_VERSION_8187
VERSION_8187B_E	r8180_hw.h	/^	VERSION_8187B_E,  \/\/E-cut   \/\/added 2007-9-14$/;"	e	enum:_VERSION_8187
VERSION_8187_B	r8180_hw.h	/^	VERSION_8187_B, \/\/ B-cut$/;"	e	enum:_VERSION_8187
VERSION_8187_D	r8180_hw.h	/^	VERSION_8187_D, \/\/ D-cut$/;"	e	enum:_VERSION_8187
VIQ_ACM_CTL	r8180_hw.h	506;"	d
VIQ_ACM_EN	r8180_hw.h	501;"	d
VI_PRIORITY	r8187.h	/^	VI_PRIORITY, \/\/0x05$/;"	e	enum:__anon14
VOQ_ACM_CTL	r8180_hw.h	505;"	d
VOQ_ACM_EN	r8180_hw.h	500;"	d
VO_PRIORITY	r8187.h	/^	VO_PRIORITY,$/;"	e	enum:__anon14
WARN	Makefile	/^WARN := -W$/;"	m
WCAMI	r8187.h	100;"	d
WEP_KEYS	ieee80211.h	732;"	d
WEP_KEY_LEN	ieee80211.h	733;"	d
WIRELESS_MODE	r8187.h	/^} WIRELESS_MODE;$/;"	t	typeref:enum:_WIRELESS_MODE
WIRELESS_MODE_A	r8187.h	/^	WIRELESS_MODE_A = 0x01,$/;"	e	enum:_WIRELESS_MODE
WIRELESS_MODE_AUTO	r8187.h	/^	WIRELESS_MODE_AUTO = 0x08,$/;"	e	enum:_WIRELESS_MODE
WIRELESS_MODE_B	r8187.h	/^	WIRELESS_MODE_B = 0x02,$/;"	e	enum:_WIRELESS_MODE
WIRELESS_MODE_G	r8187.h	/^	WIRELESS_MODE_G = 0x04,$/;"	e	enum:_WIRELESS_MODE
WIRELESS_MODE_UNKNOWN	r8187.h	/^	WIRELESS_MODE_UNKNOWN = 0x00,$/;"	e	enum:_WIRELESS_MODE
WIRELESS_SPY	ieee80211.h	469;"	d
WLAN_AUTH_CHALLENGE_LEN	ieee80211.h	508;"	d
WLAN_AUTH_OPEN	ieee80211.h	505;"	d
WLAN_AUTH_SHARED_KEY	ieee80211.h	506;"	d
WLAN_CAPABILITY_BSS	ieee80211.h	510;"	d
WLAN_CAPABILITY_CF_POLLABLE	ieee80211.h	512;"	d
WLAN_CAPABILITY_CF_POLL_REQUEST	ieee80211.h	513;"	d
WLAN_CAPABILITY_CHANNEL_AGILITY	ieee80211.h	517;"	d
WLAN_CAPABILITY_IBSS	ieee80211.h	511;"	d
WLAN_CAPABILITY_PBCC	ieee80211.h	516;"	d
WLAN_CAPABILITY_PRIVACY	ieee80211.h	514;"	d
WLAN_CAPABILITY_SHORT_PREAMBLE	ieee80211.h	515;"	d
WLAN_CAPABILITY_SHORT_SLOT	ieee80211.h	518;"	d
WLAN_EID_CF_PARAMS	ieee80211.h	554;"	d
WLAN_EID_CHALLENGE	ieee80211.h	557;"	d
WLAN_EID_DS_PARAMS	ieee80211.h	553;"	d
WLAN_EID_FH_PARAMS	ieee80211.h	552;"	d
WLAN_EID_GENERIC	ieee80211.h	559;"	d
WLAN_EID_IBSS_PARAMS	ieee80211.h	556;"	d
WLAN_EID_RSN	ieee80211.h	558;"	d
WLAN_EID_SSID	ieee80211.h	550;"	d
WLAN_EID_SUPP_RATES	ieee80211.h	551;"	d
WLAN_EID_TIM	ieee80211.h	555;"	d
WLAN_FC_GET_STYPE	ieee80211.h	499;"	d
WLAN_FC_GET_TYPE	ieee80211.h	498;"	d
WLAN_GET_SEQ_FRAG	ieee80211.h	501;"	d
WLAN_GET_SEQ_SEQ	ieee80211.h	502;"	d
WLAN_REASON_CLASS2_FRAME_FROM_NONAUTH_STA	ieee80211.h	543;"	d
WLAN_REASON_CLASS3_FRAME_FROM_NONASSOC_STA	ieee80211.h	544;"	d
WLAN_REASON_DEAUTH_LEAVING	ieee80211.h	540;"	d
WLAN_REASON_DISASSOC_AP_BUSY	ieee80211.h	542;"	d
WLAN_REASON_DISASSOC_DUE_TO_INACTIVITY	ieee80211.h	541;"	d
WLAN_REASON_DISASSOC_STA_HAS_LEFT	ieee80211.h	545;"	d
WLAN_REASON_PREV_AUTH_NOT_VALID	ieee80211.h	539;"	d
WLAN_REASON_STA_REQ_ASSOC_WITHOUT_AUTH	ieee80211.h	546;"	d
WLAN_REASON_UNSPECIFIED	ieee80211.h	538;"	d
WLAN_STATUS_AP_UNABLE_TO_HANDLE_NEW_STA	ieee80211.h	530;"	d
WLAN_STATUS_ASSOC_DENIED_NOAGILITY	ieee80211.h	535;"	d
WLAN_STATUS_ASSOC_DENIED_NOPBCC	ieee80211.h	534;"	d
WLAN_STATUS_ASSOC_DENIED_NOSHORT	ieee80211.h	533;"	d
WLAN_STATUS_ASSOC_DENIED_RATES	ieee80211.h	531;"	d
WLAN_STATUS_ASSOC_DENIED_UNSPEC	ieee80211.h	525;"	d
WLAN_STATUS_AUTH_TIMEOUT	ieee80211.h	529;"	d
WLAN_STATUS_CAPS_UNSUPPORTED	ieee80211.h	523;"	d
WLAN_STATUS_CHALLENGE_FAIL	ieee80211.h	528;"	d
WLAN_STATUS_NOT_SUPPORTED_AUTH_ALG	ieee80211.h	526;"	d
WLAN_STATUS_REASSOC_NO_ASSOC	ieee80211.h	524;"	d
WLAN_STATUS_SUCCESS	ieee80211.h	521;"	d
WLAN_STATUS_UNKNOWN_AUTH_TRANSACTION	ieee80211.h	527;"	d
WLAN_STATUS_UNSPECIFIED_FAILURE	ieee80211.h	522;"	d
WME_ACI_MASK	ieee80211.h	952;"	d
WME_AC_BE	ieee80211.h	948;"	d
WME_AC_BK	ieee80211.h	949;"	d
WME_AC_PRAM_LEN	ieee80211.h	954;"	d
WME_AC_VI	ieee80211.h	950;"	d
WME_AC_VO	ieee80211.h	951;"	d
WME_AIFSN_MASK	ieee80211.h	953;"	d
WMM_Hang_8187	ieee80211.h	945;"	d
WMM_all_frame	ieee80211.h	/^enum {WMM_all_frame, WMM_two_frame, WMM_four_frame, WMM_six_frame};$/;"	e	enum:__anon7
WMM_four_frame	ieee80211.h	/^enum {WMM_all_frame, WMM_two_frame, WMM_four_frame, WMM_six_frame};$/;"	e	enum:__anon7
WMM_six_frame	ieee80211.h	/^enum {WMM_all_frame, WMM_two_frame, WMM_four_frame, WMM_six_frame};$/;"	e	enum:__anon7
WMM_two_frame	ieee80211.h	/^enum {WMM_all_frame, WMM_two_frame, WMM_four_frame, WMM_six_frame};$/;"	e	enum:__anon7
WPA_CONFIG	r8180_hw.h	344;"	d
Wakeup0	r8180_hw.h	376;"	d
Wakeup0_END	r8180_hw.h	377;"	d
Wakeup1	r8180_hw.h	379;"	d
Wakeup1_END	r8180_hw.h	380;"	d
Wakeup2HD	r8180_hw.h	384;"	d
Wakeup2HD_END	r8180_hw.h	385;"	d
Wakeup2LD	r8180_hw.h	382;"	d
Wakeup2LD_END	r8180_hw.h	383;"	d
Wakeup3HD	r8180_hw.h	389;"	d
Wakeup3HD_END	r8180_hw.h	390;"	d
Wakeup3LD	r8180_hw.h	387;"	d
Wakeup3LD_END	r8180_hw.h	388;"	d
Wakeup4HD	r8180_hw.h	394;"	d
Wakeup4HD_END	r8180_hw.h	395;"	d
Wakeup4LD	r8180_hw.h	392;"	d
Wakeup4LD_END	r8180_hw.h	393;"	d
Z1_HIPWR_LOWER_TH	r8180_dm.c	28;"	d	file:
Z1_HIPWR_UPPER_TH	r8180_dm.c	27;"	d	file:
Z2HiPwrLowerTh	r8187.h	/^	u8   Z2HiPwrLowerTh;$/;"	m	struct:r8180_priv
Z2HiPwrUpperTh	r8187.h	/^	u8   Z2HiPwrUpperTh;$/;"	m	struct:r8180_priv
Z2RSSIHiPwrLowerTh	r8187.h	/^	u8   Z2RSSIHiPwrLowerTh;$/;"	m	struct:r8180_priv
Z2RSSIHiPwrUpperTh	r8187.h	/^	u8   Z2RSSIHiPwrUpperTh;$/;"	m	struct:r8180_priv
Z2_HIPWR_LOWER_TH	r8180_dm.c	30;"	d	file:
Z2_HIPWR_UPPER_TH	r8180_dm.c	29;"	d	file:
ZEBRA2_CCK_OFDM_GAIN_SETTING	r8180_rtl8225z2.c	/^u8 ZEBRA2_CCK_OFDM_GAIN_SETTING[]={$/;"	v
ZEBRA_AGC	r8180_rtl8225z2.c	/^static u8  ZEBRA_AGC[]={$/;"	v	file:
ZEBRA_Config_87BASIC	r8180_rtl8225z2.c	/^void ZEBRA_Config_87BASIC(struct net_device *dev)$/;"	f
ZEBRA_Config_87BASIC_HardCode	r8180_rtl8225z2.c	/^void ZEBRA_Config_87BASIC_HardCode(struct net_device* dev)$/;"	f
ZEBRA_RF_RX_GAIN_TABLE	r8180_rtl8225z2.c	/^static u32 ZEBRA_RF_RX_GAIN_TABLE[]={	$/;"	v	file:
_ACI_AIFSN	r8187.h	/^typedef	union _ACI_AIFSN{$/;"	u
_AC_PARAM	r8187.h	/^typedef	union _AC_PARAM{$/;"	u
_CHANNEL_LIST	r8187.h	/^typedef struct _CHANNEL_LIST{$/;"	s
_ECW	r8187.h	/^typedef	union _ECW{$/;"	u
_LED_8187	r8187_led.h	/^typedef struct _LED_8187{$/;"	s
_LED_CTL_MODE	ieee80211.h	/^typedef enum _LED_CTL_MODE {$/;"	g
_LED_PIN_8187	r8187_led.h	/^typedef enum _LED_PIN_8187{$/;"	g
_LED_STATE_8187	r8187_led.h	/^typedef	enum _LED_STATE_8187{$/;"	g
_LED_STRATEGY_8187	r8187_led.h	/^typedef	enum _LED_STRATEGY_8187{$/;"	g
_MESH_CLASS_HDR_H_	msh_class.h	9;"	d
_RF_TYPE_8187	r8180_hw.h	/^typedef	enum _RF_TYPE_8187{$/;"	g
_RT_CID_TYPE	r8187_led.h	/^typedef enum _RT_CID_TYPE {$/;"	g
_RT_PS_MODE	r8187.h	/^typedef	enum _RT_PS_MODE	$/;"	g
_RT_RF_POWER_STATE	r8187.h	/^typedef	enum _RT_RF_POWER_STATE$/;"	g
_TR_SWITCH_STATE	r8187.h	/^typedef enum _TR_SWITCH_STATE{$/;"	g
_VERSION_8187	r8180_hw.h	/^typedef enum _VERSION_8187{$/;"	g
_WIRELESS_MODE	r8187.h	/^typedef enum _WIRELESS_MODE {$/;"	g
__adddf3	r8187_core.c	/^double __adddf3(double a, double b) { return a+b; }$/;"	f
__addsf3	r8187_core.c	/^double __addsf3(float a, float b) { return a+b; }$/;"	f
__extendsfdf2	r8187_core.c	/^double __extendsfdf2(float a) {return a;}$/;"	f
__fixunsdfsi	r8187_core.c	/^unsigned int __fixunsdfsi (double d) { return d; }$/;"	f
__floatsidf	r8187_core.c	/^double __floatsidf (int i) { return i; }$/;"	f
__subdf3	r8187_core.c	/^double __subdf3(double a, double b) { return a-b; }$/;"	f
_link_detect_t	r8187.h	/^typedef struct _link_detect_t$/;"	s
_rtl8180_up	r8187_core.c	/^int _rtl8180_up(struct net_device *dev)$/;"	f
aSifsTime	ieee80211.h	69;"	d
abg_true	ieee80211.h	/^	int abg_true;   \/* ABG flag              *\/$/;"	m	struct:ieee80211_device
ac_aci_acm_aifsn	ieee80211.h	/^	u8 ac_aci_acm_aifsn;$/;"	m	struct:ieee80211_wmm_ac_param
ac_dir_tid	ieee80211.h	/^	u8 ac_dir_tid;$/;"	m	struct:ieee80211_wmm_ts_info
ac_ecwmin_ecwmax	ieee80211.h	/^	u8 ac_ecwmin_ecwmax;$/;"	m	struct:ieee80211_wmm_ac_param
ac_txop_limit	ieee80211.h	/^	u16 ac_txop_limit;$/;"	m	struct:ieee80211_wmm_ac_param
ac_up_psb	ieee80211.h	/^	u8 ac_up_psb;$/;"	m	struct:ieee80211_wmm_ts_info
active_key	ieee80211.h	/^	u16 active_key:2,$/;"	m	struct:ieee80211_security
active_scan	ieee80211.h	/^	short active_scan;$/;"	m	struct:ieee80211_device
actscanning	ieee80211.h	/^	bool actscanning;$/;"	m	struct:ieee80211_device
addr	r8187.h	/^                unsigned char addr;$/;"	m	struct:rtl_reg_debug::__anon13
addr1	ieee80211.h	/^	u8 addr1[6];$/;"	m	struct:ieee80211_header_data
addr1	ieee80211.h	/^	u8 addr1[ETH_ALEN];$/;"	m	struct:ieee80211_hdr
addr1	ieee80211.h	/^	u8 addr1[ETH_ALEN];$/;"	m	struct:ieee80211_hdr_3addr
addr1	ieee80211.h	/^	u8 addr1[ETH_ALEN];$/;"	m	struct:ieee80211_hdr_3addr_QOS
addr1	ieee80211.h	/^	u8 addr1[ETH_ALEN];$/;"	m	struct:ieee80211_hdr_QOS
addr2	ieee80211.h	/^	u8 addr2[6];$/;"	m	struct:ieee80211_header_data
addr2	ieee80211.h	/^	u8 addr2[ETH_ALEN];$/;"	m	struct:ieee80211_hdr
addr2	ieee80211.h	/^	u8 addr2[ETH_ALEN];$/;"	m	struct:ieee80211_hdr_3addr
addr2	ieee80211.h	/^	u8 addr2[ETH_ALEN];$/;"	m	struct:ieee80211_hdr_3addr_QOS
addr2	ieee80211.h	/^	u8 addr2[ETH_ALEN];$/;"	m	struct:ieee80211_hdr_QOS
addr3	ieee80211.h	/^	u8 addr3[6];$/;"	m	struct:ieee80211_header_data
addr3	ieee80211.h	/^	u8 addr3[ETH_ALEN];$/;"	m	struct:ieee80211_hdr
addr3	ieee80211.h	/^	u8 addr3[ETH_ALEN];$/;"	m	struct:ieee80211_hdr_3addr
addr3	ieee80211.h	/^	u8 addr3[ETH_ALEN];$/;"	m	struct:ieee80211_hdr_3addr_QOS
addr3	ieee80211.h	/^	u8 addr3[ETH_ALEN];$/;"	m	struct:ieee80211_hdr_QOS
addr4	ieee80211.h	/^	u8 addr4[ETH_ALEN];$/;"	m	struct:ieee80211_hdr
addr4	ieee80211.h	/^	u8 addr4[ETH_ALEN];$/;"	m	struct:ieee80211_hdr_QOS
agc	r8187_core.c	/^unsigned char	agc;$/;"	m	struct:rx_desc_rtl8187b	file:
agc	r8187_core.c	/^unsigned char   agc;$/;"	m	struct:rx_desc_rtl8187	file:
agc	r8187_core.c	/^unsigned short	agc:8;$/;"	m	struct:tx_desc	file:
aid	ieee80211.h	/^	u16 aid;$/;"	m	struct:ieee80211_assoc_response_frame
alg	ieee80211.h	/^			u8 alg[IEEE_CRYPT_ALG_NAME_LEN];$/;"	m	struct:ieee_param::__anon2::__anon6
alg	r8187_core.c	/^                        u8 alg[16];$/;"	m	struct:ipw_param::__anon8::__anon12	file:
algorithm	ieee80211.h	/^	u16 algorithm;$/;"	m	struct:ieee80211_authentication
alloc_ieee80211	ieee80211.h	128;"	d
alloc_tx_beacon_desc_ring	r8187_core.c	/^int alloc_tx_beacon_desc_ring(struct net_device *dev, int count)$/;"	f
antenna	r8187_core.c	/^unsigned char	antenna:1;$/;"	m	struct:rx_desc_rtl8187b	file:
antenna	r8187_core.c	/^unsigned char   antenna:1;$/;"	m	struct:rx_desc_rtl8187	file:
antenna	r8187_core.c	/^unsigned short	antenna:1;$/;"	m	struct:tx_desc	file:
antenna_flag	r8187.h	/^        u8                      antenna_flag;$/;"	m	struct:r8180_priv
ap_mac_addr	ieee80211.h	/^	u8 ap_mac_addr[6];$/;"	m	struct:ieee80211_device
assoc_id	ieee80211.h	/^	u16 assoc_id;$/;"	m	struct:ieee80211_device
associate_complete_wq	ieee80211.h	/^	struct tq_struct associate_complete_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::tq_struct
associate_complete_wq	ieee80211.h	/^	struct work_struct associate_complete_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::work_struct
associate_procedure_wq	ieee80211.h	/^	struct tq_struct associate_procedure_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::tq_struct
associate_procedure_wq	ieee80211.h	/^	struct work_struct associate_procedure_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::work_struct
associate_retry_wq	ieee80211.h	/^	struct tq_struct associate_retry_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::tq_struct
associate_retry_wq	ieee80211.h	/^        struct delayed_work associate_retry_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::delayed_work
associate_retry_wq	ieee80211.h	/^        struct work_struct associate_retry_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::work_struct
associate_seq	ieee80211.h	/^	u16 associate_seq;$/;"	m	struct:ieee80211_device
associate_timer	ieee80211.h	/^	struct timer_list associate_timer;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::timer_list
atim_window	ieee80211.h	/^	u16 atim_window;$/;"	m	struct:ieee80211_network
auth_algo	ieee80211.h	/^            auth_algo:4,$/;"	m	struct:ieee80211_security
auth_mode	ieee80211.h	/^	    auth_mode:2,$/;"	m	struct:ieee80211_security
bBusyTraffic	r8187.h	/^	bool				bBusyTraffic;    \/\/when it is set to 1, UI cann't scan at will.$/;"	m	struct:_link_detect_t
bCCKThMechanism	r8187.h	/^	bool bCCKThMechanism;$/;"	m	struct:r8180_priv
bCurCCKPkt	r8187.h	/^	bool bCurCCKPkt;$/;"	m	struct:r8180_priv
bDigMechanism	r8187.h	/^	bool bDigMechanism;$/;"	m	struct:r8180_priv
bEnableLedCtrl	r8187.h	/^        u8                      bEnableLedCtrl;$/;"	m	struct:r8180_priv
bHwRadioOff	ieee80211.h	/^	bool bHwRadioOff;\/\/by lizhaoming$/;"	m	struct:ieee80211_device
bInHctTest	r8187.h	/^	bool bInHctTest;$/;"	m	struct:r8180_priv
bInactivePs	ieee80211.h	/^	bool bInactivePs;$/;"	m	struct:ieee80211_device
bInactivePs	r8187.h	/^	bool bInactivePs;$/;"	m	struct:r8180_priv
bLedBlinkInProgress	r8187_led.h	/^	u8				bLedBlinkInProgress; \/\/ TRUE if it is blinking, FALSE o.w..$/;"	m	struct:_LED_8187
bLedOn	r8187_led.h	/^	u8				bLedOn; \/\/ TRUE if LED is ON, FALSE if LED is OFF.$/;"	m	struct:_LED_8187
bLeisurePs	r8187.h	/^	bool bLeisurePs;$/;"	m	struct:r8180_priv
bRegHighPowerMechanism	r8187.h	/^	bool bRegHighPowerMechanism;$/;"	m	struct:r8180_priv
bSwRfProcessing	r8187.h	/^	bool bSwRfProcessing;$/;"	m	struct:r8180_priv
bToUpdateTxPwr	r8187.h	/^	bool bToUpdateTxPwr;$/;"	m	struct:r8180_priv
bTryuping	r8187.h	/^        unsigned short          bTryuping;$/;"	m	struct:r8180_priv
bar	r8187_core.c	/^unsigned int	bar:1;$/;"	m	struct:rx_desc_rtl8187b	file:
bar	r8187_core.c	/^unsigned int    bar:1;$/;"	m	struct:rx_desc_rtl8187	file:
basic_rate	ieee80211.h	/^	int basic_rate;$/;"	m	struct:ieee80211_device
bckey	r8187_core.c	/^unsigned char	bckey:6;$/;"	m	struct:tx_desc	file:
bcrx_sta_key	ieee80211.h	/^	int bcrx_sta_key; \/* use individual keys to override default keys even$/;"	m	struct:ieee80211_device
beacon_interval	ieee80211.h	/^	u16 beacon_interval;$/;"	m	struct:ieee80211_network
beacon_interval	ieee80211.h	/^	u16 beacon_interval;$/;"	m	struct:ieee80211_probe_response
beacon_lock	ieee80211.h	/^	spinlock_t beacon_lock;$/;"	m	struct:ieee80211_device
beacon_timer	ieee80211.h	/^	struct timer_list beacon_timer;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::timer_list
beacon_txing	ieee80211.h	/^	short beacon_txing;$/;"	m	struct:ieee80211_device
beaconflag_lock	ieee80211.h	/^        spinlock_t beaconflag_lock;$/;"	m	struct:ieee80211_device
bool	ieee80211.h	/^typedef enum{false = 0, true} bool;$/;"	t	typeref:enum:__anon1
broadcast_key_type	ieee80211.h	/^	u16 broadcast_key_type;$/;"	m	struct:ieee80211_device
bssid	ieee80211.h	/^	u8 bssid[ETH_ALEN];$/;"	m	struct:ieee80211_network
buf	r8187.h	/^	u32 *buf;$/;"	m	struct:buffer
buf	r8187.h	/^        unsigned char buf[0xff];$/;"	m	struct:rtl_reg_debug
bufaddr	r8187_core.c	/^unsigned int	bufaddr;$/;"	m	struct:tx_desc	file:
buffer	r8187.h	/^typedef struct buffer$/;"	s
buffer	r8187.h	/^} buffer;$/;"	t	typeref:struct:buffer
capability	ieee80211.h	/^	u16 capability;$/;"	m	struct:ieee80211_assoc_request_frame
capability	ieee80211.h	/^	u16 capability;$/;"	m	struct:ieee80211_assoc_response_frame
capability	ieee80211.h	/^	u16 capability;$/;"	m	struct:ieee80211_network
capability	ieee80211.h	/^	u16 capability;$/;"	m	struct:ieee80211_probe_response
card_8187	r8187.h	/^	short card_8187; \/* O: rtl8180, 1:rtl8185 V B\/C, 2:rtl8185 V D *\/$/;"	m	struct:r8180_priv
card_8187_Bversion	r8187.h	/^	short card_8187_Bversion; \/* if TCR reports card V B\/C this discriminates *\/$/;"	m	struct:r8180_priv
card_type	r8187.h	/^	enum card_type {PCI,MINIPCI,CARDBUS,USB\/*rtl8187*\/}card_type;$/;"	g	struct:r8180_priv
card_type	r8187.h	/^	enum card_type {PCI,MINIPCI,CARDBUS,USB\/*rtl8187*\/}card_type;$/;"	m	struct:r8180_priv	typeref:enum:r8180_priv::card_type
cck_txpwr_base	r8187.h	/^	u8 cck_txpwr_base;$/;"	m	struct:r8180_priv
cfo_bias	r8187_core.c	/^unsigned int	cfo_bias:6;$/;"	m	struct:rx_desc_rtl8187b	file:
challow	r8187.h	/^	u8 challow[15]; \/\/channels from 1 to 14, 0 not used$/;"	m	struct:r8180_priv
chan	r8187.h	/^	short chan;$/;"	m	struct:r8180_priv
channel	ieee80211.h	/^	u8 channel;$/;"	m	struct:ieee80211_network
channel_map	ieee80211.h	/^	int channel_map[MAX_CHANNEL_NUMBER+1];$/;"	m	struct:ieee80211_device
channels	r8187_core.c	/^static int channels = 0x3fff;$/;"	v	file:
charData	r8187.h	/^	u8	charData;$/;"	m	union:_ACI_AIFSN
charData	r8187.h	/^	u8	charData;$/;"	m	union:_ECW
charData	r8187.h	/^	u8	charData[4];$/;"	m	union:_AC_PARAM
check_nic_enought_desc	r8187_core.c	/^short check_nic_enought_desc(struct net_device *dev, priority_t priority)$/;"	f
chtxpwr	r8187.h	/^	u8 chtxpwr[15]; \/\/channels from 1 to 14, 0 not used$/;"	m	struct:r8180_priv
chtxpwr_ofdm	r8187.h	/^	u8 chtxpwr_ofdm[15]; \/\/channels from 1 to 14, 0 not used$/;"	m	struct:r8180_priv
cmd	ieee80211.h	/^	u32 cmd;$/;"	m	struct:ieee_param
cmd	r8187.h	/^        unsigned int  cmd;$/;"	m	struct:rtl_reg_debug
cmd	r8187_core.c	/^        u32 cmd;$/;"	m	struct:ipw_param	file:
command	ieee80211.h	/^			int command;$/;"	m	struct:ieee_param::__anon2::__anon5
command	r8187_core.c	/^                        u32 command;$/;"	m	struct:ipw_param::__anon8::__anon11	file:
config	ieee80211.h	/^	u32 config;$/;"	m	struct:ieee80211_device
control	ieee80211.h	/^	u8 control;$/;"	m	struct:ieee80211_rx_stats
crc32	r8187_core.c	/^unsigned int	crc32:1;$/;"	m	struct:rx_desc_rtl8187b	file:
crc32	r8187_core.c	/^unsigned int    crc32:1;$/;"	m	struct:rx_desc_rtl8187	file:
crcmon	r8187.h	/^	short crcmon; \/\/if 1 allow bad crc frame reception in monitor mode$/;"	m	struct:r8180_priv
crypt	ieee80211.h	/^		} crypt;$/;"	m	union:ieee_param::__anon2	typeref:struct:ieee_param::__anon2::__anon6
crypt	ieee80211.h	/^	struct ieee80211_crypt_data *crypt[WEP_KEYS];$/;"	m	struct:ieee80211_crypt_data_list	typeref:struct:ieee80211_crypt_data_list::ieee80211_crypt_data
crypt	ieee80211.h	/^	struct ieee80211_crypt_data *crypt[WEP_KEYS];$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::ieee80211_crypt_data
crypt	r8187_core.c	/^                } crypt;$/;"	m	union:ipw_param::__anon8	typeref:struct:ipw_param::__anon8::__anon12	file:
crypt_deinit_list	ieee80211.h	/^	struct list_head crypt_deinit_list;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::list_head
crypt_deinit_timer	ieee80211.h	/^	struct timer_list crypt_deinit_timer;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::timer_list
cryptlist	ieee80211.h	/^	struct ieee80211_crypt_data_list* cryptlist[MAX_MP];$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::ieee80211_crypt_data_list
crypto_alloc_tfm	ieee80211_crypt.h	87;"	d
crypto_free_tfm	ieee80211_crypt.h	88;"	d
ctrl	ieee80211.h	/^        u8    ctrl;   \/* always 0x03 *\/$/;"	m	struct:ieee80211_snap_hdr
ctsen	r8187_core.c	/^unsigned int    ctsen:1;$/;"	m	struct:tx_desc	file:
current_network	ieee80211.h	/^	struct ieee80211_network current_network;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::ieee80211_network
data	ieee80211.h	/^			u8 data[0];$/;"	m	struct:ieee_param::__anon2::__anon4
data	ieee80211.h	/^	u8 data[0];$/;"	m	struct:ieee80211_info_element
data	r8187_core.c	/^                        u8 data[0];$/;"	m	struct:ipw_param::__anon8::__anon10	file:
data_hard_resume	ieee80211.h	/^	void (*data_hard_resume)(struct net_device *dev);$/;"	m	struct:ieee80211_device
data_hard_stop	ieee80211.h	/^	void (*data_hard_stop)(struct net_device *dev);$/;"	m	struct:ieee80211_device
decrypt_mpdu	ieee80211_crypt.h	/^	int (*decrypt_mpdu)(struct sk_buff *skb, int hdr_len, void *priv);$/;"	m	struct:ieee80211_crypto_ops
decrypt_msdu	ieee80211_crypt.h	/^	int (*decrypt_msdu)(struct sk_buff *skb, int keyidx, int hdr_len,$/;"	m	struct:ieee80211_crypto_ops
decrypted	r8187_core.c	/^unsigned char 	decrypted:1;$/;"	m	struct:rx_desc_rtl8187b	file:
decrypted	r8187_core.c	/^unsigned char   decrypted:1;$/;"	m	struct:rx_desc_rtl8187	file:
deinit	ieee80211_crypt.h	/^	void (*deinit)(void *priv);$/;"	m	struct:ieee80211_crypto_ops
delay_bound	ieee80211.h	/^	u32 delay_bound;$/;"	m	struct:ieee80211_wmm_tspec_elem
delaybound	r8187_core.c	/^unsigned short	delaybound;$/;"	m	struct:tx_desc	file:
desc_87	r8187_core.c	/^struct	rx_desc_rtl8187	 desc_87;$/;"	m	union:rx_desc	typeref:struct:rx_desc::rx_desc_rtl8187	file:
desc_87b	r8187_core.c	/^struct	rx_desc_rtl8187b desc_87b;$/;"	m	union:rx_desc	typeref:struct:rx_desc::rx_desc_rtl8187b	file:
dev	ieee80211.h	/^	struct net_device *dev;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::net_device
dev	r8187.h	/^	struct net_device *dev;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::net_device
dev	r8187.h	/^	struct net_device *dev;$/;"	m	struct:ssid_thread	typeref:struct:ssid_thread::net_device
dir_dev	r8187.h	/^	struct proc_dir_entry *dir_dev;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::proc_dir_entry
dmafail	r8187_core.c	/^unsigned int	dmafail:1;$/;"	m	struct:rx_desc_rtl8187b	file:
dmafail	r8187_core.c	/^unsigned int    dmafail:1;$/;"	m	struct:rx_desc_rtl8187	file:
dmaok	r8187_core.c	/^unsigned int	dmaok:1;$/;"	m	struct:tx_desc	file:
dot11PowerSaveMode	r8187.h	/^	RT_PS_MODE dot11PowerSaveMode;$/;"	m	struct:r8180_priv
drop_unencrypted	ieee80211.h	/^	int drop_unencrypted;$/;"	m	struct:ieee80211_device
dsap	ieee80211.h	/^        u8    dsap;   \/* always 0xAA *\/$/;"	m	struct:ieee80211_snap_hdr
dst_addr	ieee80211.h	/^	u8 dst_addr[ETH_ALEN];$/;"	m	struct:ieee80211_frag_entry
dtim_data	ieee80211.h	/^	u8 dtim_data;$/;"	m	struct:ieee80211_network
dtim_period	ieee80211.h	/^	u8 dtim_period;$/;"	m	struct:ieee80211_network
dummy	r8180_wx.c	/^static int dummy(struct net_device *dev, struct iw_request_info *a,$/;"	f	file:
dump_eprom	r8187_core.c	/^void dump_eprom(struct net_device *dev)$/;"	f
dur	r8187_core.c	/^unsigned short	dur;$/;"	m	struct:tx_desc	file:
duration_id	ieee80211.h	/^	u16 duration_id;$/;"	m	struct:ieee80211_hdr
duration_id	ieee80211.h	/^	u16 duration_id;$/;"	m	struct:ieee80211_hdr_3addr
duration_id	ieee80211.h	/^	u16 duration_id;$/;"	m	struct:ieee80211_hdr_3addr_QOS
duration_id	ieee80211.h	/^	u16 duration_id;$/;"	m	struct:ieee80211_hdr_QOS
duration_id	ieee80211.h	/^	u16 duration_id;$/;"	m	struct:ieee80211_header_data
eActive	r8187.h	/^	eActive,	\/\/ Active\/Continuous access.$/;"	e	enum:_RT_PS_MODE
eFastPs	r8187.h	/^	eFastPs		\/\/ Fast power save mode.$/;"	e	enum:_RT_PS_MODE
eInactivePowerState	r8187.h	/^	RT_RF_POWER_STATE	eInactivePowerState;$/;"	m	struct:r8180_priv
eMaxPs	r8187.h	/^	eMaxPs,		\/\/ Max power save mode.$/;"	e	enum:_RT_PS_MODE
eRFPowerState	r8187.h	/^	RT_RF_POWER_STATE eRFPowerState;$/;"	m	struct:r8180_priv
eRfOff	r8187.h	/^	eRfOff$/;"	e	enum:_RT_RF_POWER_STATE
eRfOn	r8187.h	/^	eRfOn,$/;"	e	enum:_RT_RF_POWER_STATE
eRfSleep	r8187.h	/^	eRfSleep,$/;"	e	enum:_RT_RF_POWER_STATE
eap_get_type	ieee80211.h	/^static inline const char *eap_get_type(int type)$/;"	f
eap_type	ieee80211.h	/^enum eap_type {$/;"	g
eap_types	ieee80211.h	/^static const char *eap_types[] = {$/;"	v
eapol	ieee80211.h	/^struct eapol {$/;"	s
enable_gpio0	r8187.h	/^	short enable_gpio0;$/;"	m	struct:r8180_priv
enabled	ieee80211.h	/^            enabled:1,$/;"	m	struct:ieee80211_security
enbckey	r8187_core.c	/^unsigned char	enbckey:1;$/;"	m	struct:tx_desc	file:
encrypt_mpdu	ieee80211_crypt.h	/^	int (*encrypt_mpdu)(struct sk_buff *skb, int hdr_len, void *priv);$/;"	m	struct:ieee80211_crypto_ops
encrypt_msdu	ieee80211_crypt.h	/^	int (*encrypt_msdu)(struct sk_buff *skb, int hdr_len, void *priv);$/;"	m	struct:ieee80211_crypto_ops
encrypted	ieee80211.h	/^	u8 encrypted;$/;"	m	struct:ieee80211_txb
enpmpd	r8187_core.c	/^unsigned char	enpmpd:1;$/;"	m	struct:tx_desc	file:
enter_sleep_state	ieee80211.h	/^	void (*enter_sleep_state) (struct net_device *dev, u32 th, u32 tl);$/;"	m	struct:ieee80211_device
eor	r8187_core.c	/^unsigned int	eor:1;$/;"	m	struct:rx_desc_rtl8187b	file:
eor	r8187_core.c	/^unsigned int    eor:1;$/;"	m	struct:rx_desc_rtl8187	file:
eprom_ck_cycle	r8180_93cx6.c	/^void eprom_ck_cycle(struct net_device *dev)$/;"	f
eprom_cs	r8180_93cx6.c	/^void eprom_cs(struct net_device *dev, short bit)$/;"	f
eprom_r	r8180_93cx6.c	/^short eprom_r(struct net_device *dev)$/;"	f
eprom_read	r8180_93cx6.c	/^u32 eprom_read(struct net_device *dev, u32 addr)$/;"	f
eprom_send_bits_string	r8180_93cx6.c	/^void eprom_send_bits_string(struct net_device *dev, short b[], int len)$/;"	f
eprom_w	r8180_93cx6.c	/^void eprom_w(struct net_device *dev,short bit)$/;"	f
epromtype	r8187.h	/^	short epromtype;$/;"	m	struct:r8180_priv
eqMacAddr	r8187_core.c	180;"	d	file:
err	ieee80211.h	/^			u32 err;$/;"	m	struct:ieee_param::__anon2::__anon6
err	r8187_core.c	/^                        u32 err;$/;"	m	struct:ipw_param::__anon8::__anon12	file:
escape_essid	ieee80211.h	/^static inline const char *escape_essid(const char *essid, u8 essid_len) {$/;"	f
ether_dhost	ieee80211.h	/^	u8 ether_dhost[ETHER_ADDR_LEN];$/;"	m	struct:ether_header
ether_header	ieee80211.h	/^struct	ether_header {$/;"	s
ether_shost	ieee80211.h	/^	u8 ether_shost[ETHER_ADDR_LEN];$/;"	m	struct:ether_header
ether_type	ieee80211.h	/^	u16 ether_type;$/;"	m	struct:ether_header
ethertype	ieee80211.h	/^	u16 ethertype;$/;"	m	struct:eapol
ext_entry	ieee80211.h	/^	void *ext_entry;$/;"	m	struct:ieee80211_network
ext_patch_create_proc	msh_class.h	/^	void (*ext_patch_create_proc) (struct r8180_priv *priv);$/;"	m	struct:mshclass
ext_patch_get_beacon_get_probersp	ieee80211.h	/^	struct sk_buff* (*ext_patch_get_beacon_get_probersp)(struct ieee80211_device *ieee, u8 *dest, struct ieee80211_network *net);$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::ext_patch_get_beacon_get_probersp
ext_patch_get_beacon_get_probersp	msh_class.h	/^	struct sk_buff* (*ext_patch_get_beacon_get_probersp)(struct ieee80211_device *ieee, u8 *dest, struct ieee80211_network *net);$/;"	m	struct:mshclass	typeref:struct:mshclass::ext_patch_get_beacon_get_probersp
ext_patch_ieee80211_acl_query	ieee80211.h	/^	u8 (*ext_patch_ieee80211_acl_query) (struct ieee80211_device *ieee, u8 *sa);$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_acl_query	msh_class.h	/^	u8 (*ext_patch_ieee80211_acl_query) (struct ieee80211_device *ieee, u8 *sa);$/;"	m	struct:mshclass
ext_patch_ieee80211_assoc_resp_by_net_1	ieee80211.h	/^	void (*ext_patch_ieee80211_assoc_resp_by_net_1) (struct ieee80211_assoc_response_frame *assoc);$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_assoc_resp_by_net_1	msh_class.h	/^	void (*ext_patch_ieee80211_assoc_resp_by_net_1) (struct ieee80211_assoc_response_frame *assoc);$/;"	m	struct:mshclass
ext_patch_ieee80211_assoc_resp_by_net_2	ieee80211.h	/^	u8* (*ext_patch_ieee80211_assoc_resp_by_net_2) (struct ieee80211_device *ieee, struct ieee80211_network *pstat, int pkt_type, struct sk_buff *skb);$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_assoc_resp_by_net_2	msh_class.h	/^	u8* (*ext_patch_ieee80211_assoc_resp_by_net_2) (struct ieee80211_device *ieee, struct ieee80211_network *pstat, int pkt_type, struct sk_buff *skb);$/;"	m	struct:mshclass
ext_patch_ieee80211_association_req_1	ieee80211.h	/^	void (*ext_patch_ieee80211_association_req_1) (struct ieee80211_assoc_request_frame *hdr);$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_association_req_1	msh_class.h	/^	void (*ext_patch_ieee80211_association_req_1) (struct ieee80211_assoc_request_frame *hdr);$/;"	m	struct:mshclass
ext_patch_ieee80211_association_req_2	ieee80211.h	/^	u8* (*ext_patch_ieee80211_association_req_2) (struct ieee80211_device *ieee, struct ieee80211_network *pstat, struct sk_buff *skb);$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_association_req_2	msh_class.h	/^	u8* (*ext_patch_ieee80211_association_req_2) (struct ieee80211_device *ieee, struct ieee80211_network *pstat, struct sk_buff *skb);$/;"	m	struct:mshclass
ext_patch_ieee80211_ext_stop_scan_wq_set_channel	ieee80211.h	/^	int (*ext_patch_ieee80211_ext_stop_scan_wq_set_channel) (struct ieee80211_device *ieee);$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_ext_stop_scan_wq_set_channel	msh_class.h	/^	int (*ext_patch_ieee80211_ext_stop_scan_wq_set_channel) (struct ieee80211_device *ieee);$/;"	m	struct:mshclass
ext_patch_ieee80211_probe_req_1	ieee80211.h	/^	short (*ext_patch_ieee80211_probe_req_1) (struct ieee80211_device *ieee); \/\/ return = 0: no more phases,  >0: another phase$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_probe_req_1	msh_class.h	/^	short (*ext_patch_ieee80211_probe_req_1) (struct ieee80211_device *ieee); \/\/ return = 0: no more phases,  >0: another phase$/;"	m	struct:mshclass
ext_patch_ieee80211_probe_req_2	ieee80211.h	/^	u8* (*ext_patch_ieee80211_probe_req_2) (struct ieee80211_device *ieee, struct sk_buff *skb, u8 *tag); \/\/ return tag$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_probe_req_2	msh_class.h	/^	u8* (*ext_patch_ieee80211_probe_req_2) (struct ieee80211_device *ieee, struct sk_buff *skb, u8 *tag); \/\/ return tag	$/;"	m	struct:mshclass
ext_patch_ieee80211_process_probe_response_1	ieee80211.h	/^	unsigned int(*ext_patch_ieee80211_process_probe_response_1)(struct ieee80211_device *ieee,	struct ieee80211_probe_response *beacon,	struct ieee80211_rx_stats *stats);$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_process_probe_response_1	msh_class.h	/^	unsigned int (*ext_patch_ieee80211_process_probe_response_1)  (	struct ieee80211_device *ieee,	struct ieee80211_probe_response *beacon,	struct ieee80211_rx_stats *stats);$/;"	m	struct:mshclass
ext_patch_ieee80211_rx_frame_get_hdrlen	ieee80211.h	/^	int (*ext_patch_ieee80211_rx_frame_get_hdrlen) (struct ieee80211_device *ieee, struct sk_buff *skb);$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_rx_frame_get_hdrlen	msh_class.h	/^	int (*ext_patch_ieee80211_rx_frame_get_hdrlen) (struct ieee80211_device *ieee, struct sk_buff *skb);$/;"	m	struct:mshclass
ext_patch_ieee80211_rx_frame_softmac_on_assoc_req	ieee80211.h	/^	int (*ext_patch_ieee80211_rx_frame_softmac_on_assoc_req) (struct ieee80211_device *ieee, struct sk_buff *skb);$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_rx_frame_softmac_on_assoc_req	msh_class.h	/^	int (*ext_patch_ieee80211_rx_frame_softmac_on_assoc_req) (struct ieee80211_device *ieee, struct sk_buff *skb);$/;"	m	struct:mshclass
ext_patch_ieee80211_rx_frame_softmac_on_assoc_rsp	ieee80211.h	/^	int (*ext_patch_ieee80211_rx_frame_softmac_on_assoc_rsp) (struct ieee80211_device *ieee, struct sk_buff *skb);$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_rx_frame_softmac_on_assoc_rsp	msh_class.h	/^	int (*ext_patch_ieee80211_rx_frame_softmac_on_assoc_rsp) (struct ieee80211_device *ieee, struct sk_buff *skb);$/;"	m	struct:mshclass
ext_patch_ieee80211_rx_frame_softmac_on_auth	ieee80211.h	/^	int (*ext_patch_ieee80211_rx_frame_softmac_on_auth)(struct ieee80211_device *ieee, struct sk_buff *skb, struct ieee80211_rx_stats *rx_stats);$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_rx_frame_softmac_on_auth	msh_class.h	/^	int (*ext_patch_ieee80211_rx_frame_softmac_on_auth)(struct ieee80211_device *ieee, struct sk_buff *skb, struct ieee80211_rx_stats *rx_stats);$/;"	m	struct:mshclass
ext_patch_ieee80211_rx_frame_softmac_on_deauth	ieee80211.h	/^	int (*ext_patch_ieee80211_rx_frame_softmac_on_deauth)(struct ieee80211_device *ieee, struct sk_buff *skb, struct ieee80211_rx_stats *rx_stats);$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_rx_frame_softmac_on_deauth	msh_class.h	/^	int (*ext_patch_ieee80211_rx_frame_softmac_on_deauth)(struct ieee80211_device *ieee, struct sk_buff *skb, struct ieee80211_rx_stats *rx_stats);$/;"	m	struct:mshclass
ext_patch_ieee80211_rx_is_valid_framectl	ieee80211.h	/^	int (*ext_patch_ieee80211_rx_is_valid_framectl) (struct ieee80211_device *ieee, u16 fc, u16 type, u16 stype);$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_rx_is_valid_framectl	msh_class.h	/^	int (*ext_patch_ieee80211_rx_is_valid_framectl) (struct ieee80211_device *ieee, u16 fc, u16 type, u16 stype);$/;"	m	struct:mshclass
ext_patch_ieee80211_rx_mgt_on_probe_req	ieee80211.h	/^	void (*ext_patch_ieee80211_rx_mgt_on_probe_req) ( struct ieee80211_device *ieee, struct ieee80211_probe_request *beacon, struct ieee80211_rx_stats *stats);$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_rx_mgt_on_probe_req	msh_class.h	/^	void (*ext_patch_ieee80211_rx_mgt_on_probe_req) ( struct ieee80211_device *ieee, struct ieee80211_probe_request *beacon, struct ieee80211_rx_stats *stats);$/;"	m	struct:mshclass
ext_patch_ieee80211_rx_mgt_update_expire	ieee80211.h	/^	void (*ext_patch_ieee80211_rx_mgt_update_expire) ( struct ieee80211_device *ieee, struct sk_buff *skb);$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_rx_mgt_update_expire	msh_class.h	/^	void (*ext_patch_ieee80211_rx_mgt_update_expire) ( struct ieee80211_device *ieee, struct sk_buff *skb);$/;"	m	struct:mshclass
ext_patch_ieee80211_rx_on_rx	ieee80211.h	/^	int (*ext_patch_ieee80211_rx_on_rx) (struct ieee80211_device *ieee, struct sk_buff *skb, struct ieee80211_rx_stats *rx_stats, u16 type, u16 stype);$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_rx_on_rx	msh_class.h	/^	int (*ext_patch_ieee80211_rx_on_rx) (struct ieee80211_device *ieee, struct sk_buff *skb, struct ieee80211_rx_stats *rx_stats, u16 type, u16 stype);$/;"	m	struct:mshclass
ext_patch_ieee80211_rx_process_dataframe	ieee80211.h	/^	int (*ext_patch_ieee80211_rx_process_dataframe) (struct ieee80211_device *ieee, struct sk_buff *skb, struct ieee80211_rx_stats *rx_stats);$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_rx_process_dataframe	msh_class.h	/^	int (*ext_patch_ieee80211_rx_process_dataframe) (struct ieee80211_device *ieee, struct sk_buff *skb, struct ieee80211_rx_stats *rx_stats);$/;"	m	struct:mshclass
ext_patch_ieee80211_softmac_xmit_get_rate	ieee80211.h	/^	int (*ext_patch_ieee80211_softmac_xmit_get_rate) (struct ieee80211_device *ieee, struct sk_buff *skb);$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_softmac_xmit_get_rate	msh_class.h	/^	int (*ext_patch_ieee80211_softmac_xmit_get_rate) (struct ieee80211_device *ieee, struct sk_buff *skb);$/;"	m	struct:mshclass
ext_patch_ieee80211_start_mesh	ieee80211.h	/^	void (*ext_patch_ieee80211_start_mesh)(struct ieee80211_device *ieee);$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_start_mesh	msh_class.h	/^	void (*ext_patch_ieee80211_start_mesh)(struct ieee80211_device *ieee);$/;"	m	struct:mshclass
ext_patch_ieee80211_start_protocol	ieee80211.h	/^	int (*ext_patch_ieee80211_start_protocol) (struct ieee80211_device *ieee); \/\/ start special mode$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_start_protocol	msh_class.h	/^	int (*ext_patch_ieee80211_start_protocol) (struct ieee80211_device *ieee); \/\/ start special mode$/;"	m	struct:mshclass
ext_patch_ieee80211_stop_protocol	ieee80211.h	/^	void (*ext_patch_ieee80211_stop_protocol) (struct ieee80211_device *ieee); \/\/ stop timer$/;"	m	struct:ieee80211_device
ext_patch_ieee80211_stop_protocol	msh_class.h	/^	void (*ext_patch_ieee80211_stop_protocol) (struct ieee80211_device *ieee); \/\/ stop timer$/;"	m	struct:mshclass
ext_patch_ieee80211_xmit	ieee80211.h	/^	struct ieee80211_txb* (*ext_patch_ieee80211_xmit) (struct sk_buff *skb, struct net_device *dev);$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::ext_patch_ieee80211_xmit
ext_patch_ieee80211_xmit	msh_class.h	/^	struct ieee80211_txb* (*ext_patch_ieee80211_xmit) (struct sk_buff *skb, struct net_device *dev);$/;"	m	struct:mshclass	typeref:struct:mshclass::ext_patch_ieee80211_xmit
ext_patch_is_duplicate_packet	msh_class.h	/^	int (*ext_patch_is_duplicate_packet) (struct ieee80211_device *ieee, struct ieee80211_hdr *header, u16 type, u16 stype);$/;"	m	struct:mshclass
ext_patch_r8180_wx_disable_mesh	msh_class.h	/^	int (*ext_patch_r8180_wx_disable_mesh) (struct net_device *dev);$/;"	m	struct:mshclass
ext_patch_r8180_wx_enable_mesh	msh_class.h	/^	int (*ext_patch_r8180_wx_enable_mesh) (struct net_device *dev);$/;"	m	struct:mshclass
ext_patch_r8180_wx_get_mac_allow	msh_class.h	/^	int (*ext_patch_r8180_wx_get_mac_allow) (struct net_device *dev, struct iw_request_info *info, union iwreq_data *wrqu, char *extra);$/;"	m	struct:mshclass
ext_patch_r8180_wx_get_mac_deny	msh_class.h	/^	int (*ext_patch_r8180_wx_get_mac_deny) (struct net_device *dev, struct iw_request_info *info, union iwreq_data *wrqu, char *extra);$/;"	m	struct:mshclass
ext_patch_r8180_wx_get_mesh_list	msh_class.h	/^	int (*ext_patch_r8180_wx_get_mesh_list) (struct net_device *dev, struct iw_request_info *info, union iwreq_data *wrqu, char *extra);$/;"	m	struct:mshclass
ext_patch_r8180_wx_get_meshinfo	msh_class.h	/^	int (*ext_patch_r8180_wx_get_meshinfo) (struct net_device *dev, struct iw_request_info *info, union iwreq_data *wrqu, char *extra);$/;"	m	struct:mshclass
ext_patch_r8180_wx_get_selected_mesh	msh_class.h	/^	int (*ext_patch_r8180_wx_get_selected_mesh)(struct net_device *dev, int en, char *cho, char* id);$/;"	m	struct:mshclass
ext_patch_r8180_wx_get_selected_mesh_channel	msh_class.h	/^	int (*ext_patch_r8180_wx_get_selected_mesh_channel)(struct net_device *dev, char* extmeshid, char *cho);$/;"	m	struct:mshclass
ext_patch_r8180_wx_mesh_scan	msh_class.h	/^	int (*ext_patch_r8180_wx_mesh_scan) (struct net_device *dev, struct iw_request_info *info, union iwreq_data *wrqu, char *extra);$/;"	m	struct:mshclass
ext_patch_r8180_wx_set_add_mac_allow	msh_class.h	/^	int (*ext_patch_r8180_wx_set_add_mac_allow) (struct net_device *dev, struct iw_request_info *info, union iwreq_data *wrqu, char *extra);$/;"	m	struct:mshclass
ext_patch_r8180_wx_set_add_mac_deny	msh_class.h	/^	int (*ext_patch_r8180_wx_set_add_mac_deny) (struct net_device *dev, struct iw_request_info *info, union iwreq_data *wrqu, char *extra);$/;"	m	struct:mshclass
ext_patch_r8180_wx_set_channel	msh_class.h	/^	void (*ext_patch_r8180_wx_set_channel) (struct ieee80211_device *ieee, int ch);$/;"	m	struct:mshclass
ext_patch_r8180_wx_set_del_mac_allow	msh_class.h	/^	int (*ext_patch_r8180_wx_set_del_mac_allow) (struct net_device *dev, struct iw_request_info *info, union iwreq_data *wrqu, char *extra);$/;"	m	struct:mshclass
ext_patch_r8180_wx_set_del_mac_deny	msh_class.h	/^	int (*ext_patch_r8180_wx_set_del_mac_deny) (struct net_device *dev, struct iw_request_info *info, union iwreq_data *wrqu, char *extra);$/;"	m	struct:mshclass
ext_patch_r8180_wx_set_meshID	msh_class.h	/^	int (*ext_patch_r8180_wx_set_meshID) ( struct net_device *dev, char *ext);$/;"	m	struct:mshclass
ext_patch_r8180_wx_set_mesh_chan	msh_class.h	/^	int (*ext_patch_r8180_wx_set_mesh_chan)(struct net_device *dev, unsigned char channel);$/;"	m	struct:mshclass
ext_patch_remove_proc	msh_class.h	/^	void (*ext_patch_remove_proc) (struct r8180_priv *priv);$/;"	m	struct:mshclass
ext_patch_rtl8180_ioctl	msh_class.h	/^	int (*ext_patch_rtl8180_ioctl) (struct net_device *dev, struct ifreq *rq, int cmd);$/;"	m	struct:mshclass
ext_patch_rtl8180_up	msh_class.h	/^	u8 (*ext_patch_rtl8180_up) (struct mshclass *priv);$/;"	m	struct:mshclass
ext_send_beacon_wq	ieee80211.h	/^	struct tq_struct ext_send_beacon_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::tq_struct
ext_send_beacon_wq	ieee80211.h	/^	struct work_struct ext_send_beacon_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::work_struct
ext_stop_scan_wq	ieee80211.h	/^	struct tq_struct ext_stop_scan_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::tq_struct
ext_stop_scan_wq	ieee80211.h	/^	struct work_struct ext_stop_scan_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::work_struct
extra_postfix_len	ieee80211_crypt.h	/^	int extra_prefix_len, extra_postfix_len;$/;"	m	struct:ieee80211_crypto_ops
extra_prefix_len	ieee80211_crypt.h	/^	int extra_prefix_len, extra_postfix_len;$/;"	m	struct:ieee80211_crypto_ops
f	r8187.h	/^	}f;	\/\/ Field$/;"	m	union:_ACI_AIFSN	typeref:struct:_ACI_AIFSN::__anon17
f	r8187.h	/^	}f;	\/\/ Field$/;"	m	union:_AC_PARAM	typeref:struct:_AC_PARAM::__anon18
f	r8187.h	/^	}f;	\/\/ Field$/;"	m	union:_ECW	typeref:struct:_ECW::__anon16
false	ieee80211.h	/^typedef enum{false = 0, true} bool;$/;"	e	enum:__anon1
first	r8187_core.c	/^unsigned int	first:1;$/;"	m	struct:rx_desc_rtl8187b	file:
first	r8187_core.c	/^unsigned int	first:1;$/;"	m	struct:tx_desc	file:
first	r8187_core.c	/^unsigned int    first:1;$/;"	m	struct:rx_desc_rtl8187	file:
first_frag_time	ieee80211.h	/^	unsigned long first_frag_time;$/;"	m	struct:ieee80211_frag_entry
flag_beacon	r8187.h	/^        bool                    flag_beacon;$/;"	m	struct:r8180_priv
flags	ieee80211.h	/^	u16 flags;$/;"	m	struct:ieee80211_security
flags	ieee80211.h	/^	u8 flags;$/;"	m	struct:ieee80211_network
force_pci_posting	r8187_core.c	/^inline void force_pci_posting(struct net_device *dev)$/;"	f
fot	r8187_core.c	/^unsigned int	fot:8;$/;"	m	struct:rx_desc_rtl8187b	file:
fovf	r8187_core.c	/^unsigned int	fovf:1;$/;"	m	struct:rx_desc_rtl8187b	file:
fovf	r8187_core.c	/^unsigned int    fovf:1;$/;"	m	struct:rx_desc_rtl8187	file:
frag	ieee80211.h	/^	int frag;$/;"	m	struct:tx_pending_t
frag_cache	ieee80211.h	/^	struct ieee80211_frag_entry frag_cache[17][IEEE80211_FRAG_CACHE_LEN];$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::ieee80211_frag_entry
frag_next_idx	ieee80211.h	/^	unsigned int frag_next_idx[17];$/;"	m	struct:ieee80211_device
frag_num	ieee80211.h	/^	u16 frag_num;$/;"	m	struct:ieee_mesh_seq
frag_num	ieee80211.h	/^	u16 frag_num[17];$/;"	m	struct:ieee_ibss_seq
frag_size	ieee80211.h	/^	u16 frag_size;$/;"	m	struct:ieee80211_txb
fragments	ieee80211.h	/^	struct sk_buff *fragments[0];$/;"	m	struct:ieee80211_txb	typeref:struct:ieee80211_txb::sk_buff
fragqsz	r8187_core.c	/^unsigned short	fragqsz;$/;"	m	struct:tx_desc	file:
frame_ctl	ieee80211.h	/^	u16 frame_ctl;$/;"	m	struct:ieee80211_hdr
frame_ctl	ieee80211.h	/^	u16 frame_ctl;$/;"	m	struct:ieee80211_hdr_3addr
frame_ctl	ieee80211.h	/^	u16 frame_ctl;$/;"	m	struct:ieee80211_hdr_3addr_QOS
frame_ctl	ieee80211.h	/^	u16 frame_ctl;$/;"	m	struct:ieee80211_hdr_QOS
frame_ctl	ieee80211.h	/^	u16 frame_ctl;$/;"	m	struct:ieee80211_header_data
free_ieee80211	ieee80211.h	127;"	d
freq	ieee80211.h	/^	u8 freq;$/;"	m	struct:ieee80211_rx_stats
freq_band	ieee80211.h	/^	int freq_band;  \/* 2.4Ghz, 5.2Ghz, Mixed *\/$/;"	m	struct:ieee80211_device
fts	ieee80211.h	/^	u16 fts; \/* Fragmentation Threshold *\/$/;"	m	struct:ieee80211_device
get_key	ieee80211_crypt.h	/^	int (*get_key)(void *key, int len, u8 *seq, void *priv);$/;"	m	struct:ieee80211_crypto_ops
gpio_change_polling	r8187_core.c	/^void gpio_change_polling(unsigned long data)$/;"	f
gpio_polling_timer	r8187.h	/^	struct timer_list gpio_polling_timer;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::timer_list
hard_start_xmit	ieee80211.h	/^	int (*hard_start_xmit)(struct ieee80211_txb *txb,$/;"	m	struct:ieee80211_device
head	r8187.h	/^        } head;$/;"	m	struct:rtl_reg_debug	typeref:struct:rtl_reg_debug::__anon13
header	ieee80211.h	/^	struct ieee80211_hdr_3addr header;$/;"	m	struct:ieee80211_assoc_request_frame	typeref:struct:ieee80211_assoc_request_frame::ieee80211_hdr_3addr
header	ieee80211.h	/^	struct ieee80211_hdr_3addr header;$/;"	m	struct:ieee80211_assoc_response_frame	typeref:struct:ieee80211_assoc_response_frame::ieee80211_hdr_3addr
header	ieee80211.h	/^	struct ieee80211_header_data header;$/;"	m	struct:ieee80211_authentication	typeref:struct:ieee80211_authentication::ieee80211_header_data
header	ieee80211.h	/^	struct ieee80211_header_data header;$/;"	m	struct:ieee80211_probe_request	typeref:struct:ieee80211_probe_request::ieee80211_header_data
header	ieee80211.h	/^	struct ieee80211_header_data header;$/;"	m	struct:ieee80211_probe_response	typeref:struct:ieee80211_probe_response::ieee80211_header_data
host_decrypt	ieee80211.h	/^	int host_decrypt;$/;"	m	struct:ieee80211_device
host_encrypt	ieee80211.h	/^	int host_encrypt;$/;"	m	struct:ieee80211_device
hw_dig_wq	ieee80211.h	/^	struct delayed_work hw_dig_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::delayed_work
hw_dig_wq	ieee80211.h	/^	struct work_struct hw_dig_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::work_struct
hw_plcp_len	r8187.h	/^	short hw_plcp_len;$/;"	m	struct:r8180_priv
ibss_mac_hash	ieee80211.h	/^	struct list_head ibss_mac_hash[IEEE_IBSS_MAC_HASH_SIZE];$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::list_head
icv	r8187_core.c	/^unsigned int	icv:1;$/;"	m	struct:rx_desc_rtl8187b	file:
icv	r8187_core.c	/^unsigned int    icv:1;$/;"	m	struct:rx_desc_rtl8187	file:
id	ieee80211.h	/^	u8 id;$/;"	m	struct:ieee80211_info_element
id	ieee80211.h	/^	u8 id;$/;"	m	struct:ieee80211_info_element_hdr
idx	ieee80211.h	/^			u8 idx;$/;"	m	struct:ieee_param::__anon2::__anon6
idx	r8187_core.c	/^                        u8 idx;$/;"	m	struct:ipw_param::__anon8::__anon12	file:
ieee80211	r8187.h	/^	struct ieee80211_device *ieee80211;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::ieee80211_device
ieee80211_assoc_request_frame	ieee80211.h	/^struct ieee80211_assoc_request_frame {$/;"	s
ieee80211_assoc_response_frame	ieee80211.h	/^struct ieee80211_assoc_response_frame {$/;"	s
ieee80211_authentication	ieee80211.h	/^struct ieee80211_authentication {$/;"	s
ieee80211_crypt_data	ieee80211_crypt.h	/^struct ieee80211_crypt_data {$/;"	s
ieee80211_crypt_data_list	ieee80211.h	/^struct ieee80211_crypt_data_list{$/;"	s
ieee80211_crypt_deinit_entries	ieee80211.h	141;"	d
ieee80211_crypt_deinit_handler	ieee80211.h	142;"	d
ieee80211_crypt_delayed_deinit	ieee80211.h	136;"	d
ieee80211_crypto_ops	ieee80211_crypt.h	/^struct ieee80211_crypto_ops {$/;"	s
ieee80211_device	ieee80211.h	/^struct ieee80211_device {$/;"	s
ieee80211_find_MP	ieee80211.h	/^extern inline int ieee80211_find_MP(struct ieee80211_device* ieee, const u8* addr, u8 set)$/;"	f
ieee80211_frag_entry	ieee80211.h	/^struct ieee80211_frag_entry {$/;"	s
ieee80211_get_crypto_ops	ieee80211.h	135;"	d
ieee80211_get_hdrlen	ieee80211.h	/^extern inline int ieee80211_get_hdrlen(u16 fc)$/;"	f
ieee80211_get_scans	ieee80211.h	/^extern inline int ieee80211_get_scans(struct ieee80211_device *ieee)$/;"	f
ieee80211_hdr	ieee80211.h	/^struct ieee80211_hdr {$/;"	s
ieee80211_hdr_3addr	ieee80211.h	/^struct ieee80211_hdr_3addr {$/;"	s
ieee80211_hdr_3addr_QOS	ieee80211.h	/^struct ieee80211_hdr_3addr_QOS {$/;"	s
ieee80211_hdr_QOS	ieee80211.h	/^struct ieee80211_hdr_QOS {$/;"	s
ieee80211_header_data	ieee80211.h	/^struct ieee80211_header_data {$/;"	s
ieee80211_increment_scans	ieee80211.h	/^extern inline void ieee80211_increment_scans(struct ieee80211_device *ieee)$/;"	f
ieee80211_info_element	ieee80211.h	/^struct ieee80211_info_element {$/;"	s
ieee80211_info_element_hdr	ieee80211.h	/^struct ieee80211_info_element_hdr {$/;"	s
ieee80211_is_empty_essid	ieee80211.h	/^extern inline int ieee80211_is_empty_essid(const char *essid, int essid_len)$/;"	f
ieee80211_is_valid_mode	ieee80211.h	/^extern inline int ieee80211_is_valid_mode(struct ieee80211_device *ieee, int mode)$/;"	f
ieee80211_led_contorl	ieee80211.h	/^	void (*ieee80211_led_contorl) (struct net_device *dev, LED_CTL_MODE LedAction);$/;"	m	struct:ieee80211_device
ieee80211_network	ieee80211.h	/^struct ieee80211_network {$/;"	s
ieee80211_priv	ieee80211.h	/^extern inline void *ieee80211_priv(struct net_device *dev)$/;"	f
ieee80211_probe_request	ieee80211.h	/^struct ieee80211_probe_request {$/;"	s
ieee80211_probe_response	ieee80211.h	/^struct ieee80211_probe_response {$/;"	s
ieee80211_register_crypto_ops	ieee80211.h	139;"	d
ieee80211_rx	ieee80211.h	131;"	d
ieee80211_rx_stats	ieee80211.h	/^struct ieee80211_rx_stats {$/;"	s
ieee80211_security	ieee80211.h	/^struct ieee80211_security {$/;"	s
ieee80211_snap_hdr	ieee80211.h	/^struct ieee80211_snap_hdr {$/;"	s
ieee80211_softmac_stats	ieee80211.h	/^struct ieee80211_softmac_stats{$/;"	s
ieee80211_start_scan	ieee80211.h	138;"	d
ieee80211_state	ieee80211.h	/^enum ieee80211_state {$/;"	g
ieee80211_stats	ieee80211.h	/^struct ieee80211_stats {$/;"	s
ieee80211_stop_queue	ieee80211.h	133;"	d
ieee80211_txb	ieee80211.h	/^struct ieee80211_txb {$/;"	s
ieee80211_unregister_crypto_ops	ieee80211.h	140;"	d
ieee80211_wake_queue	ieee80211.h	132;"	d
ieee80211_wmm_ac_param	ieee80211.h	/^struct ieee80211_wmm_ac_param {$/;"	s
ieee80211_wmm_ts_info	ieee80211.h	/^struct ieee80211_wmm_ts_info {$/;"	s
ieee80211_wmm_tspec_elem	ieee80211.h	/^struct ieee80211_wmm_tspec_elem {$/;"	s
ieee80211_wx_get_encode	ieee80211.h	123;"	d
ieee80211_wx_get_name	ieee80211.h	126;"	d
ieee80211_wx_get_scan	ieee80211.h	121;"	d
ieee80211_wx_set_auth	ieee80211.h	134;"	d
ieee80211_wx_set_encode	ieee80211.h	122;"	d
ieee802_1x	ieee80211.h	/^	int ieee802_1x; \/* is IEEE 802.1X used *\/$/;"	m	struct:ieee80211_device
ieee_ibss_seq	ieee80211.h	/^struct ieee_ibss_seq {$/;"	s
ieee_mesh_seq	ieee80211.h	/^struct ieee_mesh_seq {$/;"	s
ieee_param	ieee80211.h	/^typedef struct ieee_param {$/;"	s
ieee_param	ieee80211.h	/^}ieee_param;$/;"	t	typeref:struct:ieee_param
ieee_stats	ieee80211.h	/^	struct ieee80211_stats ieee_stats;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::ieee80211_stats
ieeerate2rtlrate	r8187_core.c	/^inline u16 ieeerate2rtlrate(int rate)$/;"	f
ifname	r8187_core.c	/^static char* ifname = "wlan%d";$/;"	v	file:
inact_inter	ieee80211.h	/^	u32 inact_inter;$/;"	m	struct:ieee80211_wmm_tspec_elem
info_element	ieee80211.h	/^	struct ieee80211_info_element info_element; \/* supported rates *\/$/;"	m	struct:ieee80211_assoc_response_frame	typeref:struct:ieee80211_assoc_response_frame::ieee80211_info_element
info_element	ieee80211.h	/^	struct ieee80211_info_element info_element;$/;"	m	struct:ieee80211_probe_response	typeref:struct:ieee80211_probe_response::ieee80211_info_element
info_element	ieee80211.h	/^	struct ieee80211_info_element_hdr info_element;$/;"	m	struct:ieee80211_assoc_request_frame	typeref:struct:ieee80211_assoc_request_frame::ieee80211_info_element_hdr
init	ieee80211_crypt.h	/^	void * (*init)(int keyidx);$/;"	m	struct:ieee80211_crypto_ops
init_wmmparam_flag	ieee80211.h	/^	char init_wmmparam_flag;$/;"	m	struct:ieee80211_device
ips_sem	ieee80211.h	/^	struct semaphore ips_sem;	$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::semaphore
ipw_param	r8187_core.c	/^struct ipw_param {$/;"	s	file:
irq	r8187.h	/^	int irq;$/;"	m	struct:r8180_priv
irq_lock	r8187.h	/^	spinlock_t irq_lock;$/;"	m	struct:r8180_priv
irq_mask	r8187.h	/^	u16 irq_mask;$/;"	m	struct:r8180_priv
irq_rx_tasklet	r8187.h	/^	struct tasklet_struct irq_rx_tasklet;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::tasklet_struct
irt_counter	r8187.h	/^	atomic_t irt_counter;\/\/count for irq_rx_tasklet$/;"	m	struct:r8180_priv
is_broadcast_ether_addr	ieee80211.h	/^extern inline int is_broadcast_ether_addr(const u8 *addr)$/;"	f
is_multicast_ether_addr	ieee80211.h	/^extern inline int is_multicast_ether_addr(const u8 *addr)$/;"	f
is_same_network	r8180_wx.c	/^static inline int is_same_network(struct ieee80211_network *src,$/;"	f	file:
iw_ext_mode	ieee80211.h	/^	int iw_ext_mode; \/\/ if iw_mode == iw_ext_mode, do ext_patch_**();$/;"	m	struct:ieee80211_device
iw_mode	ieee80211.h	/^	int iw_mode; \/* operating mode (IW_MODE_*) *\/$/;"	m	struct:ieee80211_device
key	ieee80211.h	/^			u8 key[0];$/;"	m	struct:ieee_param::__anon2::__anon6
key	r8187_core.c	/^                        u8 key[0];$/;"	m	struct:ipw_param::__anon8::__anon12	file:
key_len	ieee80211.h	/^			u16 key_len;$/;"	m	struct:ieee_param::__anon2::__anon6
key_len	r8187_core.c	/^                        u16 key_len;$/;"	m	struct:ipw_param::__anon8::__anon12	file:
key_sizes	ieee80211.h	/^	u8 key_sizes[WEP_KEYS];$/;"	m	struct:ieee80211_security
keys	ieee80211.h	/^	u8 keys[WEP_KEYS][ALG_KEY_LEN];$/;"	m	struct:ieee80211_security
l_ext	r8187_core.c	/^unsigned short  l_ext:1;$/;"	m	struct:tx_desc	file:
last	r8187_core.c	/^unsigned int	last:1;$/;"	m	struct:rx_desc_rtl8187b	file:
last	r8187_core.c	/^unsigned int	last:1;$/;"	m	struct:tx_desc	file:
last	r8187_core.c	/^unsigned int    last:1;$/;"	m	struct:rx_desc_rtl8187	file:
last_associate	ieee80211.h	/^	u32 last_associate;$/;"	m	struct:ieee80211_network
last_dtim_sta_time	ieee80211.h	/^	u32 last_dtim_sta_time[2];$/;"	m	struct:ieee80211_network
last_frag	ieee80211.h	/^	unsigned int last_frag;$/;"	m	struct:ieee80211_frag_entry
last_packet_time	ieee80211.h	/^	unsigned long last_packet_time[17];$/;"	m	struct:ieee80211_device
last_rx_ps_time	ieee80211.h	/^	unsigned long last_rx_ps_time;$/;"	m	struct:ieee80211_device
last_rxfrag_num	ieee80211.h	/^	u16 last_rxfrag_num[17];\/* tx frag previous per-tid *\/$/;"	m	struct:ieee80211_device
last_rxseq_num	ieee80211.h	/^	u16 last_rxseq_num[17]; \/* rx seq previous per-tid *\/$/;"	m	struct:ieee80211_device
last_scanned	ieee80211.h	/^	unsigned long last_scanned;$/;"	m	struct:ieee80211_network
len	ieee80211.h	/^			u32 len;$/;"	m	struct:ieee_param::__anon2::__anon4
len	ieee80211.h	/^	u16 len;$/;"	m	struct:ieee80211_rx_stats
len	ieee80211.h	/^	u8 len;$/;"	m	struct:ieee80211_info_element
len	ieee80211.h	/^	u8 len;$/;"	m	struct:ieee80211_info_element_hdr
len	r8187_core.c	/^                        u32 len;$/;"	m	struct:ipw_param::__anon8::__anon10	file:
len_adjust	r8187_core.c	/^unsigned char	len_adjust:2;$/;"	m	struct:tx_desc	file:
length	ieee80211.h	/^	u16 length;$/;"	m	struct:eapol
length	r8187.h	/^                unsigned char length;$/;"	m	struct:rtl_reg_debug::__anon13
length	r8187_core.c	/^unsigned short  length:15;$/;"	m	struct:tx_desc	file:
level	ieee80211.h	/^	u8 level;$/;"	m	struct:ieee80211_security
link_change	ieee80211.h	/^	void (*link_change)(struct net_device *dev);$/;"	m	struct:ieee80211_device
link_detect	r8187.h	/^	struct _link_detect_t link_detect;  \/\/added on 1016.2008$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::_link_detect_t
link_detect_t	r8187.h	/^}link_detect_t, *plink_detect_t;$/;"	t	typeref:struct:_link_detect_t
list	ieee80211.h	/^	struct list_head list;$/;"	m	struct:ieee80211_network	typeref:struct:ieee80211_network::list_head
list	ieee80211.h	/^	struct list_head list;$/;"	m	struct:ieee_ibss_seq	typeref:struct:ieee_ibss_seq::list_head
list	ieee80211.h	/^	struct list_head list;$/;"	m	struct:ieee_mesh_seq	typeref:struct:ieee_mesh_seq::list_head
list	ieee80211_crypt.h	/^	struct list_head list; \/* delayed deletion list *\/$/;"	m	struct:ieee80211_crypt_data	typeref:struct:ieee80211_crypt_data::list_head
listen_interval	ieee80211.h	/^	u16 listen_interval;$/;"	m	struct:ieee80211_assoc_request_frame
listen_interval	ieee80211.h	/^	u16 listen_interval;$/;"	m	struct:ieee80211_network
lock	ieee80211.h	/^	spinlock_t lock;$/;"	m	struct:ieee80211_device
longData	r8187.h	/^	u32	longData;$/;"	m	union:_AC_PARAM
mac	ieee80211.h	/^	u8 mac[ETH_ALEN];$/;"	m	struct:ieee_ibss_seq
mac	ieee80211.h	/^	u8 mac[ETH_ALEN];$/;"	m	struct:ieee_mesh_seq
mac_addr	ieee80211.h	/^	u8 mac_addr[ETH_ALEN];  \/\/record mac_add$/;"	m	struct:ieee80211_crypt_data_list
mac_time	ieee80211.h	/^	u32 mac_time[2];$/;"	m	struct:ieee80211_rx_stats
mar	r8187_core.c	/^unsigned int	mar:1;$/;"	m	struct:rx_desc_rtl8187b	file:
mar	r8187_core.c	/^unsigned int    mar:1;$/;"	m	struct:rx_desc_rtl8187	file:
mask	ieee80211.h	/^	u8 mask;$/;"	m	struct:ieee80211_rx_stats
max_burst_size	ieee80211.h	/^	u32 max_burst_size;$/;"	m	struct:ieee80211_wmm_tspec_elem
max_msdu_size	ieee80211.h	/^	u16 max_msdu_size;$/;"	m	struct:ieee80211_wmm_tspec_elem
max_sens	r8187.h	/^	short max_sens;$/;"	m	struct:r8180_priv
max_serv_inter	ieee80211.h	/^	u32 max_serv_inter;$/;"	m	struct:ieee80211_wmm_tspec_elem
mean_data_rate	ieee80211.h	/^	u32 mean_data_rate;$/;"	m	struct:ieee80211_wmm_tspec_elem
medium_time	ieee80211.h	/^	u16 medium_time;$/;"	m	struct:ieee80211_wmm_tspec_elem
meshScanMode	ieee80211.h	/^        short meshScanMode;$/;"	m	struct:ieee80211_device
mesh_mac_hash	ieee80211.h	/^	struct list_head mesh_mac_hash[IEEE_MESH_MAC_HASH_SIZE];$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::list_head
meshid_set	ieee80211.h	/^	short meshid_set;	$/;"	m	struct:ieee80211_device
mgmt_queue_head	ieee80211.h	/^	int mgmt_queue_head;$/;"	m	struct:ieee80211_device
mgmt_queue_ring	ieee80211.h	/^	struct sk_buff *mgmt_queue_ring[MGMT_QUEUE_NUM];$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::sk_buff
mgmt_queue_tail	ieee80211.h	/^	int mgmt_queue_tail;$/;"	m	struct:ieee80211_device
mgmt_tx_lock	ieee80211.h	/^	spinlock_t mgmt_tx_lock;	$/;"	m	struct:ieee80211_device
miccal	r8187_core.c	/^unsigned short  miccal:1;$/;"	m	struct:tx_desc	file:
min_data_rate	ieee80211.h	/^	u32 min_data_rate;$/;"	m	struct:ieee80211_wmm_tspec_elem
min_phy_rate	ieee80211.h	/^	u32 min_phy_rate;$/;"	m	struct:ieee80211_wmm_tspec_elem
min_serv_inter	ieee80211.h	/^	u32 min_serv_inter;$/;"	m	struct:ieee80211_wmm_tspec_elem
mlme	ieee80211.h	/^		} mlme;$/;"	m	union:ieee_param::__anon2	typeref:struct:ieee_param::__anon2::__anon5
mlme	r8187_core.c	/^                } mlme;$/;"	m	union:ipw_param::__anon8	typeref:struct:ipw_param::__anon8::__anon11	file:
mode	ieee80211.h	/^	int mode;       \/* A, B, G *\/$/;"	m	struct:ieee80211_device
mode	ieee80211.h	/^	u8 mode;$/;"	m	struct:ieee80211_network
modulation	ieee80211.h	/^	int modulation; \/* CCK, OFDM *\/$/;"	m	struct:ieee80211_device
morefrag	r8187_core.c	/^unsigned int    morefrag:1;$/;"	m	struct:tx_desc	file:
mshclass	msh_class.h	/^struct mshclass {$/;"	s
mshobj	r8187.h	/^	struct mshclass			*mshobj;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::mshclass
msleep_interruptible_rtl	ieee80211.h	/^static inline unsigned long msleep_interruptible_rtl(unsigned int msecs)$/;"	f
msleep_interruptible_rtl	ieee80211.h	210;"	d
name	ieee80211.h	/^			u8 name;$/;"	m	struct:ieee_param::__anon2::__anon3
name	ieee80211_crypt.h	/^	const char *name;$/;"	m	struct:ieee80211_crypto_ops
name	r8187.h	/^       	u8 name[IW_ESSID_MAX_SIZE + 1];$/;"	m	struct:ssid_thread
name	r8187_core.c	/^                        u8 name;$/;"	m	struct:ipw_param::__anon8::__anon9	file:
network_free_list	ieee80211.h	/^	struct list_head network_free_list;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::list_head
network_list	ieee80211.h	/^	struct list_head network_list;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::list_head
networks	ieee80211.h	/^	struct ieee80211_network *networks;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::ieee80211_network
next	r8187.h	/^	struct buffer *next;$/;"	m	struct:buffer	typeref:struct:buffer::buffer
nextdescaddr	r8187_core.c	/^unsigned int	nextdescaddr;$/;"	m	struct:tx_desc	file:
nic_t	r8187.h	/^	} nic_t;$/;"	t	typeref:enum:__anon15
nic_type	ieee80211.h	/^	u8 nic_type;$/;"	m	struct:ieee80211_rx_stats
no_ass_rs	ieee80211.h	/^	unsigned int no_ass_rs;$/;"	m	struct:ieee80211_softmac_stats
no_auth_rs	ieee80211.h	/^	unsigned int no_auth_rs;$/;"	m	struct:ieee80211_softmac_stats
no_encrypt	r8187_core.c	/^unsigned int    no_encrypt:1;$/;"	m	struct:tx_desc	file:
noacm	r8187_core.c	/^unsigned short	noacm:1;$/;"	m	struct:tx_desc	file:
noise	ieee80211.h	/^	u8 noise;$/;"	m	struct:ieee80211_rx_stats
norm_msdu_size	ieee80211.h	/^	u16 norm_msdu_size;$/;"	m	struct:ieee80211_wmm_tspec_elem
nr_frags	ieee80211.h	/^	u8 nr_frags;$/;"	m	struct:ieee80211_txb
num_mcsi	r8187_core.c	/^unsigned int	num_mcsi:4;$/;"	m	struct:rx_desc_rtl8187b	file:
obj-m	Makefile	/^obj-m := r8187.o$/;"	m
ofdm_txpwr_base	r8187.h	/^	u8 ofdm_txpwr_base;$/;"	m	struct:r8180_priv
offset_in_page	ieee80211_crypt.h	86;"	d
oldaddr	r8187.h	/^	u32 *oldaddr;$/;"	m	struct:r8180_priv
open_wep	ieee80211.h	/^	int open_wep; \/* Set to 1 to allow unencrypted frames *\/$/;"	m	struct:ieee80211_device
ops	ieee80211_crypt.h	/^	struct ieee80211_crypto_ops *ops;$/;"	m	struct:ieee80211_crypt_data	typeref:struct:ieee80211_crypt_data::ieee80211_crypto_ops
oui	ieee80211.h	/^        u8    oui[P80211_OUI_LEN];    \/* organizational universal id *\/$/;"	m	struct:ieee80211_snap_hdr
own	r8187_core.c	/^unsigned int	own:1;$/;"	m	struct:rx_desc_rtl8187b	file:
own	r8187_core.c	/^unsigned int	own:1;$/;"	m	struct:tx_desc	file:
own	r8187_core.c	/^unsigned int    own:1;$/;"	m	struct:rx_desc_rtl8187	file:
owner	ieee80211_crypt.h	/^	struct module *owner;$/;"	m	struct:ieee80211_crypto_ops	typeref:struct:ieee80211_crypto_ops::module
p8187	msh_class.h	/^	struct r8180_priv *	p8187;$/;"	m	struct:mshclass	typeref:struct:mshclass::r8180_priv
packet_time	ieee80211.h	/^	unsigned long packet_time;$/;"	m	struct:ieee_mesh_seq
packet_time	ieee80211.h	/^	unsigned long packet_time[17];$/;"	m	struct:ieee_ibss_seq
page	r8187.h	/^                unsigned char page;$/;"	m	struct:rtl_reg_debug::__anon13
pairwise_key_type	ieee80211.h	/^	u16 pairwise_key_type;$/;"	m	struct:ieee80211_device
pam	r8187_core.c	/^unsigned int	pam:1;$/;"	m	struct:rx_desc_rtl8187b	file:
pam	r8187_core.c	/^unsigned int    pam:1;$/;"	m	struct:rx_desc_rtl8187	file:
payload_size	ieee80211.h	/^	u16 payload_size;$/;"	m	struct:ieee80211_txb
peak_data_rate	ieee80211.h	/^	u32 peak_data_rate;$/;"	m	struct:ieee80211_wmm_tspec_elem
phy_ver	r8187.h	/^	short phy_ver; \/* meaningful for rtl8225 1:A 2:B 3:C *\/$/;"	m	struct:r8180_priv
pifs	r8187_core.c	/^unsigned short	pifs:1;$/;"	m	struct:tx_desc	file:
plcp_preamble_mode	r8187.h	/^	short plcp_preamble_mode;$/;"	m	struct:r8180_priv
plink_detect_t	r8187.h	/^}link_detect_t, *plink_detect_t;$/;"	t	typeref:struct:_link_detect_t
pp_rxskb	r8187.h	/^        struct sk_buff **pp_rxskb;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::sk_buff
print_buffer	r8187_core.c	/^void print_buffer(u32 *buffer, int len)$/;"	f
print_stats	ieee80211_crypt.h	/^	char * (*print_stats)(char *p, void *priv);$/;"	m	struct:ieee80211_crypto_ops
priority_t	r8187.h	/^} priority_t;$/;"	t	typeref:enum:__anon14
priv	ieee80211.h	/^	u8 priv[0];$/;"	m	struct:ieee80211_device
priv	ieee80211_crypt.h	/^	void *priv;$/;"	m	struct:ieee80211_crypt_data
priv	msh_class.h	/^	u8					priv[0]; \/\/ mshclass_priv;$/;"	m	struct:mshclass
privacy_invoked	ieee80211.h	/^	int privacy_invoked;$/;"	m	struct:ieee80211_device
proc_get_cck_reg	r8187_core.c	/^static int proc_get_cck_reg(char *page, char **start,$/;"	f	file:
proc_get_ofdm_reg	r8187_core.c	/^static int proc_get_ofdm_reg(char *page, char **start,$/;"	f	file:
proc_get_registers	r8187_core.c	/^static int proc_get_registers(char *page, char **start,$/;"	f	file:
proc_get_stats_ap	r8187_core.c	/^static int proc_get_stats_ap(char *page, char **start,$/;"	f	file:
proc_get_stats_rx	r8187_core.c	/^static int proc_get_stats_rx(char *page, char **start,$/;"	f	file:
proc_get_stats_tx	r8187_core.c	/^static int proc_get_stats_tx(char *page, char **start,$/;"	f	file:
promisc	r8187.h	/^	short promisc;	$/;"	m	struct:r8180_priv
proto_started	ieee80211.h	/^	short proto_started;$/;"	m	struct:ieee80211_device
ps	ieee80211.h	/^	short ps;$/;"	m	struct:ieee80211_device
ps_is_queue_empty	ieee80211.h	/^	short (*ps_is_queue_empty) (struct net_device *dev);$/;"	m	struct:ieee80211_device
ps_mode	r8187.h	/^	bool ps_mode;$/;"	m	struct:r8180_priv
ps_request_tx_ack	ieee80211.h	/^	void (*ps_request_tx_ack) (struct net_device *dev);$/;"	m	struct:ieee80211_device
ps_task	ieee80211.h	/^	struct tasklet_struct ps_task;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::tasklet_struct
ps_th	ieee80211.h	/^	u32 ps_th;$/;"	m	struct:ieee80211_device
ps_timeout	ieee80211.h	/^	int ps_timeout;$/;"	m	struct:ieee80211_device
ps_tl	ieee80211.h	/^	u32 ps_tl;$/;"	m	struct:ieee80211_device
pten	r8187_core.c	/^unsigned char	pten:1;$/;"	m	struct:tx_desc	file:
pwdb_g12	r8187_core.c	/^int	pwdb_g12:8;$/;"	m	struct:rx_desc_rtl8187b	file:
pwrmgt	r8187_core.c	/^unsigned int	pwrmgt:1;$/;"	m	struct:rx_desc_rtl8187b	file:
pwrmgt	r8187_core.c	/^unsigned int    pwrmgt:1;$/;"	m	struct:rx_desc_rtl8187	file:
qos	r8187_core.c	/^unsigned int	qos:1;$/;"	m	struct:rx_desc_rtl8187b	file:
qos	r8187_core.c	/^unsigned int    qos:1;$/;"	m	struct:rx_desc_rtl8187	file:
queue_stop	ieee80211.h	/^	short queue_stop;$/;"	m	struct:ieee80211_device
r8180_get_wireless_stats	r8180_wx.c	/^static struct iw_statistics *r8180_get_wireless_stats(struct net_device *dev)$/;"	f	file:
r8180_get_wireless_stats	r8187_core.c	/^static struct iw_statistics *r8180_get_wireless_stats(struct net_device *dev)$/;"	f	file:
r8180_priv	r8187.h	/^typedef struct r8180_priv$/;"	s
r8180_priv	r8187.h	/^}r8180_priv;$/;"	t	typeref:struct:r8180_priv
r8180_private_args	r8180_wx.c	/^static const struct iw_priv_args r8180_private_args[] = { $/;"	v	typeref:struct:iw_priv_args	file:
r8180_private_handler	r8180_wx.c	/^static iw_handler r8180_private_handler[] = {$/;"	v	file:
r8180_set_mac_adr	r8187_core.c	/^int r8180_set_mac_adr(struct net_device *dev, void *mac)$/;"	f
r8180_set_multicast	r8187_core.c	/^static void r8180_set_multicast(struct net_device *dev)$/;"	f	file:
r8180_wx_add_mac_deny	r8180_wx.c	/^static int r8180_wx_add_mac_deny(struct net_device *dev, $/;"	f	file:
r8180_wx_del_mac_deny	r8180_wx.c	/^static int r8180_wx_del_mac_deny(struct net_device *dev, $/;"	f	file:
r8180_wx_disable_mesh	r8180_wx.c	/^static int r8180_wx_disable_mesh(struct net_device *dev, $/;"	f	file:
r8180_wx_enable_mesh	r8180_wx.c	/^static int r8180_wx_enable_mesh(struct net_device *dev, $/;"	f	file:
r8180_wx_get_ap_status	r8180_wx.c	/^static int r8180_wx_get_ap_status(struct net_device *dev,$/;"	f	file:
r8180_wx_get_enc	r8180_wx.c	/^static int r8180_wx_get_enc(struct net_device *dev, $/;"	f	file:
r8180_wx_get_essid	r8180_wx.c	/^static int r8180_wx_get_essid(struct net_device *dev, $/;"	f	file:
r8180_wx_get_frag	r8180_wx.c	/^static int r8180_wx_get_frag(struct net_device *dev, $/;"	f	file:
r8180_wx_get_freq	r8180_wx.c	/^static int r8180_wx_get_freq(struct net_device *dev,$/;"	f	file:
r8180_wx_get_mac_deny	r8180_wx.c	/^static int r8180_wx_get_mac_deny(struct net_device *dev, $/;"	f	file:
r8180_wx_get_mesh_list	r8180_wx.c	/^static int r8180_wx_get_mesh_list(struct net_device *dev, $/;"	f	file:
r8180_wx_get_meshinfo	r8180_wx.c	/^static int r8180_wx_get_meshinfo(struct net_device *dev, $/;"	f	file:
r8180_wx_get_mode	r8180_wx.c	/^static int r8180_wx_get_mode(struct net_device *dev, struct iw_request_info *a,$/;"	f	file:
r8180_wx_get_name	r8180_wx.c	/^static int r8180_wx_get_name(struct net_device *dev, $/;"	f	file:
r8180_wx_get_radion	r8180_wx.c	/^static int r8180_wx_get_radion(struct net_device *dev, $/;"	f	file:
r8180_wx_get_rate	r8180_wx.c	/^static int r8180_wx_get_rate(struct net_device *dev, $/;"	f	file:
r8180_wx_get_retry	r8180_wx.c	/^static int r8180_wx_get_retry(struct net_device *dev, $/;"	f	file:
r8180_wx_get_scan	r8180_wx.c	/^static int r8180_wx_get_scan(struct net_device *dev, struct iw_request_info *a,$/;"	f	file:
r8180_wx_get_sens	r8180_wx.c	/^static int r8180_wx_get_sens(struct net_device *dev, $/;"	f	file:
r8180_wx_get_wap	r8180_wx.c	/^static int r8180_wx_get_wap(struct net_device *dev, $/;"	f	file:
r8180_wx_handlers	r8180_wx.c	/^static iw_handler r8180_wx_handlers[] =$/;"	v	file:
r8180_wx_handlers_def	r8180_wx.c	/^struct iw_handler_def  r8180_wx_handlers_def={$/;"	v	typeref:struct:iw_handler_def
r8180_wx_join_mesh	r8180_wx.c	/^static int r8180_wx_join_mesh(struct net_device *dev, $/;"	f	file:
r8180_wx_mesh_scan	r8180_wx.c	/^static int r8180_wx_mesh_scan(struct net_device *dev, $/;"	f	file:
r8180_wx_read_bb	r8180_wx.c	/^static int r8180_wx_read_bb(struct net_device *dev, $/;"	f	file:
r8180_wx_read_nicb	r8180_wx.c	/^static int r8180_wx_read_nicb(struct net_device *dev,$/;"	f	file:
r8180_wx_read_regs	r8180_wx.c	/^static int r8180_wx_read_regs(struct net_device *dev, $/;"	f	file:
r8180_wx_set_auth	r8180_wx.c	/^static int r8180_wx_set_auth(struct net_device *dev,$/;"	f	file:
r8180_wx_set_channel	r8180_wx.c	/^EXPORT_SYMBOL(r8180_wx_set_channel);$/;"	v
r8180_wx_set_channel	r8180_wx.c	/^int r8180_wx_set_channel(struct net_device *dev, $/;"	f
r8180_wx_set_crcmon	r8180_wx.c	/^static int r8180_wx_set_crcmon(struct net_device *dev, $/;"	f	file:
r8180_wx_set_enc	r8180_wx.c	/^static int r8180_wx_set_enc(struct net_device *dev, $/;"	f	file:
r8180_wx_set_enc_ext	r8180_wx.c	/^static int r8180_wx_set_enc_ext(struct net_device *dev,$/;"	f	file:
r8180_wx_set_essid	r8180_wx.c	/^static int r8180_wx_set_essid(struct net_device *dev, $/;"	f	file:
r8180_wx_set_frag	r8180_wx.c	/^static int r8180_wx_set_frag(struct net_device *dev, $/;"	f	file:
r8180_wx_set_freq	r8180_wx.c	/^static int r8180_wx_set_freq(struct net_device *dev, struct iw_request_info *a,$/;"	f	file:
r8180_wx_set_gen_ie	r8180_wx.c	/^static int r8180_wx_set_gen_ie(struct net_device *dev,$/;"	f	file:
r8180_wx_set_meshID	r8180_wx.c	/^static int r8180_wx_set_meshID(struct net_device *dev, $/;"	f	file:
r8180_wx_set_mlme	r8180_wx.c	/^static int r8180_wx_set_mlme(struct net_device *dev,$/;"	f	file:
r8180_wx_set_mode	r8180_wx.c	/^static int r8180_wx_set_mode(struct net_device *dev, struct iw_request_info *a,$/;"	f	file:
r8180_wx_set_radion	r8180_wx.c	/^static int r8180_wx_set_radion(struct net_device *dev, $/;"	f	file:
r8180_wx_set_ratadpt	r8180_wx.c	/^static int r8180_wx_set_ratadpt (struct net_device *dev, $/;"	f	file:
r8180_wx_set_rate	r8180_wx.c	/^static int r8180_wx_set_rate(struct net_device *dev, $/;"	f	file:
r8180_wx_set_rawtx	r8180_wx.c	/^static int r8180_wx_set_rawtx(struct net_device *dev, $/;"	f	file:
r8180_wx_set_retry	r8180_wx.c	/^static int r8180_wx_set_retry(struct net_device *dev, $/;"	f	file:
r8180_wx_set_scan	r8180_wx.c	/^static int r8180_wx_set_scan(struct net_device *dev, struct iw_request_info *a,$/;"	f	file:
r8180_wx_set_scan_type	r8180_wx.c	/^static int r8180_wx_set_scan_type(struct net_device *dev, struct iw_request_info *aa, union$/;"	f	file:
r8180_wx_set_sens	r8180_wx.c	/^static int r8180_wx_set_sens(struct net_device *dev, $/;"	f	file:
r8180_wx_set_wap	r8180_wx.c	/^static int r8180_wx_set_wap(struct net_device *dev,$/;"	f	file:
r8180_wx_write_bb	r8180_wx.c	/^static int r8180_wx_write_bb(struct net_device *dev,$/;"	f	file:
r8180_wx_write_nicb	r8180_wx.c	/^static int r8180_wx_write_nicb(struct net_device *dev,$/;"	f	file:
r8180_wx_write_regs	r8180_wx.c	/^static int r8180_wx_write_regs(struct net_device *dev, $/;"	f	file:
r8187-objs	Makefile	/^r8187-objs := r8187_core.o r8180_93cx6.o r8180_wx.o r8180_rtl8225.o r8180_rtl8225z2.o r8180_pm.o r8180_dm.o r8187_led.o$/;"	m
radion	r8187.h	/^	u8			radion;$/;"	m	struct:r8180_priv
rate	ieee80211.h	/^	int rate;       \/* current rate *\/$/;"	m	struct:ieee80211_device
rate	ieee80211.h	/^	u16 rate; \/* in 100 kbps *\/$/;"	m	struct:ieee80211_rx_stats
rate_adapter_wq	ieee80211.h	/^                struct delayed_work rate_adapter_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::delayed_work
rate_adapter_wq	ieee80211.h	/^                struct work_struct rate_adapter_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::work_struct
rateadapter_timer	r8187.h	/^    struct timer_list rateadapter_timer;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::timer_list
ratefallback	r8187_core.c	/^unsigned short	ratefallback:5;$/;"	m	struct:tx_desc	file:
rates	ieee80211.h	/^	u8 rates[MAX_RATES_LENGTH];$/;"	m	struct:ieee80211_network
rates_ex	ieee80211.h	/^	u8 rates_ex[MAX_RATES_EX_LENGTH];$/;"	m	struct:ieee80211_network
rates_ex_len	ieee80211.h	/^	u8 rates_ex_len;$/;"	m	struct:ieee80211_network
rates_len	ieee80211.h	/^	u8 rates_len;$/;"	m	struct:ieee80211_network
raw_tx	ieee80211.h	/^	short raw_tx;$/;"	m	struct:ieee80211_device
read_cam	r8187_core.c	/^u32 read_cam(struct net_device *dev, u8 addr)$/;"	f
read_nic_byte	r8187_core.c	/^u8 read_nic_byte(struct net_device *dev, int indx)$/;"	f
read_nic_byte_E	r8187_core.c	/^u8 read_nic_byte_E(struct net_device *dev, int indx)$/;"	f
read_nic_dword	r8187_core.c	/^u32 read_nic_dword(struct net_device *dev, int indx)$/;"	f
read_nic_word	r8187_core.c	/^u16 read_nic_word(struct net_device *dev, int indx)$/;"	f
read_phy_cck	r8187_core.c	/^u8 read_phy_cck(struct net_device *dev, u8 adr)$/;"	f
read_phy_ofdm	r8187_core.c	/^u8 read_phy_ofdm(struct net_device *dev, u8 adr)$/;"	f
read_rtl8225	r8180_rtl8225z2.c	/^u32 read_rtl8225(struct net_device *dev, u8 adr)$/;"	f
reason_code	ieee80211.h	/^    			int reason_code;$/;"	m	struct:ieee_param::__anon2::__anon5
reason_code	r8187_core.c	/^                        u32 reason_code;$/;"	m	struct:ipw_param::__anon8::__anon11	file:
reassoc	ieee80211.h	/^	unsigned int reassoc;$/;"	m	struct:ieee80211_softmac_stats
received_channel	ieee80211.h	/^	u8 received_channel;$/;"	m	struct:ieee80211_rx_stats
refcnt	ieee80211_crypt.h	/^	atomic_t refcnt;$/;"	m	struct:ieee80211_crypt_data
res	r8187_core.c	/^unsigned int	res:1;$/;"	m	struct:rx_desc_rtl8187b	file:
res	r8187_core.c	/^unsigned int    res:1;$/;"	m	struct:rx_desc_rtl8187	file:
reserved	ieee80211.h	/^			u8 reserved[32];$/;"	m	struct:ieee_param::__anon2::__anon4
reserved	ieee80211.h	/^	u16 reserved;$/;"	m	struct:ieee80211_txb
reserved	ieee80211.h	/^	u8 reserved;$/;"	m	struct:ieee80211_wmm_ts_info
reserved	r8187_core.c	/^                        u8 reserved[32];$/;"	m	struct:ipw_param::__anon8::__anon10	file:
reset_on_keychange	ieee80211.h	/^	int reset_on_keychange; \/* Set to 1 if the HW needs to be reset on$/;"	m	struct:ieee80211_device
reset_port	ieee80211.h	/^	int (*reset_port)(struct net_device *dev);$/;"	m	struct:ieee80211_device
reset_wq	r8187.h	/^	struct tq_struct reset_wq;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::tq_struct
reset_wq	r8187.h	/^	struct work_struct reset_wq;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::work_struct
retry_data	r8187.h	/^	u8 retry_data;$/;"	m	struct:r8180_priv
retry_rts	r8187.h	/^	u8 retry_rts;$/;"	m	struct:r8180_priv
retrylimit	r8187_core.c	/^unsigned char	retrylimit;$/;"	m	struct:tx_desc	file:
rf_chip	r8187.h	/^	short rf_chip;$/;"	m	struct:r8180_priv
rf_close	r8187.h	/^	void (*rf_close)(struct net_device *dev);$/;"	m	struct:r8180_priv
rf_init	r8187.h	/^	void (*rf_init)(struct net_device *dev);$/;"	m	struct:r8180_priv
rf_ps_lock	r8187.h	/^	spinlock_t rf_ps_lock;$/;"	m	struct:r8180_priv
rf_set_chan	r8187.h	/^	void (*rf_set_chan)(struct net_device *dev,short ch);$/;"	m	struct:r8180_priv
rf_set_sens	r8187.h	/^	short (*rf_set_sens)(struct net_device *dev,short sens);$/;"	m	struct:r8180_priv
rsn_ie	ieee80211.h	/^	u8 rsn_ie[MAX_WPA_IE_LEN];$/;"	m	struct:ieee80211_network
rsn_ie_len	ieee80211.h	/^	size_t rsn_ie_len;$/;"	m	struct:ieee80211_network
rssi	ieee80211.h	/^	s8 rssi;$/;"	m	struct:ieee80211_rx_stats
rssi	r8187_core.c	/^unsigned char	rssi:7;$/;"	m	struct:rx_desc_rtl8187b	file:
rssi	r8187_core.c	/^unsigned char   rssi:7;$/;"	m	struct:rx_desc_rtl8187	file:
rsvd0	r8187_core.c	/^unsigned char	rsvd0:5;$/;"	m	struct:rx_desc_rtl8187b	file:
rsvd0	r8187_core.c	/^unsigned char   rsvd0:5;$/;"	m	struct:rx_desc_rtl8187	file:
rsvd0	r8187_core.c	/^unsigned int    rsvd0:3;$/;"	m	struct:tx_desc	file:
rsvd1	r8187_core.c	/^unsigned short  rsvd1:3;$/;"	m	struct:tx_desc	file:
rsvd2	r8187_core.c	/^unsigned short	rsvd2:4;$/;"	m	struct:tx_desc	file:
rsvd3	r8187_core.c	/^unsigned short	rsvd3:4;$/;"	m	struct:tx_desc	file:
rsvd4	r8187_core.c	/^unsigned short	rsvd4:1;$/;"	m	struct:tx_desc	file:
rsvd5	r8187_core.c	/^unsigned char	rsvd5:1;$/;"	m	struct:tx_desc	file:
rtdb	r8187_core.c	/^unsigned short	rtdb:1;$/;"	m	struct:tx_desc	file:
rtl8180_IsWirelessBMode	r8187_core.c	/^inline u8 rtl8180_IsWirelessBMode(u16 rate)$/;"	f
rtl8180_adapter_start	r8187_core.c	/^void rtl8180_adapter_start(struct net_device *dev)$/;"	f
rtl8180_close	r8187_core.c	/^int rtl8180_close(struct net_device *dev)$/;"	f
rtl8180_commit	r8187_core.c	/^void rtl8180_commit(struct net_device *dev)$/;"	f
rtl8180_data_hard_resume	r8187_core.c	/^void rtl8180_data_hard_resume(struct net_device *dev)$/;"	f
rtl8180_data_hard_stop	r8187_core.c	/^void rtl8180_data_hard_stop(struct net_device *dev)$/;"	f
rtl8180_down	r8187_core.c	/^int rtl8180_down(struct net_device *dev)$/;"	f
rtl8180_dump_reg	r8187_core.c	/^void rtl8180_dump_reg(struct net_device *dev)$/;"	f
rtl8180_enable_wake	r8180_pm.c	/^int rtl8180_enable_wake (struct pci_dev *dev, u32 state, int enable)$/;"	f
rtl8180_hard_data_xmit	r8187_core.c	/^void rtl8180_hard_data_xmit(struct sk_buff *skb, struct net_device *dev, int rate)$/;"	f
rtl8180_hard_start_xmit	r8187_core.c	/^int rtl8180_hard_start_xmit(struct sk_buff *skb,struct net_device *dev)$/;"	f
rtl8180_hw_dig_wq	r8180_dm.c	/^void rtl8180_hw_dig_wq (struct work_struct *work)$/;"	f
rtl8180_init	r8187_core.c	/^short rtl8180_init(struct net_device *dev)$/;"	f
rtl8180_ioctl	r8187_core.c	/^int rtl8180_ioctl(struct net_device *dev, struct ifreq *rq, int cmd)$/;"	f
rtl8180_irq_disable	r8187_core.c	/^void rtl8180_irq_disable(struct net_device *dev)$/;"	f
rtl8180_irq_enable	r8187_core.c	/^void rtl8180_irq_enable(struct net_device *dev)$/;"	f
rtl8180_irq_rx_tasklet	r8187_core.c	/^void rtl8180_irq_rx_tasklet(struct r8180_priv *priv)$/;"	f
rtl8180_irq_rx_tasklet_new	r8187_core.c	/^void rtl8180_irq_rx_tasklet_new(struct r8180_priv *priv){$/;"	f
rtl8180_link_detect_init	r8187_core.c	/^static void rtl8180_link_detect_init(plink_detect_t plink_detect)$/;"	f	file:
rtl8180_open	r8187_core.c	/^int rtl8180_open(struct net_device *dev)$/;"	f
rtl8180_proc	r8187_core.c	/^static struct proc_dir_entry *rtl8180_proc = NULL;$/;"	v	typeref:struct:proc_dir_entry	file:
rtl8180_proc_init_one	r8187_core.c	/^void rtl8180_proc_init_one(struct net_device *dev)$/;"	f
rtl8180_proc_module_init	r8187_core.c	/^void rtl8180_proc_module_init(void)$/;"	f
rtl8180_proc_module_remove	r8187_core.c	/^void rtl8180_proc_module_remove(void)$/;"	f
rtl8180_proc_remove_one	r8187_core.c	/^void rtl8180_proc_remove_one(struct net_device *dev)$/;"	f
rtl8180_rate2rate	r8187_core.c	/^inline u16 rtl8180_rate2rate(short rate)$/;"	f
rtl8180_rate_adapter	r8187_core.c	/^void rtl8180_rate_adapter(struct work_struct * work)$/;"	f
rtl8180_rates	r8180_wx.c	/^u32 rtl8180_rates[] = {1000000,2000000,5500000,11000000,$/;"	v
rtl8180_reset	r8187_core.c	/^void rtl8180_reset(struct net_device *dev)$/;"	f
rtl8180_restart	r8187_core.c	/^void rtl8180_restart(struct work_struct *work)$/;"	f
rtl8180_rtx_disable	r8187_core.c	/^void rtl8180_rtx_disable(struct net_device *dev)$/;"	f
rtl8180_rx_enable	r8187_core.c	/^void rtl8180_rx_enable(struct net_device *dev)$/;"	f
rtl8180_save_state	r8180_pm.c	/^int rtl8180_save_state (struct pci_dev *dev, u32 state)$/;"	f
rtl8180_set_anaparam	r8187_core.c	/^void rtl8180_set_anaparam(struct net_device *dev, u32 a)$/;"	f
rtl8180_set_chan	r8187_core.c	/^void rtl8180_set_chan(struct net_device *dev,short ch)$/;"	f
rtl8180_set_mode	r8187_core.c	/^void rtl8180_set_mode(struct net_device *dev,int mode)$/;"	f
rtl8180_stats	r8187_core.c	/^static struct net_device_stats *rtl8180_stats(struct net_device *dev)$/;"	f	file:
rtl8180_try_wake_queue	r8187_core.c	/^void rtl8180_try_wake_queue(struct net_device *dev, int pri)$/;"	f
rtl8180_tx	r8187_core.c	/^short rtl8180_tx(struct net_device *dev, u32* txbuf, int len, priority_t priority,$/;"	f
rtl8180_tx_enable	r8187_core.c	/^void rtl8180_tx_enable(struct net_device *dev)$/;"	f
rtl8180_tx_pw_wq	r8180_dm.c	/^void rtl8180_tx_pw_wq (struct work_struct *work)$/;"	f
rtl8180_up	r8187_core.c	/^int rtl8180_up(struct net_device *dev)$/;"	f
rtl8180_update_msr	r8187_core.c	/^void rtl8180_update_msr(struct net_device *dev)$/;"	f
rtl8180_watch_dog_wq	r8187_core.c	/^void rtl8180_watch_dog_wq (struct work_struct *work)$/;"	f
rtl8180_wmm_param_update	r8187_core.c	/^void rtl8180_wmm_param_update(struct work_struct* work)$/;"	f
rtl8180_wx_get_range	r8180_wx.c	/^static int rtl8180_wx_get_range(struct net_device *dev, $/;"	f	file:
rtl8185_rf_pins_enable	r8187_core.c	/^void rtl8185_rf_pins_enable(struct net_device *dev)$/;"	f
rtl8185_set_anaparam2	r8187_core.c	/^void rtl8185_set_anaparam2(struct net_device *dev, u32 a)$/;"	f
rtl8185_tx_antenna	r8187_core.c	/^void rtl8185_tx_antenna(struct net_device *dev, u8 ant)$/;"	f
rtl8187_beacon_stop	r8187_core.c	/^void rtl8187_beacon_stop(struct net_device *dev)$/;"	f
rtl8187_beacon_tx	r8187_core.c	/^void rtl8187_beacon_tx(struct net_device *dev)$/;"	f
rtl8187_beacontx_isr	r8187_core.c	/^void rtl8187_beacontx_isr(struct urb *tx_urb, struct pt_regs *regs)$/;"	f
rtl8187_betx_isr	r8187_core.c	/^void rtl8187_betx_isr(struct urb *tx_urb, struct pt_regs *regs)$/;"	f
rtl8187_bktx_isr	r8187_core.c	/^void rtl8187_bktx_isr(struct urb *tx_urb, struct pt_regs *regs)$/;"	f
rtl8187_link_change	r8187_core.c	/^void rtl8187_link_change(struct net_device *dev)$/;"	f
rtl8187_lptx_isr	r8187_core.c	/^void rtl8187_lptx_isr(struct urb *tx_urb, struct pt_regs *regs)$/;"	f
rtl8187_managetx_isr	r8187_core.c	/^void rtl8187_managetx_isr(struct urb *tx_urb, struct pt_regs *regs)$/;"	f
rtl8187_net_update	r8187_core.c	/^void rtl8187_net_update(struct net_device *dev)$/;"	f
rtl8187_nptx_isr	r8187_core.c	/^void rtl8187_nptx_isr(struct urb *tx_urb, struct pt_regs *regs)$/;"	f
rtl8187_read_phy	r8187_core.c	/^u8 rtl8187_read_phy(struct net_device *dev,u8 adr, u32 data)$/;"	f
rtl8187_resume	r8180_pm.c	/^int rtl8187_resume (struct usb_interface *intf)$/;"	f
rtl8187_rx_initiate	r8187_core.c	/^void rtl8187_rx_initiate(struct net_device *dev)$/;"	f
rtl8187_rx_isr	r8187_core.c	/^void rtl8187_rx_isr(struct urb *rx_urb, struct pt_regs *regs)$/;"	f
rtl8187_rx_manage_initiate	r8187_core.c	/^void rtl8187_rx_manage_initiate(struct net_device *dev)$/;"	f
rtl8187_rx_manage_isr	r8187_core.c	/^void rtl8187_rx_manage_isr(struct urb *rx_urb, struct pt_regs *regs)$/;"	f
rtl8187_rx_manage_urbsubmit	r8187_core.c	/^void rtl8187_rx_manage_urbsubmit(struct net_device *dev, struct urb* rx_urb)$/;"	f
rtl8187_rx_urbsubmit	r8187_core.c	/^void rtl8187_rx_urbsubmit(struct net_device *dev, struct urb* rx_urb)$/;"	f
rtl8187_set_rate	r8187_core.c	/^void rtl8187_set_rate(struct net_device *dev)$/;"	f
rtl8187_set_rxconf	r8187_core.c	/^void rtl8187_set_rxconf(struct net_device *dev)$/;"	f
rtl8187_suspend	r8180_pm.c	/^int rtl8187_suspend (struct usb_interface *intf,$/;"	f
rtl8187_usb_deleteendpoints	r8187_core.c	/^void rtl8187_usb_deleteendpoints(struct net_device *dev)$/;"	f
rtl8187_usb_disconnect	r8187_core.c	/^static void __devexit rtl8187_usb_disconnect(struct usb_interface *intf)$/;"	f	file:
rtl8187_usb_driver	r8187_core.c	/^static struct usb_driver rtl8187_usb_driver = {$/;"	v	typeref:struct:usb_driver	file:
rtl8187_usb_id_tbl	r8187_core.c	/^static struct usb_device_id rtl8187_usb_id_tbl[] = {$/;"	v	typeref:struct:usb_device_id	file:
rtl8187_usb_initendpoints	r8187_core.c	/^short rtl8187_usb_initendpoints(struct net_device *dev)$/;"	f
rtl8187_usb_module_exit	r8187_core.c	/^module_exit(rtl8187_usb_module_exit);$/;"	v
rtl8187_usb_module_exit	r8187_core.c	/^static void __exit rtl8187_usb_module_exit(void)$/;"	f	file:
rtl8187_usb_module_init	r8187_core.c	/^module_init(rtl8187_usb_module_init);$/;"	v
rtl8187_usb_module_init	r8187_core.c	/^static int __init rtl8187_usb_module_init(void)$/;"	f	file:
rtl8187_usb_probe	r8187_core.c	/^static int __devinit rtl8187_usb_probe(struct usb_interface *intf,$/;"	f	file:
rtl8187_vitx_isr	r8187_core.c	/^void rtl8187_vitx_isr(struct urb *tx_urb, struct pt_regs *regs)$/;"	f
rtl8187_votx_isr	r8187_core.c	/^void rtl8187_votx_isr(struct urb *tx_urb, struct pt_regs *regs)$/;"	f
rtl8187_write_phy	r8187_core.c	/^void rtl8187_write_phy(struct net_device *dev, u8 adr, u32 data)$/;"	f
rtl8225_SetTXPowerLevel	r8180_rtl8225.c	/^void rtl8225_SetTXPowerLevel(struct net_device *dev, short ch)$/;"	f
rtl8225_agc	r8180_rtl8225.c	/^u8 rtl8225_agc[]={$/;"	v
rtl8225_chan	r8180_rtl8225.c	/^u32 rtl8225_chan[] = {$/;"	v
rtl8225_gain	r8180_rtl8225.c	/^u8 rtl8225_gain[]={$/;"	v
rtl8225_host_pci_init	r8180_rtl8225.c	/^void rtl8225_host_pci_init(struct net_device *dev) $/;"	f
rtl8225_host_usb_init	r8180_rtl8225.c	/^void rtl8225_host_usb_init(struct net_device *dev) $/;"	f
rtl8225_is_V_z2	r8180_rtl8225z2.c	/^short rtl8225_is_V_z2(struct net_device *dev)$/;"	f
rtl8225_rf_close	r8180_rtl8225.c	/^void rtl8225_rf_close(struct net_device *dev)$/;"	f
rtl8225_rf_init	r8180_rtl8225.c	/^void rtl8225_rf_init(struct net_device *dev) $/;"	f
rtl8225_rf_set_chan	r8180_rtl8225.c	/^void rtl8225_rf_set_chan(struct net_device *dev, short ch)$/;"	f
rtl8225_rf_set_sens	r8180_rtl8225.c	/^short rtl8225_rf_set_sens(struct net_device *dev, short sens)$/;"	f
rtl8225_set_gain	r8180_rtl8225.c	/^void rtl8225_set_gain(struct net_device *dev, short gain)$/;"	f
rtl8225_threshold	r8180_rtl8225.c	/^u8 rtl8225_threshold[]={$/;"	v
rtl8225_tx_gain_cck_ofdm	r8180_rtl8225.c	/^u8 rtl8225_tx_gain_cck_ofdm[]={$/;"	v
rtl8225_tx_power_cck	r8180_rtl8225.c	/^u8 rtl8225_tx_power_cck[]={$/;"	v
rtl8225_tx_power_cck_ch14	r8180_rtl8225.c	/^u8 rtl8225_tx_power_cck_ch14[]={$/;"	v
rtl8225_tx_power_ofdm	r8180_rtl8225.c	/^u8 rtl8225_tx_power_ofdm[]={$/;"	v
rtl8225bcd_rxgain	r8180_rtl8225.c	/^u16 rtl8225bcd_rxgain[]={	$/;"	v
rtl8225z2_SetTXPowerLevel	r8180_rtl8225z2.c	/^void rtl8225z2_SetTXPowerLevel(struct net_device *dev, short ch)$/;"	f
rtl8225z2_gain_a	r8180_rtl8225z2.c	/^u8 rtl8225z2_gain_a[]={$/;"	v
rtl8225z2_gain_bg	r8180_rtl8225z2.c	/^u8 rtl8225z2_gain_bg[]={$/;"	v
rtl8225z2_rf_init	r8180_rtl8225z2.c	/^void rtl8225z2_rf_init(struct net_device *dev) $/;"	f
rtl8225z2_rf_set_chan	r8180_rtl8225z2.c	/^void rtl8225z2_rf_set_chan(struct net_device *dev, short ch)$/;"	f
rtl8225z2_rf_set_mode	r8180_rtl8225z2.c	/^void rtl8225z2_rf_set_mode(struct net_device *dev) $/;"	f
rtl8225z2_rxgain	r8180_rtl8225z2.c	/^u16 rtl8225z2_rxgain[]={	$/;"	v
rtl8225z2_set_gain	r8180_rtl8225z2.c	/^void rtl8225z2_set_gain(struct net_device *dev, short gain)$/;"	f
rtl8225z2_threshold	r8180_rtl8225z2.c	/^u8 rtl8225z2_threshold[]={$/;"	v
rtl8225z2_tx_power_cck	r8180_rtl8225z2.c	/^u8 rtl8225z2_tx_power_cck[]={$/;"	v
rtl8225z2_tx_power_cck_ch14	r8180_rtl8225z2.c	/^u8 rtl8225z2_tx_power_cck_ch14[]={$/;"	v
rtl8225z2_tx_power_ofdm	r8180_rtl8225z2.c	/^u8 rtl8225z2_tx_power_ofdm[]={$/;"	v
rtl_rate	r8187_core.c	/^static u16 rtl_rate[] = {10,20,55,110,60,90,120,180,240,360,480,540,720};$/;"	v	file:
rtl_reg_debug	r8187.h	/^typedef struct rtl_reg_debug{$/;"	s
rtl_reg_debug	r8187.h	/^}rtl_reg_debug;$/;"	t	typeref:struct:rtl_reg_debug
rts	r8187.h	/^	u16 rts;$/;"	m	struct:r8180_priv
rtsagc	r8187_core.c	/^unsigned char	rtsagc;$/;"	m	struct:tx_desc	file:
rtsdur	r8187_core.c	/^unsigned short  rtsdur;$/;"	m	struct:tx_desc	file:
rtsen	r8187_core.c	/^unsigned int    rtsen:1;$/;"	m	struct:tx_desc	file:
rtsrate	r8187_core.c	/^unsigned int    rtsrate:4;$/;"	m	struct:tx_desc	file:
rtsratefallback	r8187_core.c	/^unsigned short	rtsratefallback:4;$/;"	m	struct:tx_desc	file:
rx_ass_err	ieee80211.h	/^	unsigned int rx_ass_err;$/;"	m	struct:ieee80211_softmac_stats
rx_ass_ok	ieee80211.h	/^	unsigned int rx_ass_ok;$/;"	m	struct:ieee80211_softmac_stats
rx_ass_rq	ieee80211.h	/^	unsigned int rx_ass_rq;$/;"	m	struct:ieee80211_softmac_stats
rx_auth_rq	ieee80211.h	/^	unsigned int rx_auth_rq;$/;"	m	struct:ieee80211_softmac_stats
rx_auth_rs_err	ieee80211.h	/^	unsigned int rx_auth_rs_err;$/;"	m	struct:ieee80211_softmac_stats
rx_auth_rs_ok	ieee80211.h	/^	unsigned int rx_auth_rs_ok;$/;"	m	struct:ieee80211_softmac_stats
rx_desc	r8187_core.c	/^union rx_desc {$/;"	u	file:
rx_desc_rtl8187	r8187_core.c	/^struct rx_desc_rtl8187 {$/;"	s	file:
rx_desc_rtl8187b	r8187_core.c	/^struct rx_desc_rtl8187b {$/;"	s	file:
rx_discards_no_buffer	ieee80211.h	/^	unsigned int rx_discards_no_buffer;$/;"	m	struct:ieee80211_stats
rx_discards_undecryptable	ieee80211.h	/^	unsigned int rx_discards_undecryptable;$/;"	m	struct:ieee80211_stats
rx_fcs_errors	ieee80211.h	/^	unsigned int rx_fcs_errors;$/;"	m	struct:ieee80211_stats
rx_fragments	ieee80211.h	/^	unsigned int rx_fragments;$/;"	m	struct:ieee80211_stats
rx_inx	r8187.h	/^        int     rx_inx;$/;"	m	struct:r8180_priv
rx_message_in_bad_msg_fragments	ieee80211.h	/^	unsigned int rx_message_in_bad_msg_fragments;$/;"	m	struct:ieee80211_stats
rx_message_in_msg_fragments	ieee80211.h	/^	unsigned int rx_message_in_msg_fragments;$/;"	m	struct:ieee80211_stats
rx_multicast_frames	ieee80211.h	/^	unsigned int rx_multicast_frames;$/;"	m	struct:ieee80211_stats
rx_multicast_octets	ieee80211.h	/^	unsigned int rx_multicast_octets;$/;"	m	struct:ieee80211_stats
rx_probe_rq	ieee80211.h	/^	unsigned int rx_probe_rq;$/;"	m	struct:ieee80211_softmac_stats
rx_unicast_frames	ieee80211.h	/^	unsigned int rx_unicast_frames;$/;"	m	struct:ieee80211_stats
rx_unicast_octets	ieee80211.h	/^	unsigned int rx_unicast_octets;$/;"	m	struct:ieee80211_stats
rx_urb	r8187.h	/^	struct urb **rx_urb;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::urb
rxlen	r8187_core.c	/^unsigned int	rxlen:12;$/;"	m	struct:rx_desc_rtl8187b	file:
rxlen	r8187_core.c	/^unsigned int    rxlen:12;$/;"	m	struct:rx_desc_rtl8187	file:
rxlen	r8187_core.c	/^unsigned short	rxlen:12;$/;"	m	struct:tx_desc	file:
rxok	r8187.h	/^	unsigned long rxok;$/;"	m	struct:Stats
rxrate	r8187_core.c	/^unsigned int	rxrate:4;$/;"	m	struct:rx_desc_rtl8187b	file:
rxrate	r8187_core.c	/^unsigned int    rxrate:4;$/;"	m	struct:rx_desc_rtl8187	file:
rxstaterr	r8187.h	/^	unsigned long rxstaterr;$/;"	m	struct:Stats
rxurb_task	r8187.h	/^	struct urb *rxurb_task;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::urb
rxurberr	r8187.h	/^	unsigned long rxurberr;$/;"	m	struct:Stats
sAckCtsLng	r8187_core.c	2594;"	d	file:
sCrcLng	r8187_core.c	2593;"	d	file:
scan_age	ieee80211.h	/^	int scan_age;$/;"	m	struct:ieee80211_device
scan_sem	ieee80211.h	/^	struct semaphore scan_sem;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::semaphore
scan_syncro	ieee80211.h	/^	void (*scan_syncro)(struct net_device *dev);$/;"	m	struct:ieee80211_device
scan_timer	ieee80211.h	/^	struct timer_list scan_timer;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::timer_list
scanning	ieee80211.h	/^	short scanning;$/;"	m	struct:ieee80211_device
scans	ieee80211.h	/^	int scans;$/;"	m	struct:ieee80211_device
sens	r8187.h	/^	short sens;$/;"	m	struct:r8180_priv
seq	ieee80211.h	/^			u8 seq[8]; \/* sequence counter (set: RX, get: TX) *\/$/;"	m	struct:ieee_param::__anon2::__anon6
seq	ieee80211.h	/^	unsigned int seq;$/;"	m	struct:ieee80211_frag_entry
seq	r8187_core.c	/^                        u8 seq[8];$/;"	m	struct:ipw_param::__anon8::__anon12	file:
seq_ctl	ieee80211.h	/^	u16 seq_ctl;$/;"	m	struct:ieee80211_hdr
seq_ctl	ieee80211.h	/^	u16 seq_ctl;$/;"	m	struct:ieee80211_hdr_3addr
seq_ctl	ieee80211.h	/^	u16 seq_ctl;$/;"	m	struct:ieee80211_hdr_3addr_QOS
seq_ctl	ieee80211.h	/^	u16 seq_ctl;$/;"	m	struct:ieee80211_hdr_QOS
seq_ctrl	ieee80211.h	/^	u16 seq_ctrl;$/;"	m	struct:ieee80211_header_data
seq_ctrl	ieee80211.h	/^	u16 seq_ctrl[5];$/;"	m	struct:ieee80211_device
seq_num	ieee80211.h	/^	u16 seq_num;$/;"	m	struct:ieee_mesh_seq
seq_num	ieee80211.h	/^	u16 seq_num[17];$/;"	m	struct:ieee_ibss_seq
serv_start_time	ieee80211.h	/^	u32 serv_start_time;$/;"	m	struct:ieee80211_wmm_tspec_elem
setKey	r8187_core.c	/^void setKey(	struct net_device *dev, $/;"	f
set_chan	ieee80211.h	/^	void (*set_chan)(struct net_device *dev,short ch);$/;"	m	struct:ieee80211_device
set_key	ieee80211_crypt.h	/^	int (*set_key)(void *key, int len, u8 *seq, void *priv);$/;"	m	struct:ieee80211_crypto_ops
set_security	ieee80211.h	/^	void (*set_security)(struct net_device *dev,$/;"	m	struct:ieee80211_device
set_tx	ieee80211.h	/^			u8 set_tx;$/;"	m	struct:ieee_param::__anon2::__anon6
set_tx	r8187_core.c	/^                        u8 set_tx;$/;"	m	struct:ipw_param::__anon8::__anon12	file:
shift	r8187_core.c	/^unsigned char	shift:1;$/;"	m	struct:rx_desc_rtl8187b	file:
shift	r8187_core.c	/^unsigned char   shift:1;$/;"	m	struct:rx_desc_rtl8187	file:
short_slot	ieee80211.h	/^	int short_slot;$/;"	m	struct:ieee80211_device
signal	ieee80211.h	/^	u8 signal;$/;"	m	struct:ieee80211_rx_stats
signalstrength	ieee80211.h	/^	u8 signalstrength;$/;"	m	struct:ieee80211_rx_stats
skb	ieee80211.h	/^	struct sk_buff *skb;$/;"	m	struct:ieee80211_frag_entry	typeref:struct:ieee80211_frag_entry::sk_buff
snap	ieee80211.h	/^	u8 snap[6];$/;"	m	struct:eapol
snr_long2end	r8187_core.c	/^unsigned int	snr_long2end:6;$/;"	m	struct:rx_desc_rtl8187b	file:
softmac_data_hard_start_xmit	ieee80211.h	/^	void (*softmac_data_hard_start_xmit)(struct sk_buff *skb,$/;"	m	struct:ieee80211_device
softmac_features	ieee80211.h	/^	u16 softmac_features;$/;"	m	struct:ieee80211_device
softmac_hard_start_xmit	ieee80211.h	/^	int (*softmac_hard_start_xmit)(struct sk_buff *skb,$/;"	m	struct:ieee80211_device
softmac_scan_wq	ieee80211.h	/^	struct tq_struct softmac_scan_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::tq_struct
softmac_scan_wq	ieee80211.h	/^        struct delayed_work softmac_scan_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::delayed_work
softmac_scan_wq	ieee80211.h	/^        struct work_struct softmac_scan_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::work_struct
softmac_stats	ieee80211.h	/^	struct ieee80211_softmac_stats softmac_stats;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::ieee80211_softmac_stats
spc	r8187_core.c	/^unsigned short	spc:2;$/;"	m	struct:tx_desc	file:
splcp	r8187_core.c	/^unsigned int	splcp:1;$/;"	m	struct:rx_desc_rtl8187b	file:
splcp	r8187_core.c	/^unsigned int    splcp:1;$/;"	m	struct:rx_desc_rtl8187	file:
splcp	r8187_core.c	/^unsigned int    splcp:1;$/;"	m	struct:tx_desc	file:
sq	r8187_core.c	/^unsigned char	sq;$/;"	m	struct:rx_desc_rtl8187b	file:
sq	r8187_core.c	/^unsigned char   sq;$/;"	m	struct:rx_desc_rtl8187	file:
src_addr	ieee80211.h	/^	u8 src_addr[ETH_ALEN];$/;"	m	struct:ieee80211_frag_entry
ssap	ieee80211.h	/^        u8    ssap;   \/* always 0xAA *\/$/;"	m	struct:ieee80211_snap_hdr
ssid	ieee80211.h	/^	u8 ssid[IW_ESSID_MAX_SIZE + 1];$/;"	m	struct:ieee80211_network
ssid_len	ieee80211.h	/^	u8 ssid_len;$/;"	m	struct:ieee80211_network
ssid_set	ieee80211.h	/^	short ssid_set;$/;"	m	struct:ieee80211_device
ssid_thread	r8187.h	/^struct ssid_thread {$/;"	s
sta_addr	ieee80211.h	/^	u8 sta_addr[ETH_ALEN];$/;"	m	struct:ieee_param
sta_addr	r8187_core.c	/^        u8 sta_addr[ETH_ALEN];$/;"	m	struct:ipw_param	file:
sta_rateadaptive8187B	r8187_core.c	/^sta_rateadaptive8187B($/;"	f
sta_sleep	ieee80211.h	/^	short sta_sleep;$/;"	m	struct:ieee80211_device
sta_wake_up	ieee80211.h	/^	void (*sta_wake_up) (struct net_device *dev);$/;"	m	struct:ieee80211_device
start_ibss_wq	ieee80211.h	/^	struct delayed_work start_ibss_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::delayed_work
start_ibss_wq	ieee80211.h	/^	struct tq_struct start_ibss_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::tq_struct
start_ibss_wq	ieee80211.h	/^	struct work_struct start_ibss_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::work_struct
start_scan	ieee80211.h	/^	void (*start_scan)(struct net_device *dev);$/;"	m	struct:ieee80211_device
start_send_beacons	ieee80211.h	/^	void (*start_send_beacons) (struct net_device *dev);$/;"	m	struct:ieee80211_device
state	ieee80211.h	/^	enum ieee80211_state state;$/;"	m	struct:ieee80211_device	typeref:enum:ieee80211_device::ieee80211_state
stats	ieee80211.h	/^	struct ieee80211_rx_stats stats;$/;"	m	struct:ieee80211_network	typeref:struct:ieee80211_network::ieee80211_rx_stats
stats	ieee80211.h	/^	struct net_device_stats stats;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::net_device_stats
stats	r8187.h	/^	struct Stats stats;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::Stats
status	ieee80211.h	/^	u16 status;$/;"	m	struct:ieee80211_assoc_response_frame
status	ieee80211.h	/^	u16 status;$/;"	m	struct:ieee80211_authentication
stop_scan	ieee80211.h	/^	void (*stop_scan)(struct net_device *dev);$/;"	m	struct:ieee80211_device
stop_send_beacons	ieee80211.h	/^	void (*stop_send_beacons) (struct net_device *dev);$/;"	m	struct:ieee80211_device
surp_band_allow	ieee80211.h	/^	u16 surp_band_allow;$/;"	m	struct:ieee80211_wmm_tspec_elem
suspen_inter	ieee80211.h	/^	u32 suspen_inter;$/;"	m	struct:ieee80211_wmm_tspec_elem
swtxawake	ieee80211.h	/^	unsigned int swtxawake;$/;"	m	struct:ieee80211_softmac_stats
swtxstop	ieee80211.h	/^	unsigned int swtxstop;$/;"	m	struct:ieee80211_softmac_stats
sync_scan_hurryup	ieee80211.h	/^	short sync_scan_hurryup; $/;"	m	struct:ieee80211_device
time_stamp	ieee80211.h	/^	u32 time_stamp[2];$/;"	m	struct:ieee80211_network
time_stamp	ieee80211.h	/^	u32 time_stamp[2];$/;"	m	struct:ieee80211_probe_response
timer_rate_adaptive	r8187_core.c	/^void timer_rate_adaptive(unsigned long data)$/;"	f
tkip_countermeasures	ieee80211.h	/^	int tkip_countermeasures;$/;"	m	struct:ieee80211_device
tpcdesen	r8187_core.c	/^unsigned char	tpcdesen:1;$/;"	m	struct:tx_desc	file:
tpcen	r8187_core.c	/^unsigned char	tpcen:1;$/;"	m	struct:tx_desc	file:
tpcpolarity	r8187_core.c	/^unsigned char	tpcpolarity:2;$/;"	m	struct:tx_desc	file:
tpktsize	r8187_core.c	/^unsigned int    tpktsize:12;$/;"	m	struct:tx_desc	file:
tq_init	ieee80211.h	/^static inline void tq_init(struct tq_struct * task, void(*func)(void *), void *data)$/;"	f
transaction	ieee80211.h	/^	u16 transaction;$/;"	m	struct:ieee80211_authentication
trsw	r8187_core.c	/^unsigned int	trsw:1;$/;"	m	struct:rx_desc_rtl8187b	file:
trsw	r8187_core.c	/^unsigned int    trsw:1;$/;"	m	struct:rx_desc_rtl8187	file:
true	ieee80211.h	/^typedef enum{false = 0, true} bool;$/;"	e	enum:__anon1
ts_info	ieee80211.h	/^	struct ieee80211_wmm_ts_info ts_info;$/;"	m	struct:ieee80211_wmm_tspec_elem	typeref:struct:ieee80211_wmm_tspec_elem::ieee80211_wmm_ts_info
tsfth	r8187_core.c	/^unsigned int	tsfth;$/;"	m	struct:rx_desc_rtl8187b	file:
tsfth	r8187_core.c	/^unsigned int tsfth;$/;"	m	struct:rx_desc_rtl8187	file:
tsftl	r8187_core.c	/^unsigned int	tsftl;$/;"	m	struct:rx_desc_rtl8187b	file:
tsftl	r8187_core.c	/^unsigned int tsftl;$/;"	m	struct:rx_desc_rtl8187	file:
tx_ass_rq	ieee80211.h	/^	unsigned int tx_ass_rq;$/;"	m	struct:ieee80211_softmac_stats
tx_auth_rq	ieee80211.h	/^	unsigned int tx_auth_rq;$/;"	m	struct:ieee80211_softmac_stats
tx_beacons	ieee80211.h	/^	unsigned int tx_beacons;$/;"	m	struct:ieee80211_softmac_stats
tx_deferred_transmissions	ieee80211.h	/^	unsigned int tx_deferred_transmissions;$/;"	m	struct:ieee80211_stats
tx_desc	r8187_core.c	/^struct tx_desc {$/;"	s	file:
tx_discards	ieee80211.h	/^	unsigned int tx_discards;$/;"	m	struct:ieee80211_stats
tx_discards_wrong_sa	ieee80211.h	/^	unsigned int tx_discards_wrong_sa;$/;"	m	struct:ieee80211_stats
tx_fragments	ieee80211.h	/^	unsigned int tx_fragments;$/;"	m	struct:ieee80211_stats
tx_headroom	ieee80211.h	/^	int tx_headroom; \/* Set to size of any additional room needed at front$/;"	m	struct:ieee80211_device
tx_keyidx	ieee80211.h	/^	int tx_keyidx; \/* default TX key index (crypt[tx_keyidx]) *\/$/;"	m	struct:ieee80211_device
tx_lock	r8187.h	/^	spinlock_t tx_lock;$/;"	m	struct:r8180_priv
tx_multicast_frames	ieee80211.h	/^	unsigned int tx_multicast_frames;$/;"	m	struct:ieee80211_stats
tx_multicast_octets	ieee80211.h	/^	unsigned int tx_multicast_octets;$/;"	m	struct:ieee80211_stats
tx_multiple_retry_frames	ieee80211.h	/^	unsigned int tx_multiple_retry_frames;$/;"	m	struct:ieee80211_stats
tx_pending	ieee80211.h	/^	struct  tx_pending_t tx_pending;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::tx_pending_t
tx_pending	r8187.h	/^	atomic_t tx_pending[0x10];\/\/UART_PRIORITY+1$/;"	m	struct:r8180_priv
tx_pending_t	ieee80211.h	/^typedef struct tx_pending_t{$/;"	s
tx_pending_t	ieee80211.h	/^}tx_pending_t;$/;"	t	typeref:struct:tx_pending_t
tx_probe_rq	ieee80211.h	/^	unsigned int tx_probe_rq;$/;"	m	struct:ieee80211_softmac_stats
tx_probe_rs	ieee80211.h	/^	unsigned int tx_probe_rs;$/;"	m	struct:ieee80211_softmac_stats
tx_pw_wq	ieee80211.h	/^	struct delayed_work tx_pw_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::delayed_work
tx_pw_wq	ieee80211.h	/^	struct work_struct tx_pw_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::work_struct
tx_retry_limit_exceeded	ieee80211.h	/^	unsigned int tx_retry_limit_exceeded;$/;"	m	struct:ieee80211_stats
tx_single_retry_frames	ieee80211.h	/^	unsigned int tx_single_retry_frames;$/;"	m	struct:ieee80211_stats
tx_timeout	r8187_core.c	/^void tx_timeout(struct net_device *dev)$/;"	f
tx_unicast_frames	ieee80211.h	/^	unsigned int tx_unicast_frames;$/;"	m	struct:ieee80211_stats
tx_unicast_octets	ieee80211.h	/^	unsigned int tx_unicast_octets;$/;"	m	struct:ieee80211_stats
tx_urb_index	r8187.h	/^	short  tx_urb_index;$/;"	m	struct:r8180_priv
txb	ieee80211.h	/^	struct ieee80211_txb *txb;$/;"	m	struct:tx_pending_t	typeref:struct:tx_pending_t::ieee80211_txb
txbeacondrop	r8187.h	/^	unsigned long txbeacondrop;$/;"	m	struct:Stats
txbeaconerr	r8187.h	/^	unsigned long txbeaconerr;$/;"	m	struct:Stats
txbeaconokint	r8187.h	/^	unsigned long txbeaconokint;$/;"	m	struct:Stats
txbedrop	r8187.h	/^	unsigned long txbedrop;$/;"	m	struct:Stats
txbeerr	r8187.h	/^	unsigned long txbeerr;$/;"	m	struct:Stats
txbeokint	r8187.h	/^	unsigned long txbeokint;$/;"	m	struct:Stats
txbkdrop	r8187.h	/^	unsigned long txbkdrop;$/;"	m	struct:Stats
txbkerr	r8187.h	/^	unsigned long txbkerr;$/;"	m	struct:Stats
txbkokint	r8187.h	/^	unsigned long txbkokint;$/;"	m	struct:Stats
txdatapkt	r8187.h	/^	unsigned long txdatapkt;$/;"	m	struct:Stats
txlpdrop	r8187.h	/^	unsigned long txlpdrop;$/;"	m	struct:Stats
txlperr	r8187.h	/^	unsigned long txlperr;$/;"	m	struct:Stats
txlpokint	r8187.h	/^	unsigned long txlpokint;$/;"	m	struct:Stats
txmanagedrop	r8187.h	/^	unsigned long txmanagedrop;$/;"	m	struct:Stats
txmanageerr	r8187.h	/^	unsigned long txmanageerr;$/;"	m	struct:Stats
txmanageokint	r8187.h	/^	unsigned long txmanageokint;$/;"	m	struct:Stats
txnpdrop	r8187.h	/^	unsigned long txnpdrop;$/;"	m	struct:Stats
txnperr	r8187.h	/^	unsigned long txnperr;$/;"	m	struct:Stats
txnpokint	r8187.h	/^	unsigned long txnpokint;$/;"	m	struct:Stats
txokbytestotal	r8187.h	/^        unsigned long txokbytestotal;$/;"	m	struct:r8180_priv
txoverflow	r8187.h	/^	unsigned long txoverflow;$/;"	m	struct:Stats
txrate	r8187_core.c	/^unsigned int    txrate:4;$/;"	m	struct:tx_desc	file:
txrdu	r8187.h	/^	unsigned long txrdu;$/;"	m	struct:Stats
txresumed	r8187.h	/^	unsigned long txresumed;$/;"	m	struct:Stats
txvidrop	r8187.h	/^	unsigned long txvidrop;$/;"	m	struct:Stats
txvierr	r8187.h	/^	unsigned long txvierr;$/;"	m	struct:Stats
txviokint	r8187.h	/^	unsigned long txviokint;$/;"	m	struct:Stats
txvodrop	r8187.h	/^	unsigned long txvodrop;$/;"	m	struct:Stats
txvoerr	r8187.h	/^	unsigned long txvoerr;$/;"	m	struct:Stats
txvookint	r8187.h	/^	unsigned long txvookint;$/;"	m	struct:Stats
type	ieee80211.h	/^	u8 type;$/;"	m	struct:eapol
type	r8187.h	/^                unsigned char type;$/;"	m	struct:rtl_reg_debug::__anon13
u	ieee80211.h	/^	} u;$/;"	m	struct:ieee_param	typeref:union:ieee_param::__anon2
u	r8187_core.c	/^        } u;$/;"	m	struct:ipw_param	typeref:union:ipw_param::__anon8	file:
udev	r8187.h	/^	struct usb_device *udev;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::usb_device
unicast_uses_group	ieee80211.h	/^            unicast_uses_group:1;$/;"	m	struct:ieee80211_security
up	r8187.h	/^	short up;$/;"	m	struct:r8180_priv
usb_kill_urb	r8187_core.c	73;"	d	file:
used	ieee80211.h	/^	u8 used;$/;"	m	struct:ieee80211_crypt_data_list
value	ieee80211.h	/^			u32 value;$/;"	m	struct:ieee_param::__anon2::__anon3
value	r8187_core.c	/^                        u32 value;$/;"	m	struct:ipw_param::__anon8::__anon9	file:
version	ieee80211.h	/^	u8 version;$/;"	m	struct:eapol
wMacRegRfPinsOutput	r8187.h	/^	u32  wMacRegRfPinsOutput;$/;"	m	struct:r8180_priv
wMacRegRfPinsSelect	r8187.h	/^	u32  wMacRegRfPinsSelect;$/;"	m	struct:r8180_priv
wakeup	r8187_core.c	/^unsigned char	wakeup:1;$/;"	m	struct:rx_desc_rtl8187b	file:
wakeup	r8187_core.c	/^unsigned char   wakeup:1;$/;"	m	struct:rx_desc_rtl8187	file:
wap_set	ieee80211.h	/^	short wap_set;$/;"	m	struct:ieee80211_device
watch_dog_adaptive	r8187_core.c	/^void watch_dog_adaptive(unsigned long data)$/;"	f
watch_dog_timer	r8187.h	/^	struct timer_list watch_dog_timer;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::timer_list
watch_dog_wq	ieee80211.h	/^	struct delayed_work watch_dog_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::delayed_work
watch_dog_wq	ieee80211.h	/^	struct work_struct watch_dog_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::work_struct
wlan_first_up_flag1	r8187.h	/^	u8 wlan_first_up_flag1;$/;"	m	struct:r8180_priv
wmm_info	ieee80211.h	/^	u8 wmm_info;$/;"	m	struct:ieee80211_network
wmm_param	ieee80211.h	/^	struct ieee80211_wmm_ac_param wmm_param[4];$/;"	m	struct:ieee80211_network	typeref:struct:ieee80211_network::ieee80211_wmm_ac_param
wmm_param_update_wq	ieee80211.h	/^	struct tq_struct wmm_param_update_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::tq_struct
wmm_param_update_wq	ieee80211.h	/^	struct work_struct wmm_param_update_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::work_struct
wpa_enabled	ieee80211.h	/^	int wpa_enabled;$/;"	m	struct:ieee80211_device
wpa_ie	ieee80211.h	/^		} wpa_ie;$/;"	m	union:ieee_param::__anon2	typeref:struct:ieee_param::__anon2::__anon4
wpa_ie	ieee80211.h	/^	u8 *wpa_ie;$/;"	m	struct:ieee80211_device
wpa_ie	ieee80211.h	/^	u8 wpa_ie[MAX_WPA_IE_LEN];$/;"	m	struct:ieee80211_network
wpa_ie	r8187_core.c	/^                } wpa_ie;$/;"	m	union:ipw_param::__anon8	typeref:struct:ipw_param::__anon8::__anon10	file:
wpa_ie_len	ieee80211.h	/^	size_t wpa_ie_len;$/;"	m	struct:ieee80211_device
wpa_ie_len	ieee80211.h	/^	size_t wpa_ie_len;$/;"	m	struct:ieee80211_network
wpa_param	ieee80211.h	/^		} wpa_param;$/;"	m	union:ieee_param::__anon2	typeref:struct:ieee_param::__anon2::__anon3
wpa_param	r8187_core.c	/^                } wpa_param;$/;"	m	union:ipw_param::__anon8	typeref:struct:ipw_param::__anon8::__anon9	file:
wpax_suitlist_lock	ieee80211.h	/^	spinlock_t wpax_suitlist_lock;$/;"	m	struct:ieee80211_device
wpax_type_notify	ieee80211.h	/^	u32 wpax_type_notify; \/\/{added by David, 2006.9.26}$/;"	m	struct:ieee80211_device
wpax_type_set	ieee80211.h	/^	u8  wpax_type_set;    \/\/{added by David, 2006.9.28}$/;"	m	struct:ieee80211_device
wq	ieee80211.h	/^	struct workqueue_struct *wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::workqueue_struct
write_cam	r8187_core.c	/^void write_cam(struct net_device *dev, u8 addr, u32 data)$/;"	f
write_nic_byte	r8187_core.c	/^void write_nic_byte(struct net_device *dev, int indx, u8 data)$/;"	f
write_nic_byte_E	r8187_core.c	/^void write_nic_byte_E(struct net_device *dev, int indx, u8 data)$/;"	f
write_nic_dword	r8187_core.c	/^void write_nic_dword(struct net_device *dev, int indx, u32 data)$/;"	f
write_nic_word	r8187_core.c	/^void write_nic_word(struct net_device *dev, int indx, u16 data)$/;"	f
write_phy_cck	r8187_core.c	/^void write_phy_cck (struct net_device *dev, u8 adr, u32 data)$/;"	f
write_phy_ofdm	r8187_core.c	/^inline void write_phy_ofdm (struct net_device *dev, u8 adr, u32 data)$/;"	f
write_rtl8225	r8180_rtl8225.c	/^void write_rtl8225(struct net_device *dev, u8 adr, u16 data)$/;"	f
write_rtl8225_patch	r8180_rtl8225.c	/^void write_rtl8225_patch(struct net_device *dev, u8 adr, u16 data)$/;"	f
wstats	r8187.h	/^	struct iw_statistics wstats;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::iw_statistics
wx_sem	ieee80211.h	/^	struct semaphore wx_sem;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::semaphore
wx_sem	r8187.h	/^	struct semaphore wx_sem;$/;"	m	struct:r8180_priv	typeref:struct:r8180_priv::semaphore
wx_sync_scan_wq	ieee80211.h	/^	struct tq_struct wx_sync_scan_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::tq_struct
wx_sync_scan_wq	ieee80211.h	/^	struct work_struct wx_sync_scan_wq;$/;"	m	struct:ieee80211_device	typeref:struct:ieee80211_device::work_struct
