; "MDMCHIPV.INF"
;
; Manufacturer: Conexant Systems Inc.
; Copyright (C) 2003 Conexant Systems Inc.
;
[Version]
Signature="$CHICAGO$"
Class=Modem
ClassGUID={4D36E96D-E325-11CE-BFC1-08002BE10318}
Provider=%Mfg%
DriverVer=03/19/2004, 12.0341.0027
CatalogFile=mdmchipv.cat

[DestinationDirs]
DefaultDestDir = 12
DefaultCopy = 12	
DataCopy = 11	 

[Manufacturer]
%Mfg% = Models

[ControlFlags]
ExcludeFromSelect=PCI\VEN_134D&DEV_7890
ExcludeFromSelect=PCI\VEN_134D&DEV_7891
ExcludeFromSelect=PCI\VEN_134D&DEV_7892
ExcludeFromSelect=PCI\VEN_134D&DEV_7893
ExcludeFromSelect=PCI\VEN_134D&DEV_7894
ExcludeFromSelect=PCI\VEN_134D&DEV_7895
ExcludeFromSelect=PCI\VEN_134D&DEV_7896
ExcludeFromSelect=PCI\VEN_134D&DEV_7897
ExcludeFromSelect=PCI\VEN_1317&DEV_2850
ExcludeFromSelect=PCI\VEN_134D&DEV_2189
ExcludeFromSelect=PCI\VEN_8086&DEV_2416
ExcludeFromSelect=PCI\VEN_8086&DEV_2426
ExcludeFromSelect=PCI\VEN_8086&DEV_2446
ExcludeFromSelect=PCI\VEN_8086&DEV_2486
ExcludeFromSelect=PCI\VEN_8086&DEV_24C6
ExcludeFromSelect=PCI\VEN_8086&DEV_24D6
ExcludeFromSelect=PCI\VEN_8086&DEV_7196
ExcludeFromSelect=PCI\VEN_1106&DEV_3068
ExcludeFromSelect=PCI\VEN_1039&DEV_7013
ExcludeFromSelect=PCI\VEN_10B9&DEV_5457
ExcludeFromSelect=PCI\VEN_10B9&DEV_5450&SUBSYS_4C215349 
ExcludeFromSelect=PCI\VEN_10EC&DEV_8197&SUBSYS_69611462
ExcludeFromSelect=PCI\VEN_10EC&DEV_8197&SUBSYS_819710EC
ExcludeFromSelect=PCI\VEN_10DE&DEV_01C1
ExcludeFromSelect=PCI\VEN_10DE&DEV_0069
ExcludeFromSelect=PCI\VEN_10DE&DEV_00D9
ExcludeFromSelect=PCI\VEN_1002&DEV_434D

;
; Modem models
;
[Models]     
%Modem1% = Modem,PCI\VEN_134D&DEV_7890
%Modem1% = Modem,PCI\VEN_134D&DEV_7891
%Modem1% = Modem,PCI\VEN_134D&DEV_7892
%Modem1% = Modem,PCI\VEN_134D&DEV_7893
%Modem1% = Modem,PCI\VEN_134D&DEV_7894
%Modem1% = Modem,PCI\VEN_134D&DEV_7895
%Modem1% = Modem,PCI\VEN_134D&DEV_7896
%Modem1% = Modem,PCI\VEN_134D&DEV_7897
%Modem1% = Modem,PCI\VEN_1317&DEV_2850	;Admtek
%Modem1% = Modem,PCI\VEN_134D&DEV_2189
%Modem2% = Modem,PCI\VEN_8086&DEV_7196	;Intel
%Modem2% = Modem,PCI\VEN_8086&DEV_2416
%Modem2% = Modem,PCI\VEN_8086&DEV_2426
%Modem2% = Modem,PCI\VEN_8086&DEV_2446
%Modem2% = Modem,PCI\VEN_8086&DEV_2486
%Modem2% = Modem,PCI\VEN_8086&DEV_24C6
%Modem2% = Modem,PCI\VEN_8086&DEV_24D6
%Modem3% = Modem,PCI\VEN_1106&DEV_3068	;VIA
%Modem4% = Modem,PCI\VEN_1039&DEV_7013	;SIS
%Modem5% = Modem,PCI\VEN_10B9&DEV_5457	;ALI+
%Modem6% = Modem,PCI\VEN_10B9&DEV_5450	;ALI
%Modem6% = Modem,PCI\VEN_10B9&DEV_5450&SUBSYS_4C215349 
%Modem6% = Modem,PCI\VEN_10B9&DEV_5450&SUBSYS_545110B9
%Modem6% = Modem,PCI\VEN_10B9&DEV_5450&SUBSYS_00011179
%Modem7% = Modem,PCI\VEN_10EC&DEV_8197&SUBSYS_69611462	;Realtek
%Modem7% = Modem,PCI\VEN_10EC&DEV_8197&SUBSYS_819710EC
%Modem8% = Modem,PCI\VEN_10DE&DEV_01C1
%Modem8% = Modem,PCI\VEN_10DE&DEV_0069
%Modem8% = Modem,PCI\VEN_10DE&DEV_00D9
%Modem9% = Modem,PCI\VEN_1002&DEV_434D

[Modem.NT]
AddReg=All, MfgAddReg, Modem.AddReg, V44AddReg, PCTEL_VOICE_ALL,PCTEL_VOICE_SERWAVE,PCTEL_SPKPHONE_SERWAVE
CopyFiles = DefaultCopy, DataCopy

;
; User visible strings
;
[Strings]
Mfg = "Conexant"
; Model strings
Modem1="HSP56 MicroModem"
Modem2="HSP56 MR (Intel)"
Modem3="HSP56 MR (VIA)"
Modem4="HSP56 MR (SIS)"
Modem5="HSP56 MR (ALI+)"
Modem6="HSP56 MR (ALI)"
Modem7="HSP56 MR (Realtek)"
Modem8="HSP56 MR (NVidia)"
Modem9="HSP56 MR (ATI)"
ID1="Disk 1"
;

[DefaultCopy]
ptserial.sys,,,6
vpctcom.sys,,,6
vmodem.sys,,,6
vvoice.sys,,,6

[DataCopy]
pctspk.exe,,,6
ptuninst.exe,,,6
ptsetup.dll,,,6

[SourceDisksNames]
1=%ID1%

[SourceDisksFiles]
ptserial.sys=1
vpctcom.sys=1
vmodem.sys=1
vvoice.sys=1
pctspk.exe=1
ptuninst.exe=1
ptsetup.dll=1

[Modem.NT.Services]
AddService=Ptserial,0x00000000,Ptserial_Service_Inst
AddService=Vpctcom,0x00000000,Vpctcom_Service_Inst
AddService=Vmodem,0x00000000,Vmodem_Service_Inst
AddService=Vvoice,0x00000000,Vvoice_Service_Inst

[Modem.NT.HW]
AddReg=LowerFilterAddReg

[Modem.AddReg]
HKLM,"Software\Microsoft\Windows\CurrentVersion\Uninstall\Installing HSP56 MicroModem Drivers",UninstallString,,"ptuninst.exe"
HKLM,"Software\Microsoft\Windows\CurrentVersion\Uninstall\Installing HSP56 MicroModem Drivers",DisplayName,,"HSP56 Modem Drivers"
HKLM,SOFTWARE\MICROSOFT\WINDOWS\CURRENTVERSION\RUN,"PCTVOICE",,"pctspk.exe"
HKLM,SOFTWARE\MICROSOFT\WINDOWS\CURRENTVERSION\RUNONCE,"RUNHSP",,"RUNDLL32.EXE PTSETUP.DLL,RUNHSP"

[LowerFilterAddReg]
HKR,,"LowerFilters",0x00010000,Vvoice,Vpctcom,Vmodem,Ptserial

[Ptserial_Service_Inst]
DisplayName="W2K Conexant Serial Device Driver"
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\ptserial.sys
AddReg=PtserialAddReg

[Vpctcom_Service_Inst]
DisplayName="W2K Vpctcom"
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\vpctcom.sys

[Vmodem_Service_Inst]
DisplayName="W2K Vmodem"
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\vmodem.sys

[Vvoice_Service_Inst]
DisplayName="W2K Vvoice"
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\vvoice.sys

;
; AddReg sections
;

; --------------------------------------------------------------
; Common Registry Sections
;
; The [All] section is installed for all modems.
;
[All]
HKLM,"SOFTWARE\PCTEL\HSPModem\Settings",language,0x00010001,0
HKLM,"SOFTWARE\PCTEL\HSPModem\Settings",DFGAIN,0x00010001,0
HKLM,"SOFTWARE\PCTEL\HSPModem\Settings",VCPMGAIN,0x00010001,0
HKLM,"SOFTWARE\PCTEL\HSPModem\Settings",DTMFGAIN,0x00010001,0
HKLM,"SOFTWARE\PCTEL\HSPModem\Settings",ATI5,,"OK"
HKLM,"SOFTWARE\PCTEL\HSPModem\Settings",ATI6,,"Build 0027"
HKLM,"SOFTWARE\PCTEL\HSPModem\Settings",ATI7,,"OK"
HKLM,"SOFTWARE\PCTEL\HSPModem\Settings",ATI8,,"OK"
HKLM,"SOFTWARE\PCTEL\HSPModem\Settings",ATI9,,"OK"
HKLM,"SOFTWARE\PCTEL\HSPModem\Settings",PCTELNAME,,"Conexant "
HKLM,"SOFTWARE\PCTEL\HSPModem\Settings",PRODUCTMODEL,,"HSP56 Modem "
HKLM,"Software\PCTEL\HSPModem\Settings",PCTELVERSION,,"12.0341"
HKR,, DeviceType, 1, 02      ; Internal
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 00,00,00,00, 0f,00,00,00, f7,03,00,00, 00,c2,01,00, C0,DA,00,00
HKR,,PortSubClass,1,02
HKR,,ConfigDialog,,modemui.dll
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"
;
;
[PtserialAddReg]
HKR,,ChipSet,0x00010001,2
HKR,,HSPDAT,0x00010001,0x14103FF

[MfgAddReg]
HKR,, InactivityScale, 1, 0a,00,00,00
HKR,, InactivityFormat,, "seconds"
HKR, Init,      1,, "AT<cr>"
HKR, Init,      2,, "AT&FE0&C1&D2&K3V1W3S0=0<cr>"
HKR, Monitor,   1,, "ATS0=0<cr>"
HKR, Monitor,   2,, "None"
HKR, Hangup,    1,, "ATH<cr>"
HKR, Answer,    1,, "ATA<cr>"
HKR,, Reset,, "AT&F<cr>"
HKR, Settings, Prefix,, "AT"
HKR, Settings, Terminator,, "<cr>"
HKR, Settings, DialPrefix,, "D"
HKR, Settings, DialSuffix,, ""
HKR, Settings, SpeakerVolume_Low,, "L1"
HKR, Settings, SpeakerVolume_Med,, "L2"
HKR, Settings, SpeakerVolume_High,, "L3"
HKR, Settings, SpeakerMode_Off,, "M0"
HKR, Settings, SpeakerMode_Dial,, "M1"
HKR, Settings, SpeakerMode_On,, "M2"
HKR, Settings, SpeakerMode_Setup,, "M3"
HKR, Settings, FlowControl_Off,, "&K0"
HKR, Settings, FlowControl_Hard,, "&K3"
HKR, Settings, FlowControl_Soft,, "&K4"
HKR, Settings, ErrorControl_Off,, "\N0"
HKR, Settings, ErrorControl_Forced,, "\N2"
HKR, Settings, ErrorControl_On,, "\N3"
HKR, Settings, Compression_Off,, "%%C0"
HKR, Settings, Compression_On,, "%%C3"
HKR, Settings, Modulation_CCITT,, "B0"
HKR, Settings, Modulation_Bell,, "B1"
HKR, Settings, Modulation_CCITT_V23,,"B2"
HKR, Settings, SpeedNegotiation_Off,, "N0S37=14"
HKR, Settings, SpeedNegotiation_On,, "N1"
HKR, Settings, Pulse,, "P"
HKR, Settings, Tone,, "T"
HKR, Settings, Blind_Off,, "X4"
HKR, Settings, Blind_On,, "X1"
HKR, Settings, CallSetupFailTimer,, "S7=<#>"
HKR, Settings, InactivityTimeout,, "S30=<#>"
HKR, Responses, "0<cr>", 1, 00, 00, 00,00,00,00, 00,00,00,00 ; OK
HKR, Responses, "1<cr>", 1, 02, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "2<cr>", 1, 08, 00, 00,00,00,00, 00,00,00,00 ; RING
HKR, Responses, "3<cr>", 1, 04, 00, 00,00,00,00, 00,00,00,00 ; NO CARRIER
HKR, Responses, "4<cr>", 1, 03, 00, 00,00,00,00, 00,00,00,00 ; ERROR
HKR, Responses, "5<cr>", 1, 02, 00, b0,04,00,00, 00,00,00,00
HKR, Responses, "6<cr>", 1, 05, 00, 00,00,00,00, 00,00,00,00 ; NO DIALTONE
HKR, Responses, "7<cr>", 1, 06, 00, 00,00,00,00, 00,00,00,00 ; BUSY
HKR, Responses, "8<cr>", 1, 07, 00, 00,00,00,00, 00,00,00,00 ; NO ANSWER
; The Verbose form for response
;
HKR, Responses, "<cr>", 1, 01, 00, 00,00,00,00, 00,00,00,00               ;00
HKR, Responses, "<lf>", 1, 01, 00, 00,00,00,00, 00,00,00,00               ;00

HKR, Responses, "<cr><lf>OK<cr><lf>", 1, 00, 00, 00,00,00,00, 00,00,00,00		;00
HKR, Responses, "<cr><lf>RING<cr><lf>", 1, 08, 00, 00,00,00,00, 00,00,00,00		;02
HKR, Responses, "<cr><lf>NO CARRIER<cr><lf>", 1, 04, 00, 00,00,00,00, 00,00,00,00	;03
HKR, Responses, "<cr><lf>ERROR<cr><lf>", 1, 03, 00, 00,00,00,00, 00,00,00,00		;04
HKR, Responses, "<cr><lf>NO DIALTONE<cr><lf>", 1, 05, 00, 00,00,00,00, 00,00,00,00	;06
HKR, Responses, "<cr><lf>BUSY<cr><lf>", 1, 06, 00, 00,00,00,00, 00,00,00,00		;07
HKR, Responses, "<cr><lf>NO ANSWER<cr><lf>", 1, 07, 00, 00,00,00,00, 00,00,00,00	;08
HKR, Responses, "<cr><lf>RING BACK<cr><lf>", 1, 01, 00, 00,00,00,00, 00,00,00,00	;25
HKR, Responses, "<cr><lf>+FCERROR<cr><lf>", 1, 03, 00, 00,00,00,00, 00,00,00,00		;+F4
HKR, Responses, "<cr><lf>FAX<cr><lf>", 1, 03, 00, 00,00,00,00, 00,00,00,00		;33
HKR, Responses, "<cr><lf>DATA<cr><lf>", 1, 03, 00, 00,00,00,00, 00,00,00,00		;35

HKR,Responses,"<cr><lf>CONNECT<cr><lf>", 1, 02, 00, 00,00,00,00, 00,00,00,00		;01
HKR,Responses,"<cr><lf>CONNECT 300/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,2C,01,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 300/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,2C,01,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 300/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,2C,01,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 300/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,2C,01,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 300/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,2C,01,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/75/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/75/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/75/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/75/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/75/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 75/1200/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 75/1200/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 75/1200/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 75/1200/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 75/1200/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 2400/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,60,09,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 2400/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,60,09,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 2400/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,60,09,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 2400/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,60,09,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 2400/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,60,09,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 4800/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,C0,12,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 4800/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,C0,12,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 4800/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,C0,12,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 4800/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,C0,12,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 4800/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,C0,12,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 7200/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,20,1C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 7200/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,20,1C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 7200/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,20,1C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 7200/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,20,1C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 7200/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,20,1C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 9600/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,80,25,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 9600/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,80,25,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 9600/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,80,25,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 9600/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,80,25,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 9600/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,80,25,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 12000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,E0,2E,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 12000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,E0,2E,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 12000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,E0,2E,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 12000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,E0,2E,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 12000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,E0,2E,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 14400/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,40,38,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 14400/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,40,38,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 14400/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,40,38,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 14400/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,40,38,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 14400/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,40,38,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 16800/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,A0,41,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 16800/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,A0,41,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 16800/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,A0,41,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 16800/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,A0,41,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 16800/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,A0,41,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 19200/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,00,4B,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 19200/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,00,4B,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 19200/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,00,4B,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 19200/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,00,4B,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 19200/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,00,4B,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 21600/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,60,54,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 21600/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,60,54,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 21600/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,60,54,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 21600/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,60,54,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 21600/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,60,54,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 24000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,C0,5D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 24000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,C0,5D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 24000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,C0,5D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 24000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,C0,5D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 24000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,C0,5D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 26400/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,20,67,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 26400/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,20,67,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 26400/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,20,67,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 26400/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,20,67,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 26400/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,20,67,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,60,6D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,60,6D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,60,6D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,60,6D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,60,6D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28800/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,80,70,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28800/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,80,70,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28800/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,80,70,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28800/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,80,70,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28800/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,80,70,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 29333/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,95,72,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 29333/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,95,72,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 29333/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,95,72,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 29333/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,95,72,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 29333/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,95,72,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 30666/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,CA,77,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 30666/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,CA,77,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 30666/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,CA,77,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 30666/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,CA,77,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 30666/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,CA,77,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 31200/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,E0,79,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 31200/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,E0,79,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 31200/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,E0,79,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 31200/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,E0,79,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 31200/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,E0,79,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33600/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,40,83,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33600/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,40,83,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33600/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,40,83,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33600/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,40,83,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33600/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,40,83,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 32000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,00,7D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 32000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,00,7D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 32000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,00,7D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 32000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,00,7D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 32000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,00,7D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33333/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,35,82,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33333/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,35,82,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33333/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,35,82,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33333/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,35,82,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33333/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,35,82,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,D0,84,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,D0,84,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,D0,84,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,D0,84,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,D0,84,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34666/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,6A,87,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34666/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,6A,87,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34666/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,6A,87,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34666/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,6A,87,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34666/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,6A,87,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 36000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,A0,8C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 36000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,A0,8C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 36000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,A0,8C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 36000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,A0,8C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 36000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,A0,8C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 37333/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,D5,91,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 37333/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,D5,91,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 37333/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,D5,91,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 37333/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,D5,91,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 37333/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,D5,91,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,70,94,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,70,94,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,70,94,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,70,94,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,70,94,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38666/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,0A,97,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38666/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,0A,97,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38666/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,0A,97,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38666/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,0A,97,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38666/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,0A,97,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 40000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,40,9C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 40000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,40,9C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 40000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,40,9C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 40000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,40,9C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 40000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,40,9C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 41333/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,75,A1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 41333/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,75,A1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 41333/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,75,A1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 41333/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,75,A1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 41333/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,75,A1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,10,A4,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,10,A4,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,10,A4,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,10,A4,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,10,A4,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42666/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,AA,A6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42666/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,AA,A6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42666/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,AA,A6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42666/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,AA,A6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42666/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,AA,A6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 44000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,E0,AB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 44000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,E0,AB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 44000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,E0,AB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 44000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,E0,AB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 44000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,E0,AB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 45333/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,15,B1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 45333/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,15,B1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 45333/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,15,B1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 45333/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,15,B1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 45333/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,15,B1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,B0,B3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,B0,B3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,B0,B3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,B0,B3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,B0,B3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46666/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,4A,B6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46666/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,4A,B6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46666/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,4A,B6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46666/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,4A,B6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46666/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,4A,B6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 48000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,80,BB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 48000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,80,BB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 48000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,80,BB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 48000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,80,BB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 48000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,80,BB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 49333/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,B5,C0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 49333/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,B5,C0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 49333/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,B5,C0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 49333/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,B5,C0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 49333/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,B5,C0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,50,C3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,50,C3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,50,C3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,50,C3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,50,C3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50666/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,EA,C5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50666/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,EA,C5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50666/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,EA,C5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50666/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,EA,C5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50666/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,EA,C5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 52000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,20,CB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 52000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,20,CB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 52000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,20,CB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 52000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,20,CB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 52000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,20,CB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 53333/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,55,D0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 53333/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,55,D0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 53333/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,55,D0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 53333/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,55,D0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 53333/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,55,D0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,F0,D2,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,F0,D2,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,F0,D2,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,F0,D2,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,F0,D2,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54666/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,8A,D5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54666/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,8A,D5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54666/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,8A,D5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54666/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,8A,D5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54666/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,8A,D5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 56000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,C0,DA,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 56000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,C0,DA,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 56000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,C0,DA,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 56000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,C0,DA,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 56000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,C0,DA,00,00,00,00,00,00

[V44AddReg]
HKR,Responses,"<cr><lf>CONNECT 300/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,2C,01,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/75/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 75/1200/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 2400/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,60,09,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 4800/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,C0,12,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 7200/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,20,1C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 9600/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,80,25,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 12000/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,E0,2E,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 14400/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,40,38,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 16800/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,A0,41,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 19200/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,00,4B,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 21600/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,60,54,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 24000/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,C0,5D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 26400/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,20,67,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28000/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,60,6D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28800/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,80,70,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 29333/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,95,72,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 30666/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,CA,77,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 31200/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,E0,79,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33600/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,40,83,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 32000/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,00,7D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33333/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,35,82,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34000/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,D0,84,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34666/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,6A,87,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 36000/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,A0,8C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 37333/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,D5,91,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38000/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,70,94,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38666/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,0A,97,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 40000/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,40,9C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 41333/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,75,A1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42000/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,10,A4,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42666/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,AA,A6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 44000/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,E0,AB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 45333/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,15,B1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46000/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,B0,B3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46666/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,4A,B6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 48000/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,80,BB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 49333/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,B5,C0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50000/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,50,C3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50666/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,EA,C5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 52000/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,20,CB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 53333/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,55,D0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54000/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,F0,D2,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54666/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,8A,D5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 56000/PROTOCOL: LAPM/COMPRESSION: V.44<cr><lf>",1,02,03,C0,DA,00,00,00,00,00,00


[PCTEL_VOICE_ALL]   ; PCtel baseline voice settings
HKR,,Enumerator,,serwave.vxd
HKR,, VoiceManufacturerID,  1, 01,00
HKR,, VoiceProductIDWaveIn, 1, 80,00
HKR,, VoiceProductIDWaveOut,1, 81,00
HKR,, VoiceProductIDHandsetWaveIn,1, 82,00
HKR,, VoiceProductIDHandsetWaveOut,1, 83,00
HKR,, VoiceMixerMid,          1,02,00
HKR,, VoiceMixerPid,          1,99,01
HKR,, VoiceMixerLineID,       1,00,00,05,00

HKR, EnableCallerID, 1,, "at#cid=1<cr>"
HKR, DisableCallerID, 1,, "at#cid=0<cr>"
HKR,, CallerIDPrivate,, "P"
HKR,, CallerIDOutSide,, "O"
HKR,, VariableTerminator,,<cr><lf>
HKR, GenerateDigit,           1,, "at#vts=<Digit><cr>"

HKR, Responses, "VCON", 1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "DATE = ", 1, 93, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "TIME = ", 1, 94, 00, 00,00,00,00, 00,00,00,00            
HKR, Responses, "NMBR = ", 1, 95, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "NAME = ", 1, 96, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "MESG = ", 1, 97, 00, 00,00,00,00, 00,00,00,00

[PCTEL_VOICE_SERWAVE]   ; PCtel serial wave settings
HKR,, VoiceProfile,                     1, 21,10,00,02
HKR,, HandsetCloseDelay,                1, 8,00,00,00
HKR, StartPlay,                         1,, "at#vtx<cr>"
HKR, StopPlay,                          1,, "None"
HKR, StopPlay,                          2,, "NoResponse"
HKR, StartRecord,                       1,, "at#vrx<cr>"
HKR, StopRecord,                        1,, "None"
HKR, StopRecord,                        2,, "NoResponse"
HKR,, TerminateRecord,,                 "<h10>E"
HKR,, TerminatePlay,,                   "<h10><h03>"
HKR,, AbortPlay,,                       "<h10><h18>"
HKR, LineSetPlayFormat,                 1,, "at#vls=0<cr>"
HKR, LineSetPlayFormat,                 2,, "at#tl=7fff<cr>"
HKR, LineSetRecordFormat,               1,, "None"
HKR, LineSetRecordFormat,               2,, "NoResponse"
HKR, VoiceToDataAnswer,                 1,, "at#ima=0#cls=0<cr>"
HKR, VoiceToDataAnswer,                 2,, "ata<cr>"
HKR, VoiceAnswer,                       1,, "at#cls=8#ima=1<cr>"
HKR, VoiceAnswer,                       2,, "at#vls=0<cr>"
HKR, VoiceAnswer,                       3,, "at#vbt=1<cr>"
HKR, VoiceAnswer,                       4,, "ats30=60<cr>"
HKR, VoiceAnswer,                       5,, "ata<cr>"
HKR, VoiceDialNumberSetup,              1,, "at#cls=8#ima=1<cr>"
HKR, VoiceDialNumberSetup,              2,, "at#vls=0<cr>"
HKR, VoiceDialNumberSetup,              3,, "at#vrn=0<cr>"
HKR, VoiceDialNumberSetup,              4,, "at#vbt=1<cr>"
HKR, VoiceDialNumberSetup,              5,, "ats30=60<cr>"

HKR, WaveDriver, XformModule,  , "umdmxfrm.dll"
HKR, WaveDriver, XformID,     1, 04, 00
HKR, WaveDriver, BaudRate,    1, 00, c2, 01, 00
HKR, WaveDriver, WaveDevices, 1, 01, 00
HKR, WaveDriver, WaveHardwareID, , "FullDuplex"

[PCTEL_SPKPHONE_SERWAVE]
HKR,, VoiceProfile,           1, 25,10,00,02
HKR,, SpeakerPhoneSpecs,      1, 00,00,00,00,  0f,00,00,00,  03,00,00,00,  00,00,00,00
HKR, SpeakerPhoneEnable,      1,, "at#vls=6<cr>"
HKR, SpeakerPhoneDisable,     1,, "at#spk=0,16,,<cr>"
HKR, SpeakerPhoneDisable,     2,, "at#vls=0<cr>"
HKR, SpeakerPhoneMute,        1,, "at#spk=0,,,<cr>"
HKR, SpeakerPhoneUnMute,      1,, "at#spk=1,,,<cr>"
HKR, SpeakerPhoneSetVolumeGain,  1,, "at#vls=6<cr>"
HKR, SpeakerPhoneSetVolumeGain,  2,, "at#spk=,<Vol>,<Gain><cr>"
