[Version]
signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider="Prolink"
DriverVer=06/01/2006,4.4.601
CatalogFile.ntx86=pvavsts.cat

[Manufacturer]
"Prolink"=Prolink

[SourceDisksNames]
1="Prolink Cx23880 Drivers",,,""

[SourceDisksFiles]
pvavsts.sys=1

[Prolink]
; Include swapped SSVID
%PhilipsPALDVBT.DeviceDesc%=PhilipsPALDVBT,PCI\VEN_14F1&DEV_8802&SUBSYS_49131554
%PhilipsPALDVBT.DeviceDesc%=PhilipsPALDVBT,PCI\VEN_14F1&DEV_8802&SUBSYS_88881554
%PhilipsPALDVBT.DeviceDesc%=PhilipsPALDVBT,PCI\VEN_14F1&DEV_8802&SUBSYS_49501554
%PhilipsPALDVBT.DeviceDesc%=PhilipsPALDVBT,PCI\VEN_14F1&DEV_8802&SUBSYS_49521554
%Kittyhawk2.DeviceDesc%=Kittyhawk2,PCI\VEN_14F1&DEV_8802&SUBSYS_000614F1

[PhilipsPALDVBT]
Include=    ks.inf, kscaptur.inf, bda.inf
Needs=      KS.Registration
AddReg=     pv880.AddReg,PhilipsPALDVBT.AddReg
CopyFiles=  pv880.CopyDrivers

[Kittyhawk2]
Include=    ks.inf, kscaptur.inf, bda.inf
Needs=      KS.Registration
AddReg=     pv880.AddReg,Kittyhawk2.AddReg
CopyFiles=  pv880.CopyDrivers

[DestinationDirs]
pv880.CopyDrivers=10,system32\drivers

[pv880.CopyDrivers]
pvavsts.sys

[pv880.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,pvavsts.sys
HKR,,OkToHibernate,3,01
; Disable driver page out
HKR,,PageOutWhenUnopened,3,0
;HKR,,PageOutWhenUnopened,3,01
HKR,,DontSuspendIfStreamsAreRunning,3,01
HKLM,System\CurrentControlSet\Control\MediaCategories\%TSPinID%,Display,1, 00,00,00,00
HKLM,System\CurrentControlSet\Control\MediaCategories\%TSPinID%,Name,,%TSPinName%

;
; Driver Configuration Registry Entries
;

[TS.AddReg]

[PhilipsPALDVBT.AddReg]
HKR,"DriverData","dwTS_GEN_CNTRL",0x00010001,     0x04,0x00,0x00,0x00
HKR,"DriverData","dwIsTSStream",0x00010001,       0x00,0x00,0x00,0x00
HKR,"DriverData","dwTP_PACKET_SIZE",0x00010001,   0xBC,0x00,0x00,0x00

[Kittyhawk2.AddReg]
HKR,"DriverData","dwTS_GEN_CNTRL",0x00010001,     0x00,0x00,0x00,0x00
HKR,"DriverData","dwIsTSStream",0x00010001,       0x00,0x00,0x00,0x00
HKR,"DriverData","dwTP_PACKET_SIZE",0x00010001,   0xBC,0x00,0x00,0x00

;
; Interfaces installation
;

[PhilipsPALDVBT.Interfaces]
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%KsNameFilter%,TS_Interface,

[Kittyhawk2.Interfaces]
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%KsNameFilter%,TS_Interface,

[TS_Interface]
AddReg=TS_Interface.AddReg

[TS_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%TSFriendlyName%

;
; Services installation
;

[PhilipsPALDVBT.Services]
AddService = pvavSTS,2,TS.ServiceInstall

[Kittyhawk2.Services]
AddService = pvavSTS,2,TS.ServiceInstall

[TS.ServiceInstall]
DisplayName   = %CX23880.DeviceDesc%
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %10%\system32\drivers\pvavsts.sys

;---------------------------------------------------------------
;                S t r i n g s
;---------------------------------------------------------------

[Strings]
KsNameFilter        =   "{5ea9c066-1dfe-41c5-a2de-bf766e83c98e}"

Proxy.CLSID         =   "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"

CX23880.DeviceDesc  = 	"Prolink 2388x AVStream TS Capture"
PhilipsPALDVBT.DeviceDesc= "Prolink 2388x AVStream TS Capture (DVB-T)"
Kittyhawk2.DeviceDesc=  "Prolink 2388x AVStream TS Capture (ATSC)"

TSFriendlyName      = 	"Prolink 2388x AVStream TS Capture"


TSPinID             =   "{5237C937-0A21-4f7e-B338-DE0D0793D03F}"
TSPinName           =   "TS Out"
CX23880.null        = 	"Prolink 2388x (unused device function)"
CX23881.null        = 	"Prolink 2388x (unused device function)"
