[Version]
LayoutFile=LAYOUT.INF, layout1.inf, layout2.inf
signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider="Gdi"
CatalogFile=pmc7134.cat
DriverVer=10/29/2003, 2.3.1.2

[Manufacturer]
%GDI%=GDI

[DestinationDirs]
Cap7134.CopyDrivers = 10,system32\drivers
KSUpdate.Dll = 11

[SourceDisksNames]
1=%DiskName%,,

[SourceDisksFiles]
pmc7134.sys=1
34pciurd.dll=1
34i2curd.dll=1
34api.dll=1
34dd.dll=1
34ds.dll=1
34dialog.dll=1
34dlg2.dll=1
34TvCtrl.dll=1
34com.dll=1
Prop7134.dll=1
cap7134.hlp=1

[GDI]
%Cap7134.DeviceDescUnk33%=Cap7134.MT2050,PCI\VEN_1131&DEV_7133
%Cap7134.DeviceDescProteus33%=Cap7134.MT2050,PCI\VEN_1131&DEV_7133&SUBSYS_47121554
%Cap7134.DeviceDescProteus33%=Cap7134.TDA8275,PCI\VEN_1131&DEV_7133&SUBSYS_47221554
%Cap7134.DeviceDescProteus33%=Cap7134.PMk2,PCI\VEN_1131&DEV_7133&SUBSYS_47321554

[Cap7134.MT2050]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration
AddReg=       Cap713x.AddRegMT2050, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg, Prop7134.AddReg, 34COM.AddReg
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll
KnownFiles=   Cap7134.KnownFiles

[Cap7134.MT2050.NT]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration.NT
AddReg=       Cap713x.AddRegMT2050, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg
RegisterDlls= Prop7134.Register, 34COM.Register
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll

[Cap7134.TDA8275]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration
AddReg=       Cap713x.AddRegTDA8275, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg, Prop7134.AddReg, 34COM.AddReg
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll
KnownFiles=   Cap7134.KnownFiles

[Cap7134.TDA8275.NT]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration.NT
AddReg=       Cap713x.AddRegTDA8275, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg
RegisterDlls= Prop7134.Register, 34COM.Register
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll

[Cap7134.PMk2]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration
AddReg=       Cap713x.AddRegPMk2, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg, Prop7134.AddReg, 34COM.AddReg
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll
KnownFiles=   Cap7134.KnownFiles

[Cap7134.PMk2.NT]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration.NT
AddReg=       Cap713x.AddRegPMk2, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg
RegisterDlls= Prop7134.Register, 34COM.Register
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll

[Cap713x.AddRegMT2050]
HKR, "ENUM\Device1",pnpid,,"PMCMT2050"

[Cap713x.AddRegTDA8275]
HKR, "ENUM\Device1",pnpid,,"PMCTDA8275"

[Cap713x.AddRegPMk2]
HKR, "ENUM\Device1",pnpid,,"PMCPMK2N"

[Cap713x.AddRegProteus]
HKR, "Decoder", "Tuner Channel",0x00010001,1
HKR, "Decoder", "CVBS Channel",0x00010001,0
HKR, "Decoder", "CVBS Channel2",0x00010001,2
HKR, "Decoder", "SVHS Channel",0x00010001,6
HKR, "Decoder", "SVHS Channel2",0x00010001,7
HKR, "Decoder", "Preferred Video Standard",0x00010001,0x00000010    ; KS_AnalogVideo_PAL_B
HKR, "Decoder", "VBI Sampling Frequency",0x00010001,27000000
HKR, "Decoder", "VBI Pitch",0x00010001,1440

;Common registry entries for SAA7134 and SAA7130
[Cap713x.AddReg]
HKR, "BoardSetting", "Tuner",0x00010001,1
HKR, "BoardSetting", "Composite1",0x00010001,2
HKR, "BoardSetting", "SVideo1",0x00010001,2
HKR, "BoardSetting", "Composite2",0x00010001,3
HKR, "BoardSetting", "SVideo2",0x00010001,3
HKR, "BoardSetting", "FM",0x00010001,3
HKR, "BoardSetting", "FM Radio from SIF",0x00010001,0
HKR, "", "WorkaroundforStandardChange",0x00010001,0
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,pmc7134.sys
HKR,,PageOutWhenUnopened,3,0
HKR,,DontSuspendIfStreamsAreRunning,3,00
HKR, "Parameters", "VideoTunerEnabled",0x00010001,1
HKR, "Parameters", "SVideoEnabled",0x00010001,1
HKR, "Parameters", "CompositeEnabled",0x00010001,1
;>>> decoder defaults for tuner input
HKR, "Decoder\SRC0", "Brightness",0x00010001,0x80
HKR, "Decoder\SRC0", "Contrast",0x00010001,0x44
HKR, "Decoder\SRC0", "Saturation",0x00010001,0x40
HKR, "Decoder\SRC0", "HUE",0x00010001,0x00
HKR, "Decoder\SRC0", "Sharpness",0x00010001,0x00
HKR, "Decoder\SRC0", "Source Type",0x00010001,0x02
HKR, "Decoder\SRC0", "Y-Filter",0x00010001,0x01
HKR, "Decoder\SRC0", "C-Filter",0x00010001,0x01
HKR, "Decoder\SRC0", "C-Bypass",0x00010001,0x00
;>>>  decoder defaults for composite 1 source
HKR, "Decoder\SRC1", "Brightness",0x00010001,0x80
HKR, "Decoder\SRC1", "Contrast",0x00010001,0x44
HKR, "Decoder\SRC1", "Saturation",0x00010001,0x40
HKR, "Decoder\SRC1", "HUE",0x00010001,0x00
HKR, "Decoder\SRC1", "Sharpness",0x00010001,0x00
HKR, "Decoder\SRC1", "Source Type",0x00010001,0x02
HKR, "Decoder\SRC1", "Y-Filter",0x00010001,0x01
HKR, "Decoder\SRC1", "C-Filter",0x00010001,0x01
HKR, "Decoder\SRC1", "C-Bypass",0x00010001,0x00
;>>>  decoder defaults for composite 2 source
HKR, "Decoder\SRC2", "Brightness",0x00010001,0x80
HKR, "Decoder\SRC2", "Contrast",0x00010001,0x44
HKR, "Decoder\SRC2", "Saturation",0x00010001,0x40
HKR, "Decoder\SRC2", "HUE",0x00010001,0x00
HKR, "Decoder\SRC2", "Sharpness",0x00010001,0x00
HKR, "Decoder\SRC2", "Source Type",0x00010001,0x02
HKR, "Decoder\SRC2", "Y-Filter",0x00010001,0x01
HKR, "Decoder\SRC2", "C-Filter",0x00010001,0x01
HKR, "Decoder\SRC2", "C-Bypass",0x00010001,0x00
;>>>  decoder defaults for SVHS 1 source
HKR, "Decoder\SRC3", "Brightness",0x00010001,0x80
HKR, "Decoder\SRC3", "Contrast",0x00010001,0x44
HKR, "Decoder\SRC3", "Saturation",0x00010001,0x40
HKR, "Decoder\SRC3", "HUE",0x00010001,0x00
HKR, "Decoder\SRC3", "Sharpness",0x00010001,0x00
HKR, "Decoder\SRC3", "Source Type",0x00010001,0x02
HKR, "Decoder\SRC3", "Y-Filter",0x00010001,0x00
HKR, "Decoder\SRC3", "C-Filter",0x00010001,0x00
HKR, "Decoder\SRC3", "C-Bypass",0x00010001,0x01
;>>>  decoder defaults for SVHS 2 source
HKR, "Decoder\SRC4", "Brightness",0x00010001,0x80
HKR, "Decoder\SRC4", "Contrast",0x00010001,0x44
HKR, "Decoder\SRC4", "Saturation",0x00010001,0x40
HKR, "Decoder\SRC4", "HUE",0x00010001,0x00
HKR, "Decoder\SRC4", "Sharpness",0x00010001,0x00
HKR, "Decoder\SRC4", "Source Type",0x00010001,0x02
HKR, "Decoder\SRC4", "Y-Filter",0x00010001,0x00
HKR, "Decoder\SRC4", "C-Filter",0x00010001,0x00
HKR, "Decoder\SRC4", "C-Bypass",0x00010001,0x01

;Registry entries irrelevant for SAA7130
[Cap7134.AddReg]
HKR,,Driver,,pmc7134.sys
HKR, "Parameters", "AudioEnabled",0x00010001,1          ; enable audio
HKR, "Parameters", "AudioTunerEnabled",0x00010001,1     ; enable tuner audio
;>>> audio settings for tuner input
HKR, "", "CountryCode",,"49"     ; Germany
; 'XTAL' reflects the used hardware crystal (0=32.11MHz,1=24.567MHz)
HKR, "Audio", "XTAL",0x00010001,0x00
; 'DetectMode' reflects the used audio detection mode (1=automatic mode,0=manual mode)
HKR, "Audio", "DetectMode",0x00010001,0x01
; 'Voltage Input Select' defines the input voltage of the 2 external inputs (0=1.0 Vrms/1=2.0 Vrms)
HKR, "Audio", "Voltage Input Select Ext1",0x00010001,0x00
HKR, "Audio", "Voltage Input Select Ext2",0x00010001,0x00
; 'I2S Output' reflects the state of the two I2S output channels (1=enabled/0=disabled)
HKR, "Audio", "I2S Output",0x00010001,0x01
HKR, "Audio", "I2S2 Output",0x00010001,0x01
; 'Virtual Stereo Effect' is the pre-defined width of 'Philips Incredible Stereo' (0=narrow...5=wide)
HKR, "Audio", "Virtual Stereo Effect",0x00010001,0x04
; Audio master clock settings
HKR, "Audio", "MClk Output Enable",0x00010001,0x0
HKR, "Audio", "MClk Frequency",0x00010001,0x0
HKR, "Audio", "MClk Reference Switch",0x00010001,0x0
HKR, "Audio", "MClk Reference Divider",0x00010001,0x2
; 'DefaultStandard'
HKR, "Audio\DefaultStandard", "01",0x00010001,16   ; USA:           M    BTSC
HKR, "Audio\DefaultStandard", "31",0x00010001,5    ; Netherlands:   B/G  A2
HKR, "Audio\DefaultStandard", "32",0x00010001,6    ; Belgium:       B/G  Nicam
HKR, "Audio\DefaultStandard", "33",0x00010001,11   ; France:        L/L' Nicam
HKR, "Audio\DefaultStandard", "34",0x00010001,5    ; Spain:         B/G  A2
HKR, "Audio\DefaultStandard", "39",0x00010001,5    ; Italy:         B/G  A2
HKR, "Audio\DefaultStandard", "41",0x00010001,5    ; Switzerland:   B/G  A2
HKR, "Audio\DefaultStandard", "44",0x00010001,13   ; Great Britain: I    Nicam
HKR, "Audio\DefaultStandard", "45",0x00010001,6    ; Denmark        B/G  Nicam
HKR, "Audio\DefaultStandard", "46",0x00010001,6    ; Sweden:        B/G  Nicam
HKR, "Audio\DefaultStandard", "47",0x00010001,6    ; Norway:        B/G  Nicam
HKR, "Audio\DefaultStandard", "49",0x00010001,5    ; Germany:       B/G  A2
HKR, "Audio\DefaultStandard", "81",0x00010001,16   ; Japan:         M    BTSC
HKR, "Audio\DefaultStandard", "86",0x00010001,7    ; China:         D/K  A2 Type 1
HKR, "Audio\DefaultStandard","351",0x00010001,5    ; Azores:        B/G  A2
HKR, "Audio\DefaultStandard","358",0x00010001,6    ; Finland:       B/G  Nicam
HKR, "Audio\DefaultStandard","420",0x00010001,10   ; Czech Republic:D/K  Nicam
; 'StandardTable'
HKR, "Audio\StandardTable", "01",0x00010001,0x10   ; USA:           M
HKR, "Audio\StandardTable", "31",0x00010001,0x01   ; Netherlands:   B/G
HKR, "Audio\StandardTable", "32",0x00010001,0x01   ; Belgium:       B/G
HKR, "Audio\StandardTable", "33",0x00010001,0x04   ; France:        L/L'
HKR, "Audio\StandardTable", "34",0x00010001,0x01   ; Spain:         B/G
HKR, "Audio\StandardTable", "39",0x00010001,0x01   ; Italy:         B/G
HKR, "Audio\StandardTable", "41",0x00010001,0x01   ; Switzerland:   B/G
HKR, "Audio\StandardTable", "44",0x00010001,0x08   ; Great Britain: I
HKR, "Audio\StandardTable", "45",0x00010001,0x01   ; Denmark        B/G
HKR, "Audio\StandardTable", "46",0x00010001,0x01   ; Sweden:        B/G
HKR, "Audio\StandardTable", "47",0x00010001,0x01   ; Norway:        B/G
HKR, "Audio\StandardTable", "49",0x00010001,0x01   ; Germany:       B/G
HKR, "Audio\StandardTable", "81",0x00010001,0x10   ; Japan:         M
HKR, "Audio\StandardTable", "86",0x00010001,0x02   ; China:         D/K
HKR, "Audio\StandardTable","351",0x00010001,0x01   ; Azores:        B/G
HKR, "Audio\StandardTable","358",0x00010001,0x01   ; Finland:       B/G
HKR, "Audio\StandardTable","420",0x00010001,0x02   ; Czech Republic:D/K


[Cap7134.CopyDrivers]
pmc7134.sys

[Cap7134.KnownFiles]
pmc7134.sys=safe

[Cap7134.MT2050.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},"GLOBAL",VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TVAudio

[Cap7134.MT2050.NT.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%refWave%,VideoCapture
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%refGlobal%,VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},%refGlobal%,VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,TVAudio

[Cap7134.TDA8275.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},"GLOBAL",VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TVAudio

[Cap7134.TDA8275.NT.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%refWave%,VideoCapture
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%refGlobal%,VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},%refGlobal%,VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,TVAudio

[Cap7134.PMk2.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},"GLOBAL",VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TVAudio

[Cap7134.PMk2.NT.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%refWave%,VideoCapture
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%refGlobal%,VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},%refGlobal%,VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,TVAudio

[KSUpdate.Dll]
34api.dll
34pciurd.dll
34i2curd.dll
34dd.dll
34ds.dll
34dialog.dll
34dlg2.dll
34TvCtrl.dll
34com.dll
Prop7134.dll      ; audio property dialog
cap7134.hlp

[VideoCapture]
AddReg=VideoCapture.AddReg

[VideoCrossbar]
AddReg=VideoXBar.AddReg

[TVAudio]
AddReg=TVAudio.AddReg

[VideoCapture.AddReg]
HKR,,CLSID,,{17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%Cap7134.Capture%
HKLM,SOFTWARE\Intel\Intercast\TVControl,TVControlDLL,,34TVCtrl.dll
HKLM,SOFTWARE\Intel\Intercast\Drivers,biBitCount,,16
HKLM,SOFTWARE\Intel\Intercast\Drivers,biCompression,,BI_RGB
HKLM,SOFTWARE\Intel\Intercast\Drivers,Capture Description,,%Cap7134.Capture%
HKCR,Intercast.Display,DisplayBitMask,,f
; Private Pin Names:
; MEDIATYPE_Audio:
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\{73647561-0000-0010-8000-00AA00389B71},"Name",0x00000000,"Audio"
; GUID_VSB_OUT:
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\{F3954424-34F6-11D1-821D-0000F8300212},"Name",0x00000000,"Transport In"
; MEDIUM_AUDIO_PHILDEC_ANALOGAUDIOIN:
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\{0482DEE1-7817-11cf-8a03-00aa006ecb65},"Name",0x00000000,"Analog Audio In"

[Prop7134.AddReg]
HKLM,Software\Microsoft\Windows\CurrentVersion\RunOnce,"AudioProperties",,"%11%\Regsvr32 /s %11%\Prop7134.dll"

[34COM.AddReg]
HKLM,Software\Microsoft\Windows\CurrentVersion\RunOnce,"COMInterface",,"%11%\Regsvr32 /s %11%\34com.dll"

[Prop7134.Register]
11,,Prop7134.dll,1 ;FLG_REGSVR_DLLREGISTER

[34COM.Register]
11,,34COM.dll,1 ;FLG_REGSVR_DLLREGISTER
   
[VideoXBar.AddReg]
HKR,,CLSID,,{71F96460-78F3-11d0-A18C-00A0C9118956}
HKR,,FriendlyName,,%Cap7134.Crossbar%

[TVAudio.AddReg]
HKR,,CLSID,,{71F96462-78F3-11d0-A18C-00A0C9118956}
HKR,,FriendlyName,,%Cap7134.TVAudio%

[Cap7134.MT2050.NT.Services]
AddService = Pmc7134,0x00000002,Cap7134.ServiceInstall

[Cap7134.TDA8275.NT.Services]
AddService = Pmc7134,0x00000002,Cap7134.ServiceInstall

[Cap7134.PMk2.NT.Services]
AddService = PMC7134,0x00000002,Cap7134.ServiceInstall

[Cap7134.ServiceInstall]
DisplayName   = PMC7134
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %12%\pmc7134.sys

;---------------------------------------------------------------
;                S t r i n g s
;---------------------------------------------------------------

[Strings]

;----------------
; Non-Localizable
;----------------

SERVICE_KERNEL_DRIVER=1
SERVICE_ERROR_NORMAL=1
SERVICE_AUTO_START=2
SERVICE_DEMAND_START=3

refGlobal="GLOBAL"
refWave="WAVE"

;----------------
; Localizable
;----------------

GDI=                         "ProLink Microsystems Corp"
DiskName=                    "PV Center SAA713x Drivers"
Cap7134.DeviceDescUnk33= "*** Unknown (7133) WDM Video Capture ***"
Cap7134.DeviceDescProteus33= "PV Center (7133) WDM Video Capture"
Cap7134.Capture=             "Genesis Video Capture"
Cap7134.Crossbar=            "Genesis Crossbar"
Cap7134.TVAudio=             "Genesis TvAudio"


